{"text_format":"1","workbook":"xlsx","n_sheets":11,"sheets":["EAL Information","Accreditation","2024 Full price list","Waters","Acid sulfate soil","Agricultural","Compost","Contamination","Physical","Other Solids","Admin"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":9,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"EAL Information","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Accreditation","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"2024 Full price list","index":2,"n_rows":1385,"n_cols":5,"rows_kept":1385,"cut":false,"hidden":false,"merged":[[1019,1,1019,4],[1113,1,1113,4],[0,1,0,4],[224,1,224,4],[296,1,296,4],[508,1,508,4],[803,1,803,4]]}
[null,"WATERS ANALYTICAL SERVICES"]
[null,"WATER TESTING"]
[]
[null,null,null,null,"Metals as Total Available / Acid Soluble unless requested otherwise. All packs have preparation and digest/extract charge included."]
[null,"ITEM CODE","SPECIFIC WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-002","Water Quality - Basic \nFor drinking and domestic use.  Includes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms, E.Coli Bacteria.",77,84.7]
[null,"SW-PACK-003","Water Quality - Comprehensive\nFor drinking and domestic use. Includes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms and E.Coli Bacteria; Nitrate; Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Manganese, Nickel, Lead, Zinc, Mercury.",120,132]
[null,"SW-PACK-004","Irrigation Suitability - Basic\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Iron and Manganese; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride; Turbidity, Total Alkalinity, Water Hardness (calculation), Saturation Index; Sodium Absorption Ratio (SAR).",88,96.8]
[null,"SW-PACK-005","Irrigation and Livestock Suitability – Comprehensive\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms and E.Coli Bacteria; Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Manganese, Nickel, Lead, Zinc; Nitrate, Ammonium, Phosphate; Sodium, Potassium, Calcium, Magnesium, Chloride, Sulfate, Sodium Absorption Ratio (SAR).",165,181.5]
[null,"SW-PACK-015","Wastewater Monitoring\nIncludes pH, Total Suspended Solids (TSS); Biochemical Oxygen Demand (BOD); Total Oils and Grease (TOG).",104,114.4]
[null,"SW-PACK-016","Acid Sulfate Waters\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Titratable Acidity; Dissolved Iron and Aluminium; Sulfate, Chloride, Sulfate: Chloride Ratio.",77,84.7]
[null,"SW-PACK-021","Aggressivity Assessment\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Resistivity (Calculation), Soluble Chloride, Sulfate.",49,53.9]
[null,"SW-PACK-007","Agricultural Stock Use\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Water Hardness; Total Alkalinity; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury; Nitrate, Ammonium, Phosphate; Faecal Coliforms.",135,148.5]
[null,"SW-PACK-041","Aquaculture Monitoring Suite\nIncludes pH, Total Suspended Solids (TSS), Biochemical Oxygen Demand (BOD), Total Nitrogen (TN), Total Phosphorus (TP).",99,108.9]
[null,"SW-PACK-001","Bacteria\nIncludes Total Coliforms and E.Coli.",49,53.9]
[null,"SW-PACK-025","Dust Analysis\nAs per Total Suspended Solids (TSS) and Method AS 3580.10.1.8.2.2-1991.",27,29.7]
[null,"SW-PACK-022","Dust Ashing Analysis\nIncludes Volatile Suspended Solids (VSS), Total Suspended Solids (TSS), Total Dissolved Solids (TDS).",71,78.099999999999994]
[null,"SW-PACK-018","Effluent Monitoring\nIncludes pH, Total Suspended Solids (TSS); Biochemical Oxygen Demand (BOD); Total Oils and Grease (TOG); Total Nitrogen (TN), Total Phosphorus (TP); Nitrate, Nitrite, Phosphate, Ammonium; Faecal Coliforms.",210,231]
[null,"SW-PACK-012","Environmental Monitoring 1a\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Suspended Solids (TSS); Nitrate, Nitrite, Phosphate, Ammonium; Total Nitrogen (TN), Total Phosphorus (TP).",110,121]
[null,"SW-PACK-013","Environmental Monitoring 1b (EPA Suite)\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Suspended Solids (TSS); Nitrate, Nitrite, Phosphate, Ammonium; Total Nitrogen and Total Phosphorus; Biochemical Oxygen Demand (BOD).",140,154]
[null,"SW-PACK-017","Environmental Monitoring 2\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Suspended Solids (TSS); Total Nitrogen and Total Phosphorus; Nitrate, Nitrite, Phosphate, Ammonium; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride; Bicarbonate Alkalinity, Water Hardness (calculation); Sodium Absorption Ratio (SAR).",200,220]
[null,"SW-PACK-058","Gas Contamination Monitoring for Dissolved Gases\nIncludes Acetylene, Butane, Ethane, Ethene, Methane and Propane.",155,170.5]
[null,"SW-PACK-056","Gas Contamination Water Quality Monitoring\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Total Alkalinity, Total Suspended Solids (TSS); Total Petroleum Hydrocarbons (TPH C10-C40), BTEX (Equivalent TPH C6-C10); Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",180,198]
[null,"SW-PACK-080","General Plant Pathogen Scan Plus\nGeneral plant pathogen water scan including Phytophthora, Pythium, Rhizoctonia and Fusarium.\r\n\r\nNote: 1 L of sample is required to complete testing.",550,605]
[null,"SW-PACK-078","Liquid Compost Analysis\nIncludes pH, EC; TOC, TN; NO3, NH4, PO4; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Salmonella, Ecoli, Faecal Coliforms. Note: 1 L of sample required as well as 200 mL Bacto sample.",310,341]
[null,"SW-PACK-026","Liquid - Fertiliser Totals\nIncludes acid digestion then ICP analysis for Phosphorus; Sodium, Potassium, Calcium, Magnesium, Sulfur; Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron. Also includes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Nitrogen (TN).",200,220]
[null,"SW-PACK-057","Liquid - Hydroponic Availables\nIncludes 0.45 um filter then ICP analysis for Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride; Available Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron. Also includes pH, EC; Total Nitrogen (TN), Phosphorus (TP).",140,154]
[null,"SW-PACK-070","MRTS - FORM I - Non-potable Water Testing and Assessment Report\nIncludes pH, EC; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride, Sodium Absorption Ratio (SAR); Bicarbonate / Carbonate Alkalinity;  Salmonella, Ecoli, Total Coliforms.",165,181.5]
[null,"SW-PACK-020","Nutrients - Dissolved\nIncludes Nitrate, Nitrite, Phosphate, Ammonium.",49,53.9]
[null,"SW-PACK-019","Nutrients - Total \nIncludes Total Nitrogen (TN), Total Phosphorus (TP).",55,60.5]
[null,"SW-PACK-042","Petroleum Hydrocarbons\nIncludes Total Petroleum Hydrocarbons (TPH C10-C40), BTEX (Equivalent TPH C6-C10).",88,96.8]
[null,"SW-PACK-023","Renal RO Analysis\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Sodium, Potassium, Calcium, Magnesium, Chloride, Sulfate, Water Hardness (calculation), Nitrate, Nitrite, Phosphate, Ammonium; Fluoride, Barium; Available Metals (Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury).",140,154]
[null,"SW-PACK-077","Plant pathogens in water\nIncludes Phytophthora and Pythium.",165,181.5]
[null,"SW-PACK-076","Public Pools Microbiological Monitoring\nMicrobiological analysis of Total Plate Count (ie. Heterotrophic colony count), Ecoli and Pseudomonas aeruginosa\r\n(250ml bacto sample container with thiosulfate preservative- do not rinse container).",110,121]
[null,"SW-PACK-014","Salts Suite\nIncludes pH, EC, Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride; Total Alkalinity, Water Hardness (calculation); Sodium Absorption Ratio (SAR).",77,84.7]
[null,"SW-PACK-028","Volatile Fatty Acids (VFA)\nIncludes Volatile Fatty Acids (VFA), pH, Alkalinity.",66,72.599999999999994]
[null,"SW-PACK-079","Water Contamination Assessment\nIncludes Metals (Total Available Al, As, Cd, Cr, Cu, Fe Pb, Mn, Hg, Ni, Se, Ag, Zn), PAH, TPH, BTEX, and speciated Phenolics.",240,264]
[null,"SW-PACK-071","Water quality for concrete mixes under AS1379 \nIncludes pH, EC, TDS (by calc), Total Suspended Solids, Total Oils and Grease, Sugars (Biological Oxygen Demand), Chloride, Sodium and Sulfate.",155,170.5]
[null,"SW-PACK-055","Water Analysis - Basic\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Suspended Solids (TSS).",33,36.299999999999997]
[null,"SW-PACK-073","Water Source Identification\nIncludes pH, EC, TDS (Calc), turbidity, nitrate, nitrite, ammonia, phosphate, fluoride, Total and free residual chlorine and Ecoli bacteria (used to indicate if water is sourced from town reticulation, sewage, recycling, ground, surface or rain water – comments provided on email of results).",155,170.5]
[]
[]
[null,"ITEM CODE","WATERS PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PREP-005","As Supplied - Research Samples/External Preparation\n",0,0]
[null,"SW-PREP-003","Filtered/Dissolved Metals\nImmediate filtration through 0.45 µm filter followed by acidification with Nitric acid. It is particularly important where waters are high in suspended clay matter, where Iron and Aluminium may be present.",5,5.5]
[null,"SW-PREP-006","Saline Waters Instrument Setup (per batch)\n",110,121]
[null,"SW-PREP-007","Total Acid Digestible Metals\nNitric Acid digest. Used on oils, liquid fertilisers and when requested.",33,36.299999999999997]
[null,"SW-PREP-002","Total Available/Acid Soluble Metals\nAcidification with Nitric acid.  Used on nearly all environmental waters, acid sulfate waters, groundwater and surface waters (According to ANZECC guidelines).  Also used for clean waters, drinking waters, when acidified in the field and when requested.",5,5.5]
[null,"SW-PREP-001","Total Recoverable Metals\nNitric Acid digest. Used on high sludge/solid waters and when requested.",16,17.600000000000001]
[]
[null,null,null,null,"All packs have preparation and digest/extract charge included. Saline waters that request low level metals require (SW-PREP-006)."]
[null,"ITEM CODE","METAL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-031","Basic Metals Scan - As Supplied (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",60,66]
[null,"SW-PACK-040","Basic Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-029","Basic Metals Scan - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-030","Basic Metals Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",71,78.099999999999994]
[null,"SW-PACK-043","Extra Metals Scan - As Supplied (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",60,66]
[null,"SW-PACK-044","Extra Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-045","Extra Metals Scan - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-046","Extra Metals Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",71,78.099999999999994]
[null,"SW-PACK-074","Metals Screen in Oil - Total Acid Digestible (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.\r\nNote: 25 mL required to complete testing.",99,108.9]
[null,"SW-PACK-060","Saline Water Metals (Low Level) > 20 mS/cm (As Supplied) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",88,96.8]
[null,"SW-PACK-061","Saline Water Metals (Low Level) > 20 mS/cm (Dissolved) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",93,102.3]
[null,"SW-PACK-062","Saline Water Metals (Low Level) > 20 mS/cm (Total Available/Acid Soluble) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",93,102.3]
[null,"SW-PACK-063","Saline Water Metals (Low Level) > 20 mS/cm (Total Recoverable) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",99,108.9]
[null,"SW-PACK-039","Salts Scan - As Supplied (ICPMS)\nIncludes Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",33,36.299999999999997]
[null,"SW-PACK-036","Salts Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",38,41.8]
[null,"SW-PACK-037","Salts Scan - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",38,41.8]
[null,"SW-PACK-038","Salts Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",44,48.4]
[null,"SW-PACK-051","Special - Metals and Salts Combo - As Supplied (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",120,132]
[null,"SW-PACK-052","Special - Metals and Salts Combo - Dissolved (filtered then acidified) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",130,143]
[null,"SW-PACK-053","Special - Metals and Salts Combo - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",130,143]
[null,"SW-PACK-054","Special - Metals and Salts Combo - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",135,148.5]
[null,"SW-PACK-067","Speciated Arsenic\nIncludes toxic arsenic species AsV and AsIII determination using HPLC-ICPMS (Total Arsenic analysis also included) 1% of volume HCl preservation in PP.",385,423.5]
[null,"SW-PACK-068","Speciated Chromium\nIncludes toxic hexavalent chromium species CrVI and CrIII determination using HPLC-ICPMS (Total Chromium analysis also included) 1M NaOH preservation (approx.. 3 Drops/30ml to adjust pH to 8-9.5) in PP.",385,423.5]
[null,"SW-PACK-066","Speciated Mercury\nIncludes toxic mercury species Methyl Mercury and Hg2+ determination using HPLC-ICPMS. (Total Mercury analysis also included) 1% of volume HCl preservation in glass jar.",385,423.5]
[null,"SW-PACK-047","Specific - Rare Earth - As Supplied (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",82,90.2]
[null,"SW-PACK-048","Specific - Rare Earth - Dissolved (filtered then acidified) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",88,96.8]
[null,"SW-PACK-049","Specific - Rare Earth - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",88,96.8]
[null,"SW-PACK-050","Specific - Rare Earth - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",93,102.3]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL METAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-102","General Metals - As Supplied (external prep)\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-103","General Metals - Dissolved\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-104","General Metals - Total Available/Acid Soluble\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-105","General Metals - Total Recoverable\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-133","General Metals - Total Acid Digestable\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",16,17.600000000000001]
[null,"SW-SING-106","Non-Standard Metals - As Supplied\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-107","Non-Standard Metals - Dissolved\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-108","Non-Standard Metals - Total Available/Acid Soluble\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-109","Non-Standard Metals - Total Recoverable\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[]
[null,null,null,null,"All packs have preparation and digest/extract charge included."]
[null,"ITEM CODE","RESIDUE SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-072","Complete Waters Residue Screen \nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue).",240,264]
[null,"SW-PACK-009","Pesticide Screen 1a\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).",77,84.7]
[null,"SW-PACK-010","Pesticide Screen 1b\nIncludes Organo-chlorines (OC), Organo-phosphates (OP) and Polychlorinated biphenyls (PCB).",99,108.9]
[null,"SW-PACK-024","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Organo-phosphates (OP).",140,154]
[null,"SW-PACK-027","Pesticide Screen 2b - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",155,170.5]
[null,"SW-PACK-059","Pesticide Screen 3 - In Oil (Detection est. <10ppm)\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).\r\nNote: 25 mL required.",165,181.5]
[null,"SW-PACK-075","Pesticides/ Residue Screen – In Oil (Detection 0.1ppm) \nIncludes Organo-chlorines (OC), Organo-phosphates (OP) and a Multi-residue scan.\r\nNote: 25 mL required.",200,220]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL RESIDUE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-116","Glyphosate (Round Up)\n",190,209]
[null,"SW-SING-098","Herbicides Phenoxy Acid\n",190,209]
[null,"SW-SING-062","Hydrocarbons - BTEX (Equivalent to TPH C6-C10)\n",55,60.5]
[null,"SW-SING-008","Hydrocarbons - Polycyclic Aromatic Hydrocarbons (PAH)\n",71,78.099999999999994]
[null,"SW-SING-063","Hydrocarbons - Total Petroleum (TPH C10-C40)\n",55,60.5]
[null,"SW-SING-064","Organo-chlorines (OC)\n",71,78.099999999999994]
[null,"SW-SING-113","Organo-chlorines (OC) - In Oil\nNote: 25 mL required.",135,148.5]
[null,"SW-SING-096","Organo-chlorines (OC) - Low Level\n",99,108.9]
[null,"SW-SING-065","Organo-phosphates (OP)\n",71,78.099999999999994]
[null,"SW-SING-114","Organo-phosphates (OP) - In Oil\nNote: 25 mL required.",135,148.5]
[null,"SW-SING-097","Organo-phosphates (OP) - Low Level \n",99,108.9]
[null,"SW-SING-117","Organotins (MBT, TBT, DBT)\n",285,313.5]
[null,"SW-SING-121","PFAS in water – standard level 28 suite with detection 0.01 - 0.05 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in water.",165,181.5]
[null,"SW-SING-134","PFAS in water – LOW level 28 suite with detection 0.0002 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in water.",190,209]
[null,"SW-SING-038","Phenol - Total \n",66,72.599999999999994]
[null,"SW-SING-026","Phenolics - Speciated Phenols\n",99,108.9]
[null,"SW-SING-066","Polychlorinated Biphenyls (PCB)\n",71,78.099999999999994]
[null,"SW-SING-099","Polychlorinated Biphenyls (PCB) - Low Level \n",99,108.9]
[null,"SW-SING-111","Semi-Volatile Organic Compounds (SVOC)\nSVOC includes Phenols.",240,264]
[null,"SW-SING-037","Trihalomethanes (THM)\n",66,72.599999999999994]
[null,"SW-SING-095","Volatile Halogenated Compounds (VHC)\n",99,108.9]
[null,"SW-SING-094","Volatile Organic Compounds (VOC)\nVOC includes BTEX.",130,143]
[]
[]
[null,"ITEM CODE","INDIVIDUAL MICROBIAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-039","Bacteria - Faecal Coliforms\n",38,41.8]
[null,"SW-SING-040","Bacteria - Total Coliforms\n",38,41.8]
[null,"SW-SING-041","E.Coli - 24h Incubation\n",44,48.4]
[null,"SW-SING-042","Enterococci\n",49,53.9]
[null,"SW-SING-036","Legionella\n",110,121]
[null,"SW-SING-043","Listeria\n",66,72.599999999999994]
[null,"SW-SING-044","Pseudomonas\n",49,53.9]
[null,"SW-SING-045","Salmonella\n",66,72.599999999999994]
[null,"SW-SING-046","Total Plate Count\n",49,53.9]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL NITROGEN TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-047","Ammonium\n",22,24.2]
[null,"SW-SING-048","Nitrate\n",22,24.2]
[null,"SW-SING-049","Nitrite\n",22,24.2]
[null,"SW-SING-050","NOx\n",22,24.2]
[null,"SW-SING-051","Total Kjeldahl Nitrogen (TKN)\nIncludes Total Nitrogen and NOx.",44,48.4]
[null,"SW-SING-052","Total Nitrogen (TN)\n",33,36.299999999999997]
[null,"SW-SING-118","Total Nitrogen by LECO\n",33,36.299999999999997]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL GENERAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-142","Absorbance (Wavelength 440nm – Filtered 0.22 micron)\n",22,24.2]
[null,"SW-SING-031","Acidity (Titratable)\nIncludes pH.",19,20.9]
[null,"SW-SING-022","Algae - Basic ID and Count (Blue Green Algae only) by Microscopic Identification\n",120,132]
[null,"SW-SING-123","Algae - Full ID and Count by Microscopic Identification\n",180,198]
[null,"SW-SING-075","Alkalinity - Bicarbonate\n",19,20.9]
[null,"SW-SING-076","Alkalinity - Carbonate\n",19,20.9]
[null,"SW-SING-077","Alkalinity - Total\n",19,20.9]
[null,"SW-SING-110","Biochemical Oxygen Demand (BOD) - Dissolved\n",49,53.9]
[null,"SW-SING-012","Biochemical Oxygen Demand (BOD) - Total\n",49,53.9]
[null,"SW-SING-078","Carbon - Dissolved Organic (DOC)\n",55,60.5]
[null,"SW-SING-079","Carbon - Total Organic (TOC)\n",55,60.5]
[null,"SW-SING-119","Carbon - Total Organic (TOC) by LECO\n",55,60.5]
[null,"SW-SING-013","Chemical Oxygen Demand (COD)\n",49,53.9]
[null,"SW-SING-143","Chemical Oxygen Demand - Filtered (COD-F)\nFiltered GFC 1.2micron equivalent",55,60.5]
[null,"SW-SING-080","Chloride - Available\n",19,20.9]
[null,"SW-SING-081","Chlorine - Free\n",19,20.9]
[null,"SW-SING-082","Chlorine - Total Residual\nIncludes Total Residual Chlorine and Free Chlorine.",39,42.9]
[null,"SW-SING-017","Chlorophyll 'a' and Algal Biomass\n",59,64.900000000000006]
[null,"SW-SING-030","Chromium VI - Hexavalent \nSpeciation by a screening colourimetric technique which may be subject to matrix interference. Refer to separate analysis codes for speciation using HPLC-ICPMS analysis.",39,42.9]
[null,"SW-SING-073","Colour - Apparent\n",15,16.5]
[null,"SW-SING-074","Colour - True\n",15,16.5]
[null,"SW-SING-056","Conductivity - Electrical\n",11,12.1]
[null,"SW-SING-029","Cyanide - Total\n",55,60.5]
[null,"SW-SING-083","Fluoride\n",33,36.299999999999997]
[null,"SW-SING-116","Glyphosate (Round Up)\n",190,209]
[null,"SW-SING-084","Hardness\n",19,20.9]
[null,"SW-SING-124","Insoluble Matter – Liquid Fertilisers\nIncludes insoluble matter mg/L.",33,36.299999999999997]
[null,"SW-SING-027","Iodine - Total \n",66,72.599999999999994]
[null,"SW-SING-085","Moisture (105°C)\n",22,24.2]
[null,"SW-SING-058","Oxygen - Dissolved (DO)\n",11,12.1]
[null,"SW-SING-115","Particle Size Analysis - Laser Diffraction\nParticle size analysis using a Malvern Mastersizer 3000. Span 0.01 to 3000 µm. Size classes dictated by client requirements.\r\nPrice dependent upon application and sample amounts.",190,209]
[null,"SW-SING-055","pH\n",11,12.1]
[null,"SW-SING-054","Phosphorus - Available Orthophosphate\n",22,24.2]
[null,"SW-SING-053","Phosphorus - Total (TP)\nAutoclave digestion and analysis by FIA.",33,36.299999999999997]
[null,"SW-SING-059","Redox\n",11,12.1]
[null,"SW-SING-057","Salinity\n",11,12.1]
[null,"SW-SING-141","Silica Gel Clean-up TRH\nIncludes TRH C9-C40 Natural/ Petroleum differentiation – silica gel clean-up (removes all of the biogenic, more polar material leaving just the petrogenic based TRH).",120,132]
[null,"SW-SING-122","Silica - Total\nIncludes specialised NaOH high temperature fusion extraction of silicon as per dry weight. ",165,181.5]
[null,"SW-SING-120","Specific Gravity - Hydrometer method\nIncludes specific gravity and temperature on sample volumes greater than 200 mL.",22,24.2]
[null,"SW-SING-035","Specific Gravity - Volumetric method\nIncludes specific gravity and temperature on samples with small volumes.",22,24.2]
[null,"SW-SING-067","Sulfide - Dissolved\n",33,36.299999999999997]
[null,"SW-SING-068","Sulfide - Total\n",33,36.299999999999997]
[null,"SW-SING-100","Sulfite - Dissolved\n",24,26.4]
[null,"SW-SING-101","Sulfite - Total\n",24,26.4]
[null,"SW-SING-028","Surfactant - MBAS\n",55,60.5]
[null,"SW-SING-021","Tannin/Lignin\n",66,72.599999999999994]
[null,"SW-SING-060","Temperature\n",11,12.1]
[null,"SW-SING-061","Total Dissolved Salts (TDS) (calculation)\n",11,12.1]
[null,"SW-SING-034","Total Dissolved Solids (TDS)\nIncludes filtering and TDS by evaporation.",33,36.299999999999997]
[null,"SW-SING-118","Total Nitrogen by LECO\n",33,36.299999999999997]
[null,"SW-SING-011","Total Oils and Grease (TOG) - Hexane extractable\n",55,60.5]
[null,"SW-SING-033","Total Solids\n",33,36.299999999999997]
[null,"SW-SING-003","Total Suspended Solids (TSS)\n",22,24.2]
[null,"SW-SING-069","Turbidity\n",13,14.3]
[null,"SW-SING-070","UV Absorbency\n",27,29.7]
[null,"SW-SING-072","UV Transmission - Filtered\n",27,29.7]
[null,"SW-SING-071","UV Transmission - Unfiltered\n",27,29.7]
[null,"SW-SING-005","Volatile Suspended Solids (VSS)\n",38,41.8]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL STABLE ISOTOPE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-136","Total Inorganic Carbon (TIC) - 13C Isotopes\nIncludes both saline and non-saline waters. ",55,60.5]
[null,"SW-SING-137","Total Organic Carbon (TOC) - 13C Isotopes\nIncludes both saline and non-saline waters. ",88,96.8]
[null,"SW-SING-125","Total Inorganic and Organic (TIC and TOC) - 13C Isotopes\nIncludes both saline and non-saline waters. ",135,148.5]
[null,"SW-SING-128","Dissolved Nitrogen - 15N Isotopes\nIncludes Dissolved N2 isotope testing - ratio masses 29/28.",82,90.2]
[null,"SW-SING-129","Dissolved Nitrous Oxide - 15N Isotopes\n",140,154]
[null,"SW-SING-135","Nitrate Stable Isotope Analysis - 15N & 18O Isotopes\nIncludes Delta 15N and delta 18O of nitrate fresh and saline water samples (includes nitrate analysis to confirm minimum 0.14mg/L N required for isotope analysis).",165,181.5]
[null,"SW-SING-130","Dissolved Gas Analysis\nIncludes N2/Ar non-isotope ratio measurement.",55,60.5]
[null,"SW-SING-138","Hydrogen Isotopes in Water - 2H Isotopes\n",63,69.3]
[null,"SW-SING-140","Hydrogen and Oxygen Isotopes in Water - 2H and 18O Isotopes\n",110,121]
[null,"SW-SING-139","Oxygen Isotopes in Water - 18O Isotopes\n",63,69.3]
[]
[null,"ACID SULFATE ANALYTICAL TESTING"]
[null,"SOIL TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"AS-PACK-007","Acid Sulfate pH-F and pH-FOX Testing\nIncludes moisture content, drying and ring mill grinding. Field based technique modified for lab use. Results should be used in conjunction with field descriptions to indicate which samples require further laboratory testing.",22,24.2]
[null,"AS-PACK-008","Acid Sulfate Soil Net Acidity - S-CR (National Guidance 2018)\nIncludes Net Acidity and liming rate with analysis of Reduced Inorganic Sulfur (Chromium Reducible Sulfur; S-CR), KCl extractable pH (pH-KCl), Actual Acidity (Titratable Actual Acidity; TAA) where pH-KCl < 6.5, Retained Acidity (Net Acid Soluble Sulfur; S-NAS) where pH-KCl < 4.5 and Acid Neutralising Capacity (ANC-BT) where pH-KCl => 6.5.",99,108.9]
[null,"AS-PACK-013","Acid Sulfate Soil Net Acidity - S-POS (National Guidance 2018)\nIncludes Net Acidity and liming rate with analysis of Reduced Inorganic Sulfur (Peroxide Oxidisable Sulfur; S-POS), KCl extractable pH (pH-KCl), Actual Acidity (Titratable Actual Acidity; TAA) where pH-KCl < 6.5, Retained Acidity (Net Acid Soluble Sulfur; S-NAS) where pH-KCl < 4.5 and Acid Neutralising Capacity (ANC-BT) where pH-KCl => 6.5.",140,154]
[null,"AS-PACK-011","Acid Sulfate Soil Net Acidity for Treatment Verification (National Guidance 2018)\nIncludes Net Acidity and liming rate with analysis of Reduced Inorganic Sulfur (Chromium Reducible Sulfur; S-CR), KCl extractable pH (pH-KCl), Actual Acidity (Titratable Actual Acidity; TAA) where pH-KCl < 6.5 and Acid Neutralising Capacity (ANC-BT). \r\nClient must provide pre-liming ANC-BT.\r\nRoutine TAT of 3 days with a reduced surcharge of 50% for 24 h TAT (limited to 15 samples).\r\n",110,121]
[null,"AS-PACK-004","Acid Volatile Sulfide and Reduced Inorganic Sulfur\nIncludes Acid Volatile Sulfide (S-AV) and Chromium Reducible Sulfur (S-CR).",135,148.5]
[null,"AS-PACK-001","Actual and Potential Acidity\nIncludes analysis of Reduced Inorganic Sulfur (Chromium Reducible Sulfur; S-CR), KCl extractable pH (pH-KCl), Actual Acidity (Titratable Actual Acidity; TAA) where pH-KCl < 6.5. If Net Acidity and Liming Rate are required AS-PACK-008 should be used instead of AS-PACK-001.",77,84.7]
[null,"SS-PACK-054","Incubation - Chip Tray\nThis method is used to assess the effectiveness of a soil's Acid Neutralising Capacity (ANC). Includes pH-F before and pH-INC after 9 weeks incubation, with further incubation to 19 weeks where 4 <= pH-INC <= 6.5.",66,72.599999999999994]
[null,"SS-PACK-073","Incubation - Slab\nThis method is used to assess the effectiveness of a soil's Acid Neutralising Capacity (ANC). The incubation is maintained and pH-INC taken fortnightly until the soil pH changes by at least 0.5 pH unit to below 4, or for at least 8 weeks until pH-INC is stable.",200,220]
[null,"AS-PACK-012","Sulfate to Chloride Ratio\nIncludes Sulfate and Chloride (1:1 water) and Sulfate/Chloride Ratio.\r\n",55,60.5]
[]
[]
[null,"ITEM CODE","SOIL PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-010","Acid Sulfate Soil - Sample Preparation - Required for all individual testing\nIncludes 80°C moisture content, drying and ring mill grinding. Required for all samples analysed on a dry weight basis.  ",11,12.1]
[null,"SS-PREP-016","Fizz Test for Carbonates \nThis method is used to indicate the presence of carbonates.",3,3.3]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-PREP-017","Total Dry Weight - Oven dry basis\nMass of the sample dried at 105°C. Used to calculate bulk density when cores are supplied.",11,12.1]
[]
[null,null,null,null,"All samples require Sample Preparation (SS-PREP-010) unless a discounted testing suite is selected."]
[null,"ITEM CODE","INDIVIDUAL SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-090","Acid Neutralising Capacity (ANC-BT)\nThis method is used to measure Acid Neutralising Capacity (ANC-BT) where pH-KCl > 6.5.",33,36.299999999999997]
[null,"SS-SING-201","Acid Neutralising Capacity by Total Inorganic Carbon (C-IN)\nThis method is used to measure Acid Neutralising Capacity (ANC) where the pH-KCl > 6.5.\r\n\r\n",49,53.9]
[null,"SS-SING-250","Acid Sulfate Soil Field pH-W and pH-FOX\nIncludes pH-W and pH-FOX on raw sample, as supplied. Results should be used in conjunction with field descriptions to indicate which samples require further laboratory testing.",11,12.1]
[null,"SS-SING-089","Acid Volatile Sulfide (AVS)\nThis method measures Acid Volatile Sulfides (S-AV). All samples should be frozen on collection and transported in an esky with freezer bricks.",55,60.5]
[null,"SS-SING-088","Chromium Reducible Sulfur (CRS)\nThis method measures Reduced Inorganic Sulfur (S-CR) and is not subject to interferences by sulfate minerals and organic matter.",55,60.5]
[null,"SS-SING-064","Electrical Conductivity (1:5 water)\n",16,17.600000000000001]
[null,"SS-SING-246","Elemental Sulfur\nThis includes Elemental Sulfur (S-E). 100% surcharge for single samples to cover setup costs.",155,170.5]
[null,"SS-SING-093","Net Acid Soluble Sulfur (S-NAS)\nThis method estimates Retained Acidity where pH-KCl < 4.5.",33,36.299999999999997]
[null,"SS-SING-095","Titratable Actual Acidity (TAA)\nThis method measures Actual Acidity. Titratable Actual Acidity (TAA) titrated to pH 6.5.",33,36.299999999999997]
[null,"SS-SING-097","Titratable Actual Acidity (TAA) and KCl Extractable Sulfur (S-KCl)\n",38,41.8]
[null,"SS-SING-101","pH and Sulfate (1:1 water)\nThis method is used for classification of actual acid sulfate soil materials.",33,36.299999999999997]
[null,"SS-SING-202","pH - KCl extractable (pH-KCl)\nThis method is used to determine what further testing is required for Net Acidity calculations: Titratable Actual Acidity (TAA; pH-KCl < 6.5), Net Acid Soluble Sulfur (S-NAS; pH-KCl < 4.5), Acid Neutralising Capacity (ANC-BT or C-IN; pH-KCl => 6.5).\r\n",22,24.2]
[null,"SS-SING-098","Sulfur - KCl Extractable\nThis method is used to measure sulfur concentration after Titratable Actual Acidity (TAA) analysis.",11,12.1]
[null,"SS-SING-163","Peroxide Oxidisable Sulfur (S-POS)\nThis method estimates Reduced Inorganic Sulfur. It can include interferences from sulfate minerals and organic matter.",93,102.3]
[null,"SS-SING-208","Texture - Full (NCST, 2009)\nThis method is used for acid sulfate soil action criteria.",27,29.7]
[]
[null,"ROCK TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","ROCK SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"AS-PACK-010","Acid Sulfate Rock with Chromium Reducible Sulfur\nIncludes Net Acid Producing Potential (NAPP), NAG pH and Net Acid Generation (NAG) (single addition peroxide acidity), Acid Neutralising Capacity (ANC-BT) and Reduced Inorganic Sulfur (S-CR) (combined in NAPP equation).",120,132]
[null,"AS-PACK-006","Acid Sulfate Rock with Total Sulfur\nIncludes Net Acid Producing Potential (NAPP), NAG pH and Net Acid Generation (NAG) (single addition peroxide acidity), Acid Neutralising Capacity (ANC-BT) and Total Sulfur (combined in NAPP equation).",99,108.9]
[]
[]
[null,"ITEM CODE","ROCK PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-010","Acid Sulfate Soil - Sample Preparation - Required for all individual testing\nIncludes 80°C moisture content, drying and ring mill grinding. Required for all samples analysed on a dry weight basis.  ",11,12.1]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[]
[null,null,null,null,"All samples require Sample Preparation (SS-PREP-010) unless a discounted testing suite is selected."]
[null,"ITEM CODE","INDIVIDUAL ROCK TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-090","Acid Neutralising Capacity (ANC-BT)\nThis method is used to measure Acid Neutralising Capacity (ANC-BT) where pH-KCl > 6.5.",33,36.299999999999997]
[null,"SS-SING-201","Acid Neutralising Capacity by Total Inorganic Carbon (C-IN)\nThis method is used to measure Acid Neutralising Capacity (ANC) where the pH-KCl > 6.5.\r\n\r\n",49,53.9]
[null,"SS-SING-088","Chromium Reducible Sulfur (CRS)\nThis method measures Reduced Inorganic Sulfur (S-CR) and is not subject to interferences by sulfate minerals and organic matter.",55,60.5]
[null,"SS-SING-102","Net Acid Generation (NAG)\nThis method is used to determine the Net Acid Generation (NAG) of rock material. Includes NAGpH.",55,60.5]
[null,"SS-SING-144","Total Sulfur (TS) by LECO\n",22,24.2]
[]
[null,"WATER TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-016","Acid Sulfate Waters\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Titratable Acidity; Dissolved Iron and Aluminium; Sulfate, Chloride, Sulfate: Chloride Ratio.",77,84.7]
[null,"SW-PACK-029","Basic Metals Scan - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-040","Basic Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-044","Extra Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-045","Extra Metals Scan - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-048","Specific - Rare Earth - Dissolved (filtered then acidified) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",88,96.8]
[null,"SW-PACK-049","Specific - Rare Earth - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",88,96.8]
[]
[null,"AGRICULTURAL ANALYTICAL SERVICES"]
[null,"SOIL TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","ROUTINE SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"RA-PACK-001","Agricultural - Albrecht/Reams\nIncludes pH and EC (1:5 water); Available Calcium, Magnesium, Potassium, Ammonium, Nitrate, Phosphate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), Organic Matter, TC/TN Ratio; Basic Colour, Basic Texture.",120,132]
[null,"RA-PACK-002","Agricultural - Albrecht/Reams plus Totals\nIncludes pH and EC (1:5 water); Available Calcium, Magnesium, Potassium, Ammonium, Nitrate, Phosphate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Basic Colour, Basic Texture; Total Sodium, Potassium, Calcium, Magnesium, Sulfur,  Phosphorus, Silicon, Cobalt, Molybdenum, Selenium, Zinc, Manganese, Iron, Copper, Boron and Aluminium.",180,198]
[null,"RA-PACK-003","Agricultural - Albrecht/Reams plus Totals and Heavy Metals\nIncludes pH and EC (1:5 water); Available Calcium, Magnesium, Potassium, Ammonium, Nitrate, Phosphate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Basic Colour, Basic Texture; Total Sodium, Potassium, Calcium, Magnesium, Sulfur, Phosphorus, Silicon, Cobalt, Molybdenum, Selenium, Zinc, Manganese, Iron, Copper, Boron and Aluminium; Heavy Metals Silver, Arsenic, Lead, Chromium, Nickel, Cadmium, Mercury.",200,220]
[null,"RA-PACK-014","Agricultural - Standard C\nIncludes pH and EC (1:5 water); pH (1:5 CaCl); Available (Ammonium, Nitrate, Sulfur); Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Colwell Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Basic Colour, Basic Texture.",110,121]
[null,"RA-PACK-015","Agricultural - Sugarcane Reefwise\nIncludes pH and EC (1:5 water); pH (1:5 CaCl); Available Ammonium, Nitrate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Nitric Acid Extractable Potassium; Colwell Phosphorus, Phosphorous Buffer Index (PBI), BSES Phosphorus, Silicon; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; HCl Extractable Zinc; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Organic Carbon (W-B); Basic Colour, Basic Texture.",155,170.5]
[null,"RA-PACK-017","Agricultural Basic Home\nIncludes pH and EC (1:5 water); Exchangeable Sodium, Potassium, Calcium, Magnesium, Cation Exchange Capacity; Bray I Phosphorus; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter.",66,72.599999999999994]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","OTHER SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"RA-PACK-004","Agricultural - Standard A-1\nIncludes pH and EC (1:5 water); Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Bray I Phosphorus; Total Carbon (TC), Total Nitrogen (TN), Organic Matter; Basic Colour, Basic Texture.",82,90.2]
[null,"RA-PACK-018","Agricultural - Standard A-2\nIncludes pH and EC (1:5 water); Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Colwell Phosphorus; Total Carbon (TC), Total Nitrogen (TN), Organic Matter; Basic Colour, Basic Texture.",82,90.2]
[null,"RA-PACK-013","Agricultural - Standard B\nIncludes pH and EC (1:5 water); Available Ammonium, Nitrate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Hydrogen, Cation Exchange Capacity; Bray I and II Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Basic Colour, Basic Texture.",99,108.9]
[null,"RA-PACK-041","Agricultural Sugar Cane Basic  \nIncludes Basic Texture, Basic Colour, Organic Carbon (W/B), pH/EC (H2O), pH (CaCl2), EC-SE (Calculation), Phosphorus (Colwell, BSES), Phosphorus Buffer Index, Potassium (Nitric), Exchangeable Cations (Ammonium Acetate), Aluminium (KCl), Sulfur (MCP), and Silicon (BSES, CaCl2).",135,148.5]
[null,"RA-PACK-043","Agricultural Sugar Cane Full  \nIncludes Basic Texture, Basic Colour, Organic Carbon (W/B), pH/EC (H2O), pH (CaCl2), EC-SE (Calculation), Phosphorus (Colwell, BSES), Phosphorus Buffer Index, Potassium (Nitric), Exchangeable Cations (Ammonium Acetate), Aluminium (KCl), Sulfur (MCP), Silicon (BSES, CaCl2), Zinc (HCl), Iron/Copper/Zinc/Manganese (DTPA), Chloride (H2O), Ammonium/Nitrate (KCl) and Buffer pH.",180,198]
[null,"RA-PACK-042","Agricultural Sugar Cane Standard  \nIncludes Basic Texture, Basic Colour, Organic Carbon (W/B), pH/EC (H2O), pH (CaCl2), EC-SE (Calculation), Phosphorus (Colwell, BSES), Phosphorus Buffer Index, Potassium (Nitric), Exchangeable Cations (Ammonium Acetate), Aluminium (KCl), Sulfur (MCP), Silicon (BSES, CaCl2), Zinc (HCl) and Iron/Copper/Zinc/Manganese (DTPA).",155,170.5]
[null,"SS-PACK-113","Haney – Basic Carbon and Nitrogen\nIncludes Water extractable Nitrate/Ammonium, Total Water extractable Nitrogen and Organic Carbon, Inorganic Nitrogen (Calc), Organic Nitrogen (Calc), Water extractable Organic Carbon: Organic Nitrogen Ratio (Calc).",66,72.599999999999994]
[null,"SS-PACK-114","Haney – Basic Nutrients\nIncludes Haney (H3A) extractable Nitrate, Ammonium, Calcium, Magnesium, Potassium, Sodium, Phosphorus, Sulfur, Zinc, Manganese, Iron, Copper, Aluminium.",55,60.5]
[null,"SS-PACK-115","Haney – Basic Soil Health\nIncludes Solvita CO2 respiration, Water extractable Nitrate, Ammonium; Total Water extractable Nitrogen and Organic Carbon; Inorganic Nitrogen (Calc), Organic Nitrogen (Calc), Water extractable Organic Carbon: Organic Nitrogen Ratio (Calc) and Haney Soil Health Score (Calc).",110,121]
[null,"SS-PACK-116","Haney – Routine Soil Health\nIncludes Solvita CO2 respiration, Water extractable Nitrate, Ammonium; Total Water extractable Nitrogen and Organic Carbon; Inorganic Nitrogen (Calc), Organic Nitrogen (Calc), Water extractable Organic Carbon: Organic Nitrogen Ratio (Calc) and Haney Soil Health Score (Calc). Haney (H3A) extractable Nitrate, Ammonium, Calcium, Magnesium, Potassium, Sodium, Phosphorus, Sulfur, Zinc, Manganese, Iron, Copper, Aluminium.",165,181.5]
[null,"SS-PACK-117","Haney – Total Soil Health\nIncludes Solvita CO2 respiration, Water extractable Nitrate, Ammonium; Total Water extractable Nitrogen and Organic Carbon; Inorganic Nitrogen (Calc), Organic Nitrogen (Calc), Water extractable Organic Carbon: Organic Nitrogen Ratio (Calc) and Haney Soil Health Score (Calc). Haney (H3A) extractable Nitrate, Ammonium, Calcium, Magnesium, Potassium, Sodium, Phosphorus, Sulfur, Zinc, Manganese, Iron, Copper, Aluminium. Also includes pH, EC; Total Carbon, Total Nitrogen, estimated Organic Matter and Labile Carbon.",220,242]
[null,"RA-PACK-019","Macadamia Soil Testing\nIncludes pH and EC (1:5 water); Available (Sulfur); Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Colwell Phosphorus, Phosphorus Buffer Index; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Basic Colour, Basic Texture.",110,121]
[null,"NT-PACK-005","Mehlich III Basic\nIncludes pH and EC (1:5 water); Chloride Estimate, Extractable Mehlich III Phosphorus, Sodium, Potassium, Calcium, Magnesium, Cation Exchange Capacity, Exchangeable Sodium Percentage.",60,66]
[null,"SS-PACK-037","Mehlich III Exchangeable Cations and Micronutrients\nIncludes Mehlich III Extractable Sodium, Potassium, Calcium, Magnesium, Phosphorus, Sulfur, Aluminium, Iron, Copper, Zinc, Manganese, Boron.",66,72.599999999999994]
[null,"NT-PACK-001","Mehlich III Standard\nIncludes pH and EC (1:5 water); Available Calcium, Magnesium, Potassium, Ammonium, Nitrate, Phosphate, Sulfur; Mehlich III Extractable Sodium, Potassium, Calcium, Magnesium, Hydrogen/Aluminium (calculation) Cation Exchange Capacity; Mehlich III Extractable Phosphorus, Bray II Phosphorus; Total Nitrogen (TN), Total Carbon (TC), Organic Matter; Available Micronutrients Iron, Copper, Zinc, Manganese, Silicon, Boron; Paramagnetism; Basic Colour and Basic Texture.",110,121]
[null,"SS-PACK-140","Microbial Biomass Assessment - Soil\nIncludes biomasses of 12 microbial groups relevant for soil quality, health and function. ",285,313.5]
[null,"SS-PACK-167","MIC-01: Basic Analysis of Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Total fungi (moulds), Gram negative bacteria, Filamentous actinomycetes, Yeasts. ",99,108.9]
[null,"SS-PACK-168","MIC-02: Extended Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Filamentous actinomycetes, Actinobacteria, Gram negative bacteria, Filamentous fungi (Moulds), Yeasts, Lactic acid bacteria, Total Anaerobes (includes facultative anaerobes), Sulfite Reducing Anaerobes.",210,231]
[null,"SS-PACK-014","Pesticide Screen 1b\nIncludes Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",110,121]
[null,"SS-PACK-175","Phytophthora and Pythium\nNote: 500 g of sample is required to complete testing.",165,181.50000000000003]
[null,"RA-PACK-007","Reef Wise Pack - 1\nIncludes Colwell Phosphorus; Phosphorous Buffer Index (PBI); BSES Extractable Phosphorous; Organic Carbon (W-B).",66,72.599999999999994]
[null,"RA-PACK-016","Reef Wise Pack - 2\nIncludes Colwell Phosphorus; Phosphorus Buffer Index (PBI); BSES Extractable Phosphorus, Silicon; CaCl2 Extractable Silicon; HNO3 Extractable Potassium; HCl Extractable Zinc; Organic Carbon (W-B).",82,90.2]
[null,"SS-PACK-118","Residue Screen - Extended (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",310,341]
[null,"SS-PACK-119","Residue Screen - Complete + Glyphosate (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue) + Glyphosate Screens.",470,517]
[null,"SS-PACK-182","Soil/ Sediment Contamination Assessment\nIncludes Metals (Total Available Al, As, Cd, Cr, Cu, Fe Pb, Mn, Hg, Ni, Se, Ag, Zn), PAH, TPH, BTEX, and speciated Phenolics.",240,264]
[null,"SS-PACK-052","Soluble Nitrogen - Soil\nIncludes KCl extractable Nitrate and Ammonium.",44,48.4]
[null,"SS-PACK-045","Total Acid Extractable - Heavy Metals  (ICPMS)\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",55,60.5]
[null,"RA-PACK-009","Total Acid Extractable Cobalt, Molybdenum, Selenium\n",33,36.299999999999997]
[null,"RA-PACK-012","Total Acid Extractable Cobalt, Molybdenum, Selenium, Phosphorus\n",44,48.4]
[null,"RA-PACK-008","Total Acid Extractable Elements\nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Phosphorus, Silicon, Cobalt, Molybdenum, Selenium, Zinc, Manganese, Iron, Copper, Boron, Aluminium.",88,96.8]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-013","Biosecurity Handling Charge\n",110,121]
[null,"SS-SING-038","Chloride - Water Extractable",33,36.299999999999997]
[null,"SS-SING-218","Colour (Munsell Soil Colour Classification)  \n",8,8.8000000000000007]
[null,"SS-SING-085","Emerson Dispersion Index (Loveday and Pyle, 1973)\n",49,53.9]
[null,"SS-PREP-015","Exchangeable Cation Pre-treatment for Soluble Salts\nIncludes pre-treatment with aqueous ethanol and aqueous glycerol to remove soluble salts. Recommended on soils with EC > 0.3 dS/m.",11,12.1]
[null,"SS-PREP-020","Exchangeable Cation Suppression of Carbonates \nIncludes pre-treatment with aqueous ethanol and aqueous glycerol to remove soluble salts then extraction with 1M Alcoholic NH4Cl to suppress solid phase carbonates. Testing according to Method 15C1 with other agricultural tests.",44,48.4]
[null,"SS-SING-204","Fertility Report - Ferti-Tech Soil /Leaf Report Preparation\n",52,57.2]
[null,"SS-SING-071","Fertility Report - Keycrobe Soil /Leaf Report Preparation\n",52,57.2]
[null,"SS-SING-234","Fertility Report - Vital Soils Report Preparation\n",52,57.2]
[null,"SS-SING-262","Microbiometer – Soil biomass measurement\nIncludes estimates of Total Bacteria, Fungi and Fungi:Bacteria ratio. This test should only be done in conjunction with SS-Pack-167 or SS-Pack-168.",33,36.299999999999997]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-SING-066","pH (1:5 CaCl2)\n",16,17.600000000000001]
[null,"SS-SING-034","Phosphorus - Olsen\nIncludes Olsen Phosphorous - a measure of the intensity of Phosphorus.",22,24.2]
[null,"SS-SING-032","Phosphorus - Total Acid Extractable (includes preparation)\n",44,48.4]
[null,"SS-SING-037","Phosphorus Buffer Index (PBI)\n",22,24.2]
[null,"SS-SING-076","Potassium - Colwell \n",27,29.7]
[null,"SS-PREP-018","Saturated Paste Extract\nIncludes extraction of saturated paste (14A3). Please select required analytical parameters from the waters codes.",77,84.7]
[null,"SS-SING-027","Silica - Total\nIncludes specialised NaOH high temperature fusion extraction of silicon.",135,148.5]
[null,"SS-SING-209","SOLVITA - Soil CO2 Burst\nIncludes measurement of carbon dioxide released from soil due to biological activity.",66,72.599999999999994]
[null,"SS-SING-086","Texture – Full under AS 1547:2012",27,29.7]
[null,"SS-PREP-007","Total Dry Weight - Air dry basis\nMass of the sample dried at 40°C.\r\n",6,6.6]
[]
[null,"SOIL CARBON TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SOIL CARBON SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-179","Total Organic Carbon (TOC) on Topsoils under 2021 CFI Methodology\nIn CFI methodology topsoil refers to the 0 - 30 cm layer, however this should be selected on individual depth layers up to 30cm in total. \r\nIncludes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on the air-dry soil.",63,69.3]
[null,"SS-PACK-180","Total Organic Carbon (TOC) on Subsoils under 2021 CFI Methodology\nIn CFI methodology subsoil refers to the 30+cm layer however this should be selected on a depth layer of 30-100cm only. \r\nIncludes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on the air-dry soil.",94,103.4]
[null,"SS-PACK-181","Total Organic Carbon (TOC) on Core segments under 2021 CFI Methodology\nTo be selected on core segments or soil layers 0-5cm or 0-10cm. Includes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on air-dry soil.",47,51.7]
[null,"SS-PACK-193","Total Organic Carbon on Topsoils modified from 2021 CFI Methodology – not ERF registered projects\nIn CFI methodology topsoil refers to the 0-30 cm layer, however, this should be selected on individual depth layers up to 30cm in total.                                                                                                                                                                                                                                                                                                           \r\nModified method includes representative sub-sampling and analysis on reduced mass. Includes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on the air-dry soil.",57,62.7]
[null,"SS-PACK-194","Total Organic Carbon on Subsoils modified from 2021 CFI Methodology – not ERF registered projects\nIn CFI methodology subsoil refers to the 30+cm layer, however, this should be selected on a depth layer of 30-100cm only.                                                                                                                                                                                                                                                                                                            \r\nModified method includes representative sub-sampling and analysis on reduced mass. Includes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on the air-dry soil.",89,97.9]
[null,"SS-PACK-187","Carbon - Total Organic by LECO plus Gravimetric Moisture\nIncludes gravimetric moisture and TOC by LECO combustion.",52,57.2]
[null,"SS-PACK-174","Inorganic (Carbonate) Carbon by LECO\nIncludes Total Carbon (TC), Total Organic Carbon (TOC).",60,66]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL SOIL CARBON TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-018","Carbon - Labile - Blair 0.333M KMnO4",22,24.2]
[null,"SS-SING-062","Carbon - Organic by Walkley Black\n",44,48.4]
[null,"SS-SING-061","Carbon - Total Organic by LECO\n",33,36.299999999999997]
[null,"SS-SING-276","Carbon - Total Organic by LECO plus PREP\nIncludes sample preparation and TOC by LECO combustion.",42,46.2]
[null,"SS-PREP-023","Sample Compositing for Soil Carbon Subsoils (30-100cm)\nIncludes compositing charge for composite subsoil samples tested under 2018 CFI methodology.",38,41.8]
[null,"SS-PREP-022","Sample Compositing for Soil Carbon Topsoils (0-30cm)\nIncludes compositing charge for composite topsoil samples tested under 2018 CFI methodology.",16,17.600000000000001]
[]
[null,"FERTILISER TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","FERTILISER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"FA-PACK-003","Fertiliser - Liquid  Analysis\nIncludes pH, EC, Total Dissolved Salts (TDS) (by calc.); Total Nitrogen, Total Phosphorus; Sodium, Potassium, Calcium, Magnesium, Sulfur; Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper and Boron.",220,242]
[null,"FA-PACK-001","Fertiliser - Solid  Analysis\nIncludes Moisture, pH, EC; Total Nitrogen (TN), Total Carbon (TC); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Sulfur, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron.",220,242]
[null,"FA-PACK-009","Gypsum Assessment - Fertiliser\nIncludes Moisture Content, Calcium, Magnesium, Sodium and Sulfur.",135,148.5]
[null,"FA-PACK-015","LECO - Total Carbon and Total Nitrogen - Fertiliser\nIncludes Total Carbon (TC) and Total Nitrogen (TN), TC/TN Ratio.",66,72.599999999999994]
[null,"FA-PACK-014","Lime Assessment - Basic Fertiliser\nIncludes Moisture Content, Calcium, Magnesium, Acid Neutralising Capacity (ANC-BT) and Neutralising Value.",140,154]
[null,"FA-PACK-010","Lime Assessment - Coarse Fertiliser\nIncludes Moisture Content, Calcium, Magnesium, Acid Neutralising Capacity (ANC-BT), Neutralising Value and Dry Sieving Particle Size Analysis including > 1 mm, 0.85-1 mm, 0.3-0.85 mm, < 0.3 mm fractions.",180,198]
[null,"FA-PACK-011","Lime Assessment – Fine Fertiliser \nIncludes Moisture Content, Calcium, Magnesium, Acid Neutralising Capacity (ANC-BT), Neutralising Value and Laser Diffraction Particle Size Analysis including < 0.01 mm, 0.01-0.02 mm, 0.02-0.03 mm, 0.03-0.04 mm, 0.04-0.05 mm, 0.05-0.06 mm, 0.06-0.07 mm, 0.07-0.08 mm, 0.08-0.09 mm, 0.09-0.1 mm, 0.1-0.125 mm, 0.125-0.25 mm, 0.25-0.5 mm, 0.5-1.0 mm, > 1.0 mm fractions.",285,313.5]
[null,"FA-PACK-007","NPK Analysis - Fertiliser\nIncludes Total Nitrogen, Total Phosphorus, Total Potassium.",135,148.5]
[null,"FA-PACK-012","Particle Size Analysis – Dry Sieving – Coarse Fertiliser\nDry sieving Particle Size Analysis including  > 1 mm, 0.85-1 mm, 0.3-0.85 mm, < 0.3 mm fractions.",55,60.5]
[null,"FA-PACK-013","Particle Size Analysis – Laser Diffraction – Fine Fertiliser\nLaser Diffraction Particle Size Analysis including 2000 to 0.01 µm. Size fractions include < 0.01 mm, 0.01-0.02 mm, 0.02-0.03 mm, 0.03-0.04 mm, 0.04-0.05 mm, 0.05-0.06 mm, 0.06-0.07 mm, 0.07-0.08 mm, 0.08-0.09 mm, 0.09-0.1 mm, 0.1-0.125 mm, 0.125-0.25 mm, 0.25-0.5 mm, 0.5-1.0 mm, > 1.0 mm fractions.\r\nPrice dependent upon application and sample amounts.",190,209]
[null,"FA-PACK-008","Soluble Nitrogen - Fertiliser\nIncludes water extractable nitrate and ammonium on fertilisers ",88,96.8]
[null,"FA-PACK-005","Soluble Phosphorus I - Fertiliser \nIncludes Total Phosphorus, Total Soluble Phosphorus, Water Soluble Phosphorus, 2% Citrate Soluble Phosphorus.",110,121]
[null,"FA-PACK-006","Soluble Phosphorus II - Fertiliser \nIncludes Total Phosphorus, Total Soluble Phosphorus, Water Soluble Phosphorus, 2% Citrate Soluble Phosphorus and 2% Formic Acid Soluble Phosphorus.",155,170.5]
[null,"FA-PACK-002","Total Acid Extractable - Heavy Metals  (ICPMS) - Fertiliser\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",88,96.8]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL FERTILISER TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-238","Chloride – Fertiliser \nIncludes water soluble chloride on fertilisers.",66,72.599999999999994]
[null,"SS-PREP-014","Fertiliser Handling Charge\n",55,60.5]
[null,"SS-SING-067","Fluoride - Water Extractable",66,72.599999999999994]
[null,"SW-SING-124","Insoluble Matter – Liquid Fertilisers\nIncludes insoluble matter mg/L.",33,36.299999999999997]
[null,"SS-SING-240","Insoluble Matter – Solid Fertilisers\nIncludes insoluble matter mg/kg.",44,48.4]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-SING-233","Moisture Content - As Received (%) at 40°C \nMoisture content as a per cent of air-dry equivalent soil (40°C).",11,12.1]
[null,"SS-SING-193","Solubility - Fertiliser\nIncludes maximum solubility at 20°C.",44,48.4]
[null,"SW-SING-120","Specific Gravity - Hydrometer method\nIncludes specific gravity and temperature on sample volumes greater than 200 mL.",22,24.2]
[null,"SW-SING-035","Specific Gravity - Volumetric method\nIncludes specific gravity and temperature on samples with small volumes.",22,24.2]
[null,"SW-SING-149","Silicon – 2M NaOH extraction – Liquid Fertilisers\n",65,71.5]
[]
[null,"PLANT TISSUE AND GRAIN TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","PLANT TISSUE AND GRAIN SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"PA-PACK-001","Plant Testing\nIncludes Total Nitrogen (TN), Total Carbon (TC), Total Sulfur (TS); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron.",55,60.5]
[null,"PA-PACK-008","Plant Testing - Comprehensive\nIncludes Total Nitrogen (TN), Total Carbon (TC), Total Sulfur (TS); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron, Aluminium, Selenium, Chloride, Nitrate Nitrogen, Ammonium Nitrogen.",99,108.9]
[null,"PA-PACK-004","Plant Testing with Leaf Washing\nIncludes Total Nitrogen (TN), Total Carbon (TC), Total Sulfur (TS); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron, Leaf Washing.",66,72.599999999999994]
[null,"PA-PACK-002","Plant Testing with Report\nIncludes Total Nitrogen (TN), Total Carbon (TC), Total Sulfur (TS); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron; Fertility Report.",93,102.3]
[null,"SS-PACK-118","Residue Screen - Extended (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",310,341]
[null,"PA-PACK-006","Sap Analysis\nIncludes Moisture, pH, EC, Total Nitrogen; Nitrate, Ammonium; Chloride; Calcium, Magnesium, Sodium, Potassium, Phosphorus, Sulfur, Boron, Copper, Iron, Manganese, Zinc, Aluminium, Molybdenum, Cobalt and Silicon; Brix.. Data Only (no interpretation).",88,96.8]
[null,"PA-PACK-005","Soluble Nitrogen\nIncludes Nitrate and Ammonium.",44,48.4]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL PLANT TISSUE AND GRAIN TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-271","Carbohydrates - Cold Water Soluble\n(% in plant leaf or organic material)",63,69.3]
[null,"SS-SING-277","Carbohydrates - Total Non-structural\n(% in plant leaf or organic material)",66,72.599999999999994]
[null,"SS-SING-160","Brix Reading\n",11,12.1]
[null,"SS-SING-270","Chloride – Plants\nIncludes water soluble chloride on plants.",33,36.299999999999997]
[null,"SS-SING-263","Chlorophyll 'a' Concentration \nIncludes 90% acetone extraction- requires air dry and grinding into powder.",66,72.599999999999994]
[null,"SS-SING-225","Dry Matter Content (%) at 105°C\nProportion of moisture and oven-dry solid in ‘as received’ sample (105°C). ",11,12.1]
[null,"SS-SING-204","Fertility Report - Ferti-Tech Soil /Leaf Report Preparation\n",52,57.2]
[null,"SS-SING-071","Fertility Report - Keycrobe Soil /Leaf Report Preparation\n",52,57.2]
[null,"SS-SING-022","Iodine - NaOH Extraction\n",110,121]
[null,"SS-PREP-009","Leaf Washing\nPlease advise with samples.",11,12.1]
[null,"SS-SING-136","Protein (Crude)\nIncludes Total Nitrogen (TN) and Crude Protein (Calculation).",33,36.299999999999997]
[null,"SS-SING-272","Starch Content (% in plant leaf or organic material)\n",84,92.4]
[]
[null,"FEED AND PRODUCE TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","FEED SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-107","Feed Package - Cereal Grain (NIR- Near-Infrared Analysis)\nFor oat, barley, wheat and triticale grains. \r\nIncludes Dry Matter/Moisture, Crude Protein, Acid Detergent Fibre, Neutral Detergent Fibre, Dry Matter Digestibility, Dry Organic Matter Digestibility and Metabolisable Energy, Starch and Sugar, Fat for oats. \r\n",110,121]
[null,"SS-PACK-109","Feed Package - Horse (NIR- Near-Infrared Analysis)\nFor hay, fresh cut pasture and cereal grains, includes Horse Digestible Energy. \r\nIncludes Dry Matter/Moisture, Crude Protein, Acid Detergent Fibre, Neutral Detergent Fibre, Dry Matter Digestibility, Dry Organic Matter Digestibility and Metabolisable Energy and Horse Digestible Energy.\r\n\r\n",110,121]
[null,"SS-PACK-108","Feed Package - Pelleted (NIR- Near-Infrared Analysis)\nFor pelleted and mixed feeds.\r\nIncludes Dry Matter/Moisture, Crude Protein, Acid Detergent Fibre, Neutral Detergent Fibre, Dry Matter Digestibility, Dry Organic Matter Digestibility and Metabolisable Energy, Fat and Ash. \r\n",110,121]
[null,"SS-PACK-106","Feed Package - Quality (NIR- Near-Infrared Analysis)\nFor hay, fresh cut pasture, straw, pasture silage and maize silage. \r\nIncludes Dry Matter/Moisture, Crude Protein, Acid Detergent Fibre, Neutral Detergent Fibre, Dry Matter Digestibility, Dry Organic Matter Digestibility and Metabolisable Energy. Depending on fodder type can include: Water Soluble Carbohydrates, Starch and Sugar, Fat and Ash. \r\n",110,121]
[null,"SS-PACK-145","Soluble Nitrogen - Feed\nIncludes Nitrate and Ammonium.",44,48.4]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL FEED TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-239","Cyanide (Total Prussic Acid in Plant/ Feed samples)\nIncludes sample preparation and Total Cyanide. ",110,121]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","PRODUCE SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-084","Produce Metals 1 (NATA Subcontracted)\nIncludes Cadmium and Lead.",104,114.4]
[null,"SS-PACK-085","Produce Metals 2 (NATA Subcontracted)\nIncludes Cadmium, Lead and Mercury.",120,132]
[null,"SS-PACK-083","Produce MRL - CR006 (C3/C5 Extended Residue)\nIncludes Standard Residue Screen - Analysis of Pesticides (Organo-chlorines (OC), Organo-phosphates (OP)), Herbicides, Phenols, Carbamates, Acaricides, Synthetic Pyrethroids, Fungicides, Other.",385,423.5]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL PRODUCE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-214","Produce - Single Metal\nIncludes Cadmium or Lead or Mercury. Includes preparation.",88,96.8]
[null,"SS-SING-211","Produce Bacto 1\nIncludes Produce Ecoli.",49,53.9]
[null,"SS-SING-212","Produce Bacto 2\nIncludes Produce Salmonella.",66,72.599999999999994]
[null,"SS-SING-213","Produce Bacto 3\nIncludes Produce Listeria.",60,66]
[null,"SS-SING-287","Produce Bacto 4\nIncludes Produce Faecal Coliforms.",49,53.9]
[]
[null,"COMPOST, BIOCHAR AND HAIR TESTING"]
[]
[null,null,null,null,"Basic Compost Testing Only. See Compost and Lanscape Soils Price List for comprehensive list."]
[null,"ITEM CODE","COMPOST SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-004","Compost Available Nutrients\nIncludes pH and EC; Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 200 g of sample is required.",135,148.5]
[null,"CA-PACK-001","Compost Total Nutrients\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se). Note: 200 g of sample is required.",110,121]
[null,"CA-PACK-019","Compost Total and Available Nutrients\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se); Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 300 g of sample is required.",210,231]
[null,"CA-PACK-020","Compost Total and Available Nutrients plus Heavy Metals\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag; Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 300 g of sample is required.  ",240,264]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIOCHAR SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-163","Biochar Totals Analysis Plus \nIncludes Moisture Content, Bulk Density; Ash Content and Loss on Ignition (750°C); pH, EC (1:10 water); Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC); Hydrogen, Oxygen Calc., H/Corg and O/Corg Calc; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Acid Neutralising Capacity (ANC). Note: 500 g of sample is required to complete testing.",470,517]
[null,"SS-PACK-143","Soil Testing for Biochar Application\nIncludes Moisture, pH, EC (1:5 water); Total Organic Carbon (TOC), Total Nitrogen (TN), TC/TN Ratio; Available Nitrogen (Nitrate); Soluble Chloride; Total Metals (Sb, As, Be, B, Cd, Co, Cu, Cr, Pb, Mn, Mo, Ni, Se, Sn, V, Zn, S, P, Hg); Soluble Cations (Ca, Mg, K, Na). Note: 300 g of sample is required to complete testing.",225,247.5]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","HAIR SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-050","Hair Tissue Mineral Analysis (HTMA) - Human and Animal\nIncludes Antimony, Aluminium, Arsenic, Barium, Beryllium, Bismuth, Boron, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium and Zinc.\r\nData only (no interpretation), Nitric Acid digest, minimum of 0.5 g of hair required which is equivalent to one heaped tablespoon. Collect from nape as close as possible to scalp as this reflects new growth.  Provide sample double bagged to avoid contamination when opened at the laboratory.",88,96.8]
[]
[null,"AGRICULTURAL WATER TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","AGRICULTURAL WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-007","Agricultural Stock Use\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Water Hardness; Total Alkalinity; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury; Nitrate, Ammonium, Phosphate; Faecal Coliforms.",135,148.5]
[null,"SW-PACK-005","Irrigation and Livestock Suitability – Comprehensive\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms and E.Coli Bacteria; Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Manganese, Nickel, Lead, Zinc; Nitrate, Ammonium, Phosphate; Sodium, Potassium, Calcium, Magnesium, Chloride, Sulfate, Sodium Absorption Ratio (SAR).",165,181.5]
[null,"SW-PACK-004","Irrigation Suitability - Basic\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Iron and Manganese; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride; Turbidity, Total Alkalinity, Water Hardness (calculation), Saturation Index; Sodium Absorption Ratio (SAR).",88,96.8]
[null,"SW-PACK-024","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Organo-phosphates (OP).",140,154]
[null,"SW-PACK-002","Water Quality - Basic \nFor drinking and domestic use.  Includes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms, E.Coli Bacteria.",77,84.7]
[null,"SW-PACK-003","Water Quality - Comprehensive\nFor drinking and domestic use. Includes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms and E.Coli Bacteria; Nitrate; Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Manganese, Nickel, Lead, Zinc, Mercury.",120,132]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL AGRICULTURAL WATER TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-022","Algae - Basic ID and Count (Blue Green Algae only) by Microscopic Identification\n",120,132]
[null,"SW-SING-123","Algae - Full ID and Count by Microscopic Identification\n",180,198]
[]
[null,"COMPOST AND LANDSCAPE SOIL ANALYTICAL SERVICES"]
[null,"COMPOST TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS4454 COMPOST PRODUCT SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-011","Mature Compost Analysis under AS4454\nIncludes Bulk Density; Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Bioassay; Plant Propagules, Nitrogen Drawdown Index, Specific Oxygen Uptake Rate, Solvita; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms. Acid Neutralising Capacity required if pH > 8.0. Note: 4 kg of sample required.",660,726]
[null,"CA-PACK-003","Composted Product Analysis under AS4454\nIncludes Bulk Density; Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Bioassay; Plant Propagules, Nitrogen Drawdown Index; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms. Acid Neutralising Capacity required if pH > 8.0. Note: 4 kg of sample required.",500,550]
[null,"CA-PACK-023","Pasteurized Product Analysis under AS4454\nIncludes Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; PO4; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Plant Propagules; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms. Acid Neutralising Capacity required if pH > 8.0. Note: 4 kg of sample required.",350,385]
[null,"CA-PACK-024","Raw Mulch Analysis under AS4454\nIncludes pH, EC; TOC, TN, TC/TN Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Plant Propagules; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls). Acid Neutralising Capacity required if pH > 8.0. Note: 4 kg of sample required.",200,220]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS4454 COMPOST BASIC SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-005","Compost Soluble Nutrients plus Carbon & Nitrogen under AS4454\nIncludes Moisture, pH, EC; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio. Note: 200 g of sample is required to complete testing. \r\n",99,108.9]
[null,"CA-PACK-013","LECO - Total Carbon, Total Nitrogen under AS4454/AS3743/AS4419\nIncludes Total Carbon (TC) and Total Nitrogen (TN), TC/TN Ratio. Note: 200 g of sample is required to complete testing.",38,41.8]
[null,"CA-PACK-014","Nutrients - Water Extractable under AS4454\nIncludes Moisture, Nitrate, Phosphate, Ammonium (1:5 water). Note: 200 g of sample is required to complete testing.\r\n",55,60.5]
[null,"CA-PACK-010","pH and EC under AS4454\nIncludes Moisture, pH and EC. Note: 200 g of sample is required to complete testing.",44,48.4]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","BASIC COMPOST SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-020","Compost Total and Available Nutrients plus Heavy Metals\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag; Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 300 g of sample is required.  ",240,264]
[null,"CA-PACK-019","Compost Total and Available Nutrients\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se); Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 300 g of sample is required.",210,231]
[null,"CA-PACK-001","Compost Total Nutrients\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se). Note: 200 g of sample is required.",110,121]
[null,"CA-PACK-004","Compost Available Nutrients\nIncludes pH and EC; Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 200 g of sample is required.",135,148.5]
[null,"CA-PACK-008","Compost Water Soluble Nutrients\nIncludes Moisture; Nitrate, Ammonium; Chloride; Calcium, Magnesium, Sodium, Potassium, Phosphorus, Sulfur, Boron, Copper, Iron, Manganese, Zinc, Aluminium, Molybdenum and Cobalt. Note: 200 g of sample is required to complete testing.",99,108.9]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","OTHER COMPOST SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-189","The Compost Order 2016 - Monitoring\nThis order applies to compost. In this order, compost means any combination of mulch, garden organics, food waste, manure and paunch that has undergone composting.             Includes physical contaminants with glass, metal, rigid plastics, light flexible film plastics. Also includes Salmonella, Ecoli and Faecal Coliforms. Note: 2 kg of sample is required to complete testing. ",200,220]
[null,"SS-PACK-142","The Compost Order 2016 - Compliance\nThis order applies to compost. In this order, compost means any combination of mulch, garden organics, food waste, manure and paunch that has undergone composting.             Includes physical contaminants with glass, metal, rigid plastics, light flexible film plastics, treated timber and asbestos. Also includes Salmonella, Ecoli and Faecal Coliforms. Note: 2 kg of sample is required to complete testing. ",240,264]
[null,"SS-PACK-190","The Pasteurised Garden Organics Order 2016 - Monitoring\nThis order applies to pasteurised garden organics. In this order, pasteurised garden organics means mulch and/or garden organics that have undergone the process of pasteurisation as a minimum.                                      \r\nIncludes physical contaminants with glass, metal, rigid plastics and light flexible film plastics. Note: 2 kg of sample is required to complete testing. ",44,48.4]
[null,"SS-PACK-170","The Pasteurised Garden Organics Order 2016 - Compliance\nThis order applies to pasteurised garden organics. In this order, pasteurised garden organics means mulch and/or garden organics that have undergone the process of pasteurisation as a minimum.                                      \r\nIncludes physical contaminants with glass, metal, rigid plastics, light flexible film plastics, treated timber and asbestos. Also includes Salmonella, Ecoli and Faecal Coliforms and plant propagules. Note: 2 kg of sample is required to complete testing. ",285,313.5]
[null,"SS-PACK-169","The Mulch Order 2016 - Compliance\nThis order applies to mulch. In this order, mulch means plant material shredded and/or screened to a preferred particle size grading for particular applications.                                  Includes particle Size > 5 mm and < 16 mm, physical contaminants with glass, metal, rigid plastics, light flexible film plastics, polystyrene, treated timber and asbestos. Also includes Salmonella, Ecoli and Faecal Coliforms. Also includes chemical contaminants Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls) and heavy metals. Note: 2 kg of sample is required to complete testing. ",350,385]
[null,"SS-PACK-026","Exchangeable Cations - 15D1 - 1 M NH4OAc\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-035","SOUR Test\nIncludes Moisture, Volatile Solids Concentration,  Specific Oxygen Uptake Rate (SOUR) with an incubation of 20oC.",110,121]
[null,"SS-PACK-197","Landscape Soil Testing (A1 A2 A3 A4) under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC (Water) pH (CaCl2); Soluble Chloride; Exchangeable Cations (pH and EC dependant); Available (Fe, Cu, Mn, Zn, B); Available Phosphorus (Colwell); Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles (2-20 mm, > 20 mm); Particle Size Distribution ( > 2.0 mm, 1.0-2.0 mm, 0.5-1.0 mm, 0.25-0.5 mm, 0.1-0.25 mm, 0.05-0.1 mm, 0.002-0.05 mm, < 0.002 mm); Dispersibility; Permeability (@ 16 drops); Water Repellence; Physical Contaminants. Note: 4 kg of sample is required to complete testing.",690,759]
[null,"SS-PACK-202","QLD Compost Characteristics 2023\nIncludes Bulk Density; Moisture, pH, EC; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm; Totals (As, Cd, Cr, Cu, Pb, Hg, Ni, Se, Zn); Plant Propagules (21 days), Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms. (Does NOT include trace level PFAS, TOPA or ASLP leachable PFAS. These are additional charges). Note: 2 kg of sample required.",410,451]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL COMPOST TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-090","Acid Neutralising Capacity (ANC-BT)\nThis method is used to measure Acid Neutralising Capacity (ANC-BT) where pH-KCl > 6.5.",33,36.299999999999997]
[null,"SS-SING-168","Ammonium (1:5 water) under AS4454\nIncludes moisture, extractable ammonium.",33,36.299999999999997]
[null,"SS-SING-139","Bulk Density under AS4454/AS3743\nLab based bulk density on compost and potting mix. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-062","Carbon - Organic by Walkley Black\n",44,48.4]
[null,"SS-SING-061","Carbon - Total Organic by LECO\n",33,36.299999999999997]
[null,"SS-SING-177","Carbon - Organic Matter under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC), Organic Matter by calculation.",44,48.4]
[null,"SS-SING-175","Carbon - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Carbon (TC). ",33,36.299999999999997]
[null,"SS-SING-176","Carbon - Total Organic (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC). ",44,48.4]
[null,"SS-SING-172","Chloride (1:5 water) under AS4454\nIncludes moisture, soluble chloride. ",33,36.299999999999997]
[null,"SS-SING-180","EC (1:5 water) under AS4454\nIncludes moisture, EC (1:5 water).\r\n",27,29.7]
[null,"SS-SING-170","Nitrate (1:5 water) under AS4454\nIncludes moisture, extractable nitrate.",33,36.299999999999997]
[null,"SS-SING-174","Nitrogen - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Nitrogen (TN). ",33,36.299999999999997]
[null,"SS-SING-119","Nitrogen Drawdown Index (NDI) under AS4454/AS4419\nNote: 2 kg of sample is required to complete testing.",104,114.4]
[null,"SS-SING-123","Particle Size Grading under AS4454\nIncludes percentage mass retained on 5 mm and 16 mm sieve. Note: 2 kg of sample is required to complete testing.",33,36.299999999999997]
[null,"SS-SING-178","pH (1:5 water) under AS4454\nIncludes moisture, pH (1:5 water).\r\n",27,29.7]
[null,"SS-SING-165","Phosphate (1:5 water) under AS4454\nIncludes moisture, extractable phosphate.",33,36.299999999999997]
[null,"SS-SING-145","Plant Growth Test (Bioassay) - TMECC 05.05-B\nIn-vitro germination and root elongation. Note: 1 L of sample is required to complete testing.",55,60.5]
[null,"SS-SING-189","Plant Growth Test (Bioassay) under AS4454\nUsed on fresh soils and composts.  Seedling emergence and relative root growth.  Note: 1 kg of sample is required to complete testing.",55,60.5]
[null,"SS-SING-219","Solids Energy Code (Calorific Value) \n",115,126.5]
[null,"SS-SING-245","Vermicast Sieve Test under AS4454:2012\nIncludes percentage mass retained on 1.18 mm sieve. Note: 1 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-137","Viable Plant Propagules under AS4454/AS3743\nNote: 1 kg of sample required to complete testing.",55,60.5]
[null,"SS-SING-122","Visible Contaminants under AS4454\nApplies to composts from agricultural or source separated organics. Includes contamination with glass, metal, rigid plastics, stones, lumps of clay, light flexible film plastics. Note: 2 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-072","Wettability under AS4454/AS3743\n",22,24.2]
[null,"SS-SING-292","AS4454:2012 Appendix K – Spent Mushroom Compost Classification       ",85,93.5]
[]
[null,"POTTING MIX TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS3743 POTTING MIX PRODUCT SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-007","Potting Mix and Growing Media - Premium under AS3743\nIncludes Moisture Content, Bulk Density, pH, EC (1:1.5 water); Chloride, Sodium, Calcium, Magnesium, Potassium, Phosphate, Nitrate, Ammonium, Sulfate, Iron, Copper, Manganese, Zinc, Boron; Air-Filled Porosity (AFP); Water Holding Capacity (WHC); Wettability; Plant Growth Bioassay (Toxicity Index), Nitrogen Drawdown Index (NDI). Note: 3 kg of sample is required to complete testing.\r\n\r\n",330,363]
[null,"CA-PACK-006","Potting Mix and Growing Media - Regular under AS3743\nIncludes Moisture Content, Bulk Density, pH, EC (1:1.5 water); Chloride, Sodium, Calcium, Magnesium, Potassium, Ammonium, Iron, Copper, Manganese, Zinc, Boron; Air-Filled Porosity (AFP), Water Holding Capacity (WHC); Wettability; Plant Growth Bioassay (Toxicity Index); Nitrogen Drawdown Index (NDI). Note: 3 kg of sample is required to complete testing.\r\n\r\n",300,330]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS3743 POTTING MIX BASIC SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-021","AFP and WHC under AS3743:2003\nIncludes Air-Filled Porosity (AFP) and Water Holding Capacity (WHC). Note: 2 kg of sample is required to complete testing.",55,60.5]
[null,"CA-PACK-017","Extractable Macronutrients (Ammonium Acetate) under AS3743\nIncludes Calcium, Magnesium, Sodium, Potassium, Phosphorus, Sulfur (1:1.5). Note: 200 g of sample is required to complete testing.",44,48.4]
[null,"CA-PACK-018","Extractable Micronutrients (DTPA) under AS3743\nIncludes Sodium, Calcium, Magnesium, Potassium, Phosphorus, Sulfur, Iron, Copper, Manganese, Zinc, Boron (1:1.5). Note: 200 g of sample is required to complete testing.",44,48.4]
[null,"CA-PACK-015","Nutrients - Water Extractable under AS3743\nIncludes Nitrate, Ammonium (1:1.5 water). Note: 200 g of sample is required to complete testing.\r\n ",44,48.4]
[null,"CA-PACK-016","pH and EC under AS3743\nIncludes pH and EC (1:1.5 water). Note: 200 g of sample is required to complete testing.",33,36.299999999999997]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL POTTING MIX TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-120","Air-filled Porosity (AFP) under AS3743\nNote: 2 kg of sample is required to complete testing.",27,29.7]
[null,"SS-SING-169","Ammonium (1:1.5 water) under AS3743\nIncludes extractable ammonium.",33,36.299999999999997]
[null,"SS-SING-139","Bulk Density under AS4454/AS3743\nLab based bulk density on compost and potting mix. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-177","Carbon - Organic Matter under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC), Organic Matter by calculation.",44,48.4]
[null,"SS-SING-175","Carbon - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Carbon (TC). ",33,36.299999999999997]
[null,"SS-SING-176","Carbon - Total Organic (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC). ",44,48.4]
[null,"SS-SING-173","Chloride (1:1.5 water) under AS3743\nIncludes soluble chloride. ",33,36.299999999999997]
[null,"SS-SING-181","EC (1:1.5 water) under AS3743\n\r\n",16,17.600000000000001]
[null,"SS-SING-171","Nitrate (1:1.5 water) under AS3743\nIncludes extractable nitrate.",33,36.299999999999997]
[null,"SS-SING-174","Nitrogen - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Nitrogen (TN). ",33,36.299999999999997]
[null,"SS-SING-188","Nitrogen Drawdown Index (NDI) under AS3743\nNote: 2 kg of sample is required to complete testing.",104,114.4]
[null,"SS-SING-179","pH (1:1.5 water) under AS3743\n",16,17.600000000000001]
[null,"SS-SING-166","Phosphate (1:1.5 water) under AS3743/AS4419\nIncludes extractable phosphate.",33,36.299999999999997]
[null,"SS-SING-190","Plant Growth Test (Bioassay) under AS3743/AS4419\nUsed on fresh soils and composts.  Seedling emergence and relative root growth.  Note: 1 kg of sample is required to complete testing.",55,60.5]
[null,"SS-SING-137","Viable Plant Propagules under AS4454/AS3743\nNote: 1 kg of sample required to complete testing.",55,60.5]
[null,"SS-SING-121","Water Holding Capacity (WHC) under AS3743\nNote: 2 kg of sample is required to complete testing.",27,29.7]
[null,"SS-SING-072","Wettability under AS4454/AS3743\n",22,24.2]
[]
[null,"LANDSCAPE SOIL TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS4419:2018 SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-120","Landscape Soils (On Grade) compliance under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles; Bioassay; Water Repellence; Physical Contaminants; Chemical Contaminants (Heavy Metals and Low Level (Pesticides, PCB)); Plant Propagules. Note: 4 kg of sample is required to complete testing.",550,605]
[null,"SS-PACK-127","Landscape Soils (On Grade) monitoring under AS4419:2018 \nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles; Bioassay; Water Repellence. Note: 4 kg of sample is required to complete testing.",350,385]
[null,"SS-PACK-121","Low Density Media (On Slab) compliance under AS4419:2018\nIncludes Bulk Density; pH and EC; Air-Filled Porosity; Water Holding Capacity; Available Phosphorus; Available Nitrogen (Ammonium), Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Nitrogen Drawdown Index; Physical Contaminants; Chemical Contaminants (Heavy Metals and Low Level (Pesticides, PCB)); Plant Propagules. Note: 4 kg of sample is required to complete testing.\r\n",460,506]
[null,"SS-PACK-128","Low Density Media (On Slab) monitoring under AS4419:2018\nIncludes Bulk Density; pH and EC; Air-Filled Porosity; Water Holding Capacity; Available Phosphorus; Available Nitrogen (Ammonium), Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Nitrogen Drawdown Index. Note: 3 kg of sample is required to complete testing.\r\n",260,286]
[null,"SS-PACK-122","Soils for Turf and Lawns compliance under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles; Dispersibility; Permeability; Water Repellence; Physical Contaminants; Chemical Contaminants (Heavy Metals and Low Level (Pesticides, PCB)); Plant Propagules. Note: 4 kg of sample is required to complete testing.",600,660]
[null,"SS-PACK-129","Soils for Turf and Lawns monitoring under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles; Dispersibility; Permeability; Water Repellence. Note: 3 kg of sample is required to complete testing.",400,440]
[null,"SS-PACK-123","Structural Support Soil and Wetlands compliance under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Nitrate); Organic Matter (Total Organic Carbon); Water Repellence; Permeability; Physical Contaminants; Chemical Contaminants (Heavy Metals and Low Level (Pesticides, PCB)); Plant Propagules. Note: 4 kg of sample is required to complete testing. Particle Size Analysis not included (SS-SING-243 Wetlands & SS-SING-244 Structural Support).",540,594]
[null,"SS-PACK-130","Structural Support Soil and Wetlands monitoring under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Nitrate); Organic Matter (Total Organic Carbon); Water Repellence; Permeability. Note: 3 kg of sample is required to complete testing.",340,374]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS4419 SOIL BASIC SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-013","LECO - Total Carbon, Total Nitrogen under AS4454/AS3743/AS4419\nIncludes Total Carbon (TC) and Total Nitrogen (TN), TC/TN Ratio. Note: 200 g of sample is required to complete testing.",38,41.8]
[null,"SS-PACK-131","pH and EC under AS4419:2018\nIncludes pH and EC (1:5 water) except low density soils. Note: 200 g of sample is required to complete testing.",27,29.7]
[null,"SS-PACK-146","pH and EC under AS4419:2018\nIncludes pH and EC (1:1.5 water) for low density soils. Note: 200 g of sample is required to complete testing.",33,36.299999999999997]
[null,"SS-PACK-191","Sportsturf Practical Drainage Suite under AS4419:2018\nIncludes Bulk Density (8, 16, 32 drops), Permeability (8, 16, 32 drops) and Water Holding Capacity. Note 1 kg of sample is required to complete testing.",140,154]
[null,"SS-PACK-132","Total Available Nitrogen under AS4419:2018\nIncludes KCl extractable Nitrate and Ammonium. Note 200 g of sample is required to complete testing.",27,29.7]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","OTHER SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-034","Micronutrients - 12A1 - DTPA Extractable \nIncludes Iron, Copper, Zinc, Manganese.",44,48.4]
[null,"SS-PACK-027","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.\r\n\r\n\r\n ",77,84.7]
[null,"SS-PACK-026","Exchangeable Cations - 15D1 - 1 M NH4OAc\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-001","Exchangeable Cations - 15D3 - 1 M NH4OAc plus Acidity (15G1)\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0 and exchangeable acidity (Hydrogen + Aluminium) by 1 M KCl.\r\n\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-205","Exchangeable Cations - 15D1 - 1 M NH4OAc plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.",74,81.400000000000006]
[null,"SS-PACK-206","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl  plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.",95,104.5]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-183","Bulk Density under AS4419\nLab based bulk density on landscape soils. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-274","Bulk Density under AS4419:2018 \nThis includes 8, 16 and 32 drops. Note 1kg of sample is required to complete testing.",66,72.599999999999994]
[null,"SS-SING-177","Carbon - Organic Matter under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC), Organic Matter by calculation.",44,48.4]
[null,"SS-SING-175","Carbon - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Carbon (TC). ",33,36.299999999999997]
[null,"SS-SING-176","Carbon - Total Organic (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC). ",44,48.4]
[null,"SS-SING-172","Chloride (1:5 water) under AS4454\nIncludes moisture, soluble chloride. ",33,36.299999999999997]
[null,"SS-SING-167","Dispersibility under AS4419\n",44,48.4]
[null,"SS-SING-180","EC (1:5 water) under AS4454\nIncludes moisture, EC (1:5 water).\r\n",27,29.7]
[null,"SS-SING-229","Water repellence of soil under AS4419:2018\nIncludes water repellence of soil and if required, further testing to ethanol repellence of soil. Note: 200 g of sample is required to complete testing.",15,16.5]
[null,"SS-SING-174","Nitrogen - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Nitrogen (TN). ",33,36.299999999999997]
[null,"SS-SING-119","Nitrogen Drawdown Index (NDI) under AS4454/AS4419\nNote: 2 kg of sample is required to complete testing.",104,114.4]
[null,"SS-SING-243","Particle Size Analysis for Wetlands under AS4419:2018\nParticle size of sediment and soil by hydrometer and sieve. Percentage mass retained on sieve. Includes > 2 mm, 1.0–2.0 mm, 0.5–1.0 mm, 0.25–0.5 mm, 0.1–0.25 mm, 50 µm–0.1 mm, 2–50 µm, < 2 µm fractions.  Note: 500 g of sample is required to complete testing.      ",120,132]
[null,"SS-SING-184","Particles Size Grading - Large particles under AS4419:2003\nIncludes percentage mass retained on 10 mm, 20 mm, 50 mm and 75 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-226","Particles Size Grading - Large particles under AS4419:2018\nIncludes percentage mass retained on 2 mm, 5 mm, 20 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-244","Particles Size Grading for Structural Support under AS4419:2018\nIncludes percentage mass passing on 63.0 mm, 53.0 mm, 37.5 mm, 26.5 mm, 19.0 mm, 13.2 mm, 4.75 mm fractions. Note: 2 kg of sample is required to complete testing.",66,72.599999999999994]
[null,"SS-SING-156","Permeability under AS4419:2003\nNote: 2 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-230","Permeability under AS4419:2018\nThis includes 8, 16 and 32 drops. Note: 1 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-178","pH (1:5 water) under AS4454\nIncludes moisture, pH (1:5 water).\r\n",27,29.7]
[null,"SS-SING-166","Phosphate (1:1.5 water) under AS3743/AS4419\nIncludes extractable phosphate.",33,36.299999999999997]
[null,"SS-SING-033","Phosphorus - Colwell\nIncludes Phosphorus for alkaline soils.",22,24.2]
[null,"SS-SING-034","Phosphorus - Olsen\nIncludes Olsen Phosphorous - a measure of the intensity of Phosphorus.",22,24.2]
[null,"SS-SING-228","Physical Contaminants under AS4419:2018\nApplies to soil types as identified by AS4419:2018. Includes contamination with glass, metal, rigid plastics, light flexible film plastics. Note: 2 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-190","Plant Growth Test (Bioassay) under AS3743/AS4419\nUsed on fresh soils and composts.  Seedling emergence and relative root growth.  Note: 1 kg of sample is required to complete testing.",55,60.5]
[null,"SS-SING-164","Texture - Full under AS4419\n",27,29.7]
[null,"SS-SING-227","Top Dress - Particles under AS4419:2018\nIncludes percentage mass retained of organics particles on 2 mm, 5 mm, 8 mm sieve. Also mass retained of mineral particles on 2 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-275","Water Holding Capacity under AS4419:2018\nNote: 500g of sample is required to complete testing.",27,29.7]
[null,"SS-SING-182","Wettability under AS4419\n\r\n",22,24.2]
[]
[null,"MAIN ROAD (MRTS AND R178) TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","MRTS SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-090","MRTS16 FORM C Topsoil Testing (2017)\nIncludes Bulk Density; Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC), Organic Matter; Wettability; pH and EC (1:5 water); Texture; Permeability; Extractable Phosphorus, Chloride; MCP Sulfur; Large Particles; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio Effective Cation Exchange Capacity; Water Repellence Class. Note: 4 kg of sample is required to complete testing.",330,363]
[null,"SS-PACK-067","MRTS16 FORM D Manufactured Site Topsoil Compliance Testing (2017)\nIncludes Total Organic Carbon (TOC), Organic Matter; pH and EC (1:5 water); Texture; Extractable Chloride; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Dispersion (Emerson Class); Water Repellence Class. Note: 1 kg of sample is required to complete testing.",210,231]
[null,"SS-PACK-093","MRTS16 FORM E Subsoil Testing (2017)\nIncludes Wettability; pH and EC (1:5 water); Texture; Extractable Chloride; MCP Sulfur; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Dispersion (Emerson Class); Water Repellence Class; Slaking Class; Clouding (Dispersion) Class. Note: 1 kg of sample is required to complete testing.",220,242]
[null,"SS-PACK-097","MRTS16 FORM F Drainage Basin Soil Testing (2017)\nIncludes Moisture Content; pH and EC (1:5 water); Extractable Chloride; MCP Sulfur; Dispersion (Emerson Class); Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Dispersion (Emerson Class); Slaking Class; Clouding (Dispersion) Class. Note: 1 kg of sample is required to complete testing.",210,231]
[null,"SS-PACK-100","MRTS16 FORM G Organic Soil Conditioner Testing (2017)\nIncludes Bulk Density; Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Bioassay; Plant Propagules, Nitrogen Drawdown Index, Specific Oxygen Uptake Rate, Solvita; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms; Legionella, Listeria; Asbestos; PFAS - Low Level. Acid Neutralising Capacity required if pH > 8.0. Note: 5 kg of sample required.",1160,1276]
[]
[]
[null,"ITEM CODE","MRTS WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-070","MRTS - FORM I - Non-potable Water Testing and Assessment Report\nIncludes pH, EC; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride, Sodium Absorption Ratio (SAR); Bicarbonate / Carbonate Alkalinity;  Salmonella, Ecoli, Total Coliforms.",165,181.5]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","R178 SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-095","R178 FORM E1 Subsoil Testing (2017)\nIncludes Wettability; pH and EC (1:5 water); Texture; Extractable Phosphorus, Extractable Chloride; MCP Sulfur; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Water Repellence Class; Slaking Class; Clouding (Dispersion) Class. Note: 1 kg of sample is required to complete testing.",220,242]
[null,"SS-PACK-092","R178 FORM E2 Topsoil Testing - Site Won, Manufactured and Imported  (2017)\nIncludes Bulk Density; Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC), Organic Matter; Wettability; pH and EC (1:5 water); Texture; Permeability; Extractable Phosphorus, Chloride; MCP Sulfur; Large Particles; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio Effective Cation Exchange Capacity; Dispersion (Emerson Class); Water Repellence Class; Slaking Class; Clouding (Dispersion) Class. Note: 4 kg of sample is required to complete testing.",330,363]
[null,"SS-PACK-099","R178 FORM E3 Drainage Basin Soil Testing (2017)\nIncludes Moisture Content; pH and EC (1:5 water); Extractable Chloride; MCP Sulfur; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Dispersion (Emerson Class); Slaking Class; Clouding (Dispersion) Class. Note: 1 kg of sample is required to complete testing.",190,209]
[null,"SS-PACK-101","R178 FORM G1 Organic Soil Conditioner Testing (2017)\nIncludes Bulk Density; Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Bioassay; Plant Propagules, Nitrogen Drawdown Index, Specific Oxygen Uptake Rate, Solvita; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms; Legionella, Listeria; Asbestos. Acid Neutralising Capacity required if pH > 8.0. Note: 5 kg of sample required.",940,1034]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","OTHER SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-078","Exchangeable Cations - 15B3 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium.\r\n\r\n\r\n\r\n\r\n\r\n",60,66]
[null,"SS-PACK-027","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.\r\n\r\n\r\n ",77,84.7]
[null,"SS-PACK-207","Exchangeable Cations - 15B3 - 1 M NH4Cl plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium.",74,81.400000000000006]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-183","Bulk Density under AS4419\nLab based bulk density on landscape soils. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-177","Carbon - Organic Matter under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC), Organic Matter by calculation.",44,48.4]
[null,"SS-SING-172","Chloride (1:5 water) under AS4454\nIncludes moisture, soluble chloride. ",33,36.299999999999997]
[null,"SS-SING-167","Dispersibility under AS4419\n",44,48.4]
[null,"SS-SING-025","Emerson Aggregate Test (EAT)\nProvides an Emerson Dispersion Class",49,53.9]
[null,"SS-SING-184","Particles Size Grading - Large particles under AS4419:2003\nIncludes percentage mass retained on 10 mm, 20 mm, 50 mm and 75 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-226","Particles Size Grading - Large particles under AS4419:2018\nIncludes percentage mass retained on 2 mm, 5 mm, 20 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-156","Permeability under AS4419:2003\nNote: 2 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-034","Phosphorus - Olsen\nIncludes Olsen Phosphorous - a measure of the intensity of Phosphorus.",22,24.2]
[null,"SS-SING-196","Slaking and Clouding - Test Methods Q161 and Q162\n",33,36.299999999999997]
[null,"SS-SING-082","Sulfur - MCP\n",22,24.2]
[null,"SS-SING-164","Texture - Full under AS4419\n",27,29.7]
[null,"SS-SING-197","Water repellence of soil - Test Method Q160\n",16,17.600000000000001]
[null,"SS-SING-182","Wettability under AS4419\n\r\n",22,24.2]
[]
[null,"CONTAMINATION TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","CONTAMINATION SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-004","Basic Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Aluminium, Arsenic, Beryllium, Boron, Cadmium, Chromium, Cobalt, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",77,84.7]
[null,"SS-PACK-055","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Polychlorinated Biphenyls (PCB).",135,148.5]
[null,"SS-PACK-056","Pesticide Screen 2b - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",140,154]
[null,"SS-PACK-118","Residue Screen - Extended (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",310,341]
[null,"SS-PACK-119","Residue Screen - Complete + Glyphosate (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue) + Glyphosate Screens.",470,517]
[null,"SS-PACK-045","Total Acid Extractable - Heavy Metals  (ICPMS)\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",55,60.5]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL CONTAMINATION TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-063","Asbestos Identification (Not Quantifiable)\nIdentification in building material, soil, compost and dust.",77,84.7]
[null,"SS-SING-157","Glyphosate (Round Up) + AMPA Screen (All dried solids)\n",280,308]
[null,"SS-SING-056","Organo-chlorines (OC) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-057","Organo-phosphates (OP) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-224","PFAS in ASLP leachate – standard level 28 suite with detection to 0.01 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in ASLP (Australian Standard Leachate Procedure) leachate.\r\n",230,253]
[null,"SS-SING-216","PFAS in solid – standard level 28 suite with detection 0.01 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",190,209]
[null,"SS-SING-253","PFAS in solid – LOW level 28 suite with detection 0.0008-0.0016 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",210,231]
[null,"SS-SING-278","PFAS-28 Standard Level - TOPA\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus PFAS Precursor compounds.",360,396]
[null,"SS-SING-279","PFAS-28 Standard Level - TOF\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus any Total Organofluorine compounds.",230,253]
[null,"SS-SING-058","Polychlorinated Biphenyls (PCB) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-140","Synthetic Pyrethroids\n",135,148.5]
[null,"SS-SING-288","PFAS Full Suite – 30 Trace Compounds (0.1 µg/kg)                                        \n",370,407]
[null,"SS-SING-289","TOPA – PFAS Full Suite – 30 Trace Compounds (0.1 µg/kg)                                  \n",435,478.5]
[null,"SS-SING-290","ASLP Leachate – PFAS Full Suite – 30 Trace Compounds (0.001-0.005 µg/L)                      \n",370,407]
[null,"SS-SING-291","TOF – Total OrganoFluorine                   \n",280,308]
[null,"SS-SING-285","Contamination Foreign Material Fraction Percentage – Modified RMS T276\nIncludes Fraction % (Rubber, plastic, bitumen, paper, cardboard, cloth, paint, glass, metal, Timber (engineered, painted, coated or treated)other vegetable matter). Includes photo per sample and each individual fraction.",150,165]
[]
[null,"BIOLOGICAL AND MICROBIAL TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","MICROBIAL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-185","Cryptosporidium and Giardia \nNote: 500 g of sample is required to complete testing.",940,1034]
[null,"SS-PACK-141","Microbial Biomass Assessment - Compost \nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-166","Microbial Biomass Assessment - Soil with high Organics\nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-140","Microbial Biomass Assessment - Soil\nIncludes biomasses of 12 microbial groups relevant for soil quality, health and function. ",285,313.5]
[null,"SS-PACK-167","MIC-01: Basic Analysis of Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Total fungi (moulds), Gram negative bacteria, Filamentous actinomycetes, Yeasts. ",99,108.9]
[null,"SS-PACK-168","MIC-02: Extended Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Filamentous actinomycetes, Actinobacteria, Gram negative bacteria, Filamentous fungi (Moulds), Yeasts, Lactic acid bacteria, Total Anaerobes (includes facultative anaerobes), Sulfite Reducing Anaerobes.",210,231]
[null,"SS-PACK-175","Phytophthora and Pythium\nNote: 500 g of sample is required to complete testing.",165,181.50000000000003]
[null,"SS-PACK-176","General Plant Pathogen Scan\nNote: 500 g of sample is required to complete testing.",385,423.5]
[null,"SS-PACK-059","Pathogens\nIncludes Moisture, Ecoli, Faecal Coliforms, Salmonella.",155,170.5]
[null,"SS-PACK-184","General Plant Pathogen Scan Plus\nGeneral plant pathogen scan including Phytophthora, Pythium, Rhizoctonia and Fusarium.\r\n\r\nNote: 500 g of sample is required to complete testing.",550,605]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL MICROBIAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-047","Aerobic Plate Count\n",44,48.4]
[null,"SS-SING-265","Bacillus cereus\n",135,148.5]
[null,"SS-SING-266","Clostridium perfringens\n",82,90.2]
[null,"SS-SING-267","Campylobacter\n",165,181.5]
[null,"SS-SING-044","E.Coli\n",44,48.4]
[null,"SS-SING-043","Faecal Coliforms\n",44,48.4]
[null,"SS-SING-268","Legionella spp plus longbeachae\nIncludes Legionella spp plus longbeachae in solids.",140,154]
[null,"SS-SING-046","Listeria\n",66,72.599999999999994]
[null,"SS-SING-269","Nematodes\n",110,121]
[null,"SS-SING-045","Salmonella\n",66,72.599999999999994]
[null,"SS-SING-262","Microbiometer – Soil biomass measurement\nIncludes estimates of Total Bacteria, Fungi and Fungi:Bacteria ratio. This test should only be done in conjunction with SS-Pack-167 or SS-Pack-168.",33,36.299999999999997]
[null,"SS-SING-195","SOLVITA - Compost Emissions Maturity Test\nIncludes measurement of carbon dioxide and ammonia gas released from compost due to biological activity.",66,72.599999999999994]
[null,"SS-SING-209","SOLVITA - Soil CO2 Burst\nIncludes measurement of carbon dioxide released from soil due to biological activity.",66,72.599999999999994]
[]
[null,"BIOCHAR, FILTER MEDIA AND BIOSOLID TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIOCHAR SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-163","Biochar Totals Analysis Plus \nIncludes Moisture Content, Bulk Density; Ash Content and Loss on Ignition (750°C); pH, EC (1:10 water); Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC); Hydrogen, Oxygen Calc., H/Corg and O/Corg Calc; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Acid Neutralising Capacity (ANC). Note: 500 g of sample is required to complete testing.",470,517]
[null,"SS-PACK-111","Biochar Totals Analysis\nIncludes Moisture Content, Bulk Density; Ash Content and Loss on Ignition (750°C); pH, EC (1:10 water); Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC), TC/TN Ratio, Organic Matter; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Acid Neutralising Capacity (ANC). Note: 200 g of sample is required to complete testing.",250,275]
[null,"SS-PACK-149","Biochar Ultimate Analysis\nIncludes Total Organic Carbon, Total Carbon, Total Nitrogen, Total Hydrogen and Ash Content. Oxygen Calc., H/Corg and O/Corg Calc. ",315,346.5]
[null,"SS-PACK-150","Biochar Density and Ashing\nIncludes moisture with % ash and volatiles.",77,84.7]
[null,"SS-PACK-153","Biochar Heavy Metals\nIncludes Pb, Cd, Hg, As, Cu, Ni, Zn and Cr.",88,96.8]
[null,"SS-PACK-154","Biochar Dioxin / Furans (<17 ng/kg) \n",1050,1155]
[null,"SS-PACK-155","Biochar Particle Size Analysis - Dry Sieving\nDry sieving for fractions > 2 mm, 1-2 mm, 500 µm-1 mm, 250-500 µm, 125-250 µm, 63-125 µm, < 63 µm.",99,108.9]
[null,"SS-PACK-156","Biochar Surface Area (Total and External)\n",330,363]
[null,"SS-PACK-143","Soil Testing for Biochar Application\nIncludes Moisture, pH, EC (1:5 water); Total Organic Carbon (TOC), Total Nitrogen (TN), TC/TN Ratio; Available Nitrogen (Nitrate); Soluble Chloride; Total Metals (Sb, As, Be, B, Cd, Co, Cu, Cr, Pb, Mn, Mo, Ni, Se, Sn, V, Zn, S, P, Hg); Soluble Cations (Ca, Mg, K, Na). Note: 300 g of sample is required to complete testing.",225,247.5]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIORETENTION FILTER MEDIA SUITES AND INDIVIDUAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-160","Bioretention Filter Media Analysis (FMSBS 2015)\nIncludes Moisture, pH, EC; Total Organic Carbon, Total Nitrogen, Organic Matter; Phosphate; Dry Sieving >2.0 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm; Bridging Criteria; Hydraulic Conductivity. Note: 3 kg of sample is required to complete testing.",330,363]
[null,"SS-PACK-171","Bioretention Transition Layer Analysis (FMSBS 2015)\nIncludes Dry Sieving >2.0 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm; Bridging Criteria; Hydraulic Conductivity. Note: 3 kg of sample is required to complete testing.",190,209]
[null,"SS-PACK-172","Bioretention Drainage Layer Analysis (FMSBS 2015)\nIncludes Dry Sieving > 5.0 mm, 3.4-5.0 mm, 2.0-3.4 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm; Bridging Criteria; Hydraulic  Conductivity. Note: 3 kg of sample is required to complete testing.",165,181.5]
[null,"SS-SING-231","Saturated Hydraulic Conductivity under ASTM F1815 - 11\nNote: 1 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-254","Particle Size Analysis - Dry Sieving (FMSBS 2015)\nDry sieving for fractions >2.0 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm.",82,90.2]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIOSOLIDS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"BS-PACK-001","Contaminated Grade Assessment\nIncludes Total Dry Solids Concentration, Metals Analysis Arsenic, Cadmium, Chromium, Copper, Lead, Mercury, Nickel, Selenium, Zinc; Low Level (Organo-chlorines Pesticides (OC), Polychlorinated biphenyls (PCB)).",250,275]
[null,"BS-PACK-004","Enteric Viruses Determination\nIncludes Reovirus, Enterovirus, Adenovirus (viruses per 10 g).",460,506]
[null,"BS-PACK-006","Enteric Viruses Determination plus Helminth Ova\nIncludes Reovirus, Enterovirus, Adenovirus (viruses per 10 g) plus Helminth Ova.",550,605]
[null,"BS-PACK-002","Nutrient Determination\nIncludes Moisture Content; Total Nitrogen (TN), Total Phosphorus, Total Kjeldahl Nitrogen (TKN) (by calculation); and available Nutrients (1:10 KCL extractable Nitrate, Ammonium).",99,108.9]
[null,"BS-PACK-005","SOUR Test\nIncludes Moisture, Volatile Solids Concentration, Specific Oxygen Uptake Rate (SOUR) with an incubation of 20oC.",110,121]
[null,"BS-PACK-003","Stabilisation Confirmation\nIncludes Moisture, Microbial Assessment (E.Coli, Faecal Coliforms, and Salmonella sp.), Volatile Solids Concentration, Specific Oxygen Uptake Rate (SOUR).",220,242]
[]
[null,"CONTAMINATION ASSESSMENT ANALYTICAL SERVICES"]
[null,"SOIL ASSESSMENT TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SPECIFIC SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-015","Aggressivity Assessment\nIncludes Moisture, Basic Texture; pH, EC, Resistivity (calculation), Soluble Chloride, Sulfate.",77,84.7]
[null,"SS-PACK-154","Biochar Dioxin / Furans (<17 ng/kg) \n",1050,1155]
[null,"SS-PACK-186","EPA Resource Recover Order - Waste 2017\nAnalysis of solids for moisture content and dry weight analysis of pH, EC (1:5 water), Soluble Cations and Anions (1:5 water extraction with 0.2micron filtration for Na, K, Ca, Mg, Cl, NO3), TN, TOC (LECO), and metals (Aqua regia digest and ICPMS analysis of (S, P, Sb, As, Be, B, Cd, Co, Cu, Cr, Pb, Mn, Mo, Ni, Se, Sn, V, Zn, Hg) 200g dry weight equivalent of sample requested in a jar of plastic bag.",200,220]
[null,"SS-PACK-053","Concrete Quality Analysis\nIncludes concrete crushing, Chloride and Sulfate.",88,96.8]
[null,"SS-PACK-005","Contaminated Site Assessment 1a\nIncludes Basic Texture; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury, Boron, Cobalt, Beryllium; Pesticides (Organo-chlorines (OC), Organo-phosphates (OP)).",140,154]
[null,"SS-PACK-006","Contaminated Site Assessment 1b\nIncludes Basic Texture; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury, Boron, Cobalt, Beryllium; Pesticides (Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB)).",165,181.5]
[null,"SS-PACK-007","Contaminated Site Assessment 2a\nIncludes Basic Texture; Arsenic, Lead; Pesticides (Organo-chlorines (OC), Organo-phosphates (OP)).",120,132]
[null,"SS-PACK-147","Contaminated Site Assessment 2b\nIncludes Basic Texture; Arsenic, Lead; Pesticides (Organo-chlorines (OC)).",110,121]
[null,"SS-PACK-008","Contaminated Site Assessment 3\nIncludes Basic Texture; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury, Boron, Cobalt, Beryllium; Pesticides (Organo-chlorines (OC)).",135,148.5]
[null,"SS-PACK-051","Excavated Natural Material (ENM) Classification 2014\nIncludes pH, EC (1:5 water); Foreign Material; Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury; Polycyclic Aromatic Hydrocarbons (PAH); Total Petroleum Hydrocarbons (C10-C40), BTEX (C6-C10).",285,313.5]
[null,"SS-PACK-177","Foundry Sand Analysis- RRO, 2014 \nIncludes pH, EC (1:5 water), Total Metals (Hg, Cd, Pb, As, Be, Cr, Cu, Mo, Ni, Se, Ag, Zn) and Total Fluoride (fusion method). \r\n\r\n",165,181.5]
[null,"SS-PACK-042","Health Investigation Level (HIL) Soil Assessment\nIncludes Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury, Beryllium, Boron, Cobalt; Polycyclic Aromatic Hydrocarbons (PAH), Total Petroleum Hydrocarbons (TPH), BTEX Hydrocarbons; Pesticides (Organo-chorines (OC)); Total Phenols; Total Cyanide.",350,385]
[null,"SS-PACK-023","Recovered Aggregate Exemption 2014 (suitable for waste aggregate, soil or concrete)\nIncludes EC; Mercury, Cadmium, Lead, Arsenic, Chromium, Copper, Nickel, Zinc; Fraction % (metal, plaster, rubber, plastic, paper, cloth, paint, wood, other vegetable matter).",120,132]
[null,"SS-PACK-065","Recovered Fines Order EPA 2014 Testing\nIncludes pH, EC (1:5 water); Foreign Material; Particle Size; Total Organic Carbon; Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury; Polycyclic Aromatic Hydrocarbons (PAH); Total Petroleum Hydrocarbons (C10-C36), BTEX (C6-C9); Pesticides (Organochlorine Pesticides (OC); Polychlorinated Biphenyls (PCB); Volatile Hydrocarbons (VHC).",550,605]
[null,"SS-PACK-104","Resource Recovery Exemption Analysis EPA 2017\nIncludes Moisture Content; pH, EC; Total Organic Carbon, Total Nitrogen, C/N Ratio; Soluble Cations (Sodium, Potassium, Calcium, Magnesium), Soluble Anions (Chloride, Nitrate); Totals (Antimony, Arsenic, Beryllium, Boron, Cadmium, Cobalt, Copper, Chromium, Lead, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Selenium, Sulfur, Tin, Vanadium, Zinc).",300,330]
[null,"SS-PACK-182","Soil/ Sediment Contamination Assessment\nIncludes Metals (Total Available Al, As, Cd, Cr, Cu, Fe Pb, Mn, Hg, Ni, Se, Ag, Zn), PAH, TPH, BTEX, and speciated Phenolics.",240,264]
[null,"SS-PACK-066","The Recovered Glass Sand Order 2014\nIncludes EC; Total Organic Carbon (TOC); Mercury, Cadmium, Lead, Arsenic, Chromium, Copper, Nickel, Zinc, Molybdenum; Fraction % (Plaster, clay lumps and other friable materials. Rubber, plastic, bitumen, paper, cloth, paint, wood and other vegetation matter).",150,165]
[null,"SS-PACK-080","Treated Drilling Mud Exemption 2014\nIncludes pH, EC (1:5 water); Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury; Polycyclic Aromatic Hydrocarbons (PAH); Total Petroleum Hydrocarbons (C10-C36), BTEX (C6-C9), Total Chlorinated Hydrocarbons (TCH).",310,341]
[null,"SS-PACK-105","Treated Grease Trap Waste Order EPA 2014 \nIncludes Moisture Content; pH, EC; Oil and Grease; Total Nitrogen; Totals (Arsenic, Cadmium, Chromium, Copper, Lead, Mercury, Nickel, Selenium and Zinc); Available Boron. ",200,220]
[null,"SS-PACK-148","Waste Material Biomethane Potential (BMP)\nIncludes BMP analysis using COD, Total Solids, Volatile solids (VS) and methane production normalised on a VS basis (includes assessment report with cumulative gas production graphs).\r\nNote: typically an 8 week production trial and limited sample numbers of 4 per batch) (estimated 2kg of sample solids/ sludge required for analysis.\r\n",1300,1430]
[null,"SS-PACK-198","Resource Recovery Plasterboard Order 2014 (suitable for recovered plasterboard)\nIncludes moisture content; pH (1:5 water); Metals (Mercury, Cadmium, Lead, Arsenic, Chromium, Copper, Molybdenum, Nickel, Selenium and Zinc); Nutrients/ salts (Calcium, Magnesium, Sodium and Sulfur); reporting Gypsum as % CaSO4.2H2O; and Soluble Chloride reported as % ClO2 (500g of sample requested).",170,187]
[null,"SS-PACK-201","Coffee Pod Analysis\nIncludes moisture content, coffee content, volatile content (plastic, lacquer, paint), aluminium content.",275,302.5]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","RESIDUE SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-147","Contaminated Site Assessment 2b\nIncludes Basic Texture; Arsenic, Lead; Pesticides (Organo-chlorines (OC)).",110,121]
[null,"SS-PACK-030","Contaminated Site Assessment 4 - Dip Site Screening Analysis\nIncludes Total Arsenic and Organo-chlorines (OC). Designed for dip site assessments.",88,96.8]
[null,"SS-PACK-013","Pesticide Screen 1a\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).",88,96.8]
[null,"SS-PACK-014","Pesticide Screen 1b\nIncludes Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",110,121]
[null,"SS-PACK-055","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Polychlorinated Biphenyls (PCB).",135,148.5]
[null,"SS-PACK-056","Pesticide Screen 2b - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",140,154]
[null,"SS-PACK-017","Petroleum Compounds Assessment 1a\nIncludes Total Petroleum Hydrocarbons (TPHC10-C40), BTEX (equivalent to TPHC6- C10).",99,108.9]
[null,"SS-PACK-018","Petroleum Compounds Assessment 1b (Total and Speciated)\nIncludes Total Petroleum Hydrocarbons (TPHC10-C40), BTEX (equivalent to TPHC6- C10), Speciated Total Petroleum Hydrocarbons (aromatic and aliphatic).",310,341]
[null,"SS-PACK-118","Residue Screen - Extended (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",310,341]
[null,"SS-PACK-119","Residue Screen - Complete + Glyphosate\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue) + Glyphosate Screens.",470,517]
[null,"SS-PACK-196","Residue Screen - Extended (Soil Only)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",200,220]
[null,"SS-PACK-208","Produce MRL - CR007 (Dithiocarbamates) \nProduce MRL - CR007 (Dithiocarbamates) \nIncludes Mancozeb(Dithane), Maneb, Metiram, Propineb, Zineb, Ferbam, Metham-sodium, Thiram, Ziram.",185,203.5]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","METAL SOLIDS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-004","Basic Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Aluminium, Arsenic, Beryllium, Boron, Cadmium, Chromium, Cobalt, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",77,84.7]
[null,"SS-PACK-188","Extra Elements related to Hair Analysis\nIncludes Caesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium and Zirconium.",190,209]
[null,"SS-PACK-043","Extra Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Antimony, Barium, Bismuth, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",77,84.7]
[null,"SS-PACK-046","Special - Metals and Salts Combo - Total Acid Extractable (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",135,148.5]
[null,"SS-PACK-045","Total Acid Extractable - Heavy Metals  (ICPMS)\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",55,60.5]
[null,"SS-PACK-153","Biochar Heavy Metals\nIncludes Pb, Cd, Hg, As, Cu, Ni, Zn and Cr.",88,96.8]
[null,"SS-PACK-161","Specific - ASLP Extractable (ICPMS) \nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride, Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-032","Specific - TCLP Extractable (ICPMS) \nIncludes Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-162","Specific - SPLP Extractable (ICPMS) \nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride, Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-069","Speciated Arsenic\nIncludes toxic arsenic species AsV and AsIII determination using HPLC-ICPMS (Total Arsenic analysis also included). ",330,363]
[null,"SS-PACK-070","Speciated Chromium\nIncludes toxic hexavalent chromium species CrVI and CrIII determination using HPLC-ICPMS (Total Chromium analysis also included).",330,363]
[null,"SS-PACK-068","Speciated Mercury\nIncludes toxic mercury species Methyl Mercury and Hg2+ determination using HPLC-ICPMS. (Total Mercury analysis also included).",330,363]
[]
[]
[null,"ITEM CODE","SOIL PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-002","Hotblock Digest\nIncludes total Aqua-Regia or Nitric Acid digestion of solid samples.",13,14.3]
[null,"SS-PREP-001","Sample Preparation\nIncludes drying and ring mill grinding.",11,12.1]
[null,"SS-PREP-005","TCLP Extractions\nToxicity Characteristic Leaching Procedure.",49,53.9]
[]
[null,null,null,null,"Sample Preparation may be required unless a Discounted Testing Suite is selected."]
[null,"ITEM CODE","INDIVIDUAL SOLIDS TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-149","Arsenic - Total\nIncludes sample preparation / acid digest and analysis by ICPMS.",33,36.299999999999997]
[null,"SS-SING-063","Asbestos Identification (Not Quantifiable)\nIdentification in building material, soil, compost and dust.",77,84.7]
[null,"SS-SING-161","Asbestos Identification and Quantification in Soil\nIdentification and quantification in soil (using AS4964-2004 or WA/NEPM) (% ACM, % Friable).",88,96.8]
[null,"SS-SING-162","Chromium VI - Hexavalent \nSpeciation by a screening colourimetric technique which may be subject to matrix interference. Refer to separate analysis codes for speciation using HPLC-ICPMS analysis.",39,42.9]
[null,"SS-SING-127","Contamination Foreign Material Fraction Percentage\nIncludes Fraction % (metal, plaster, rubber, plastic, paper, cloth, paint, wood, other vegetable matter).",44,48.4]
[null,"SS-SING-153","Cyanide - Free\n",49,53.9]
[null,"SS-SING-148","Cyanide - Total\n",66,72.599999999999994]
[null,"SS-SING-239","Cyanide (Total Prussic Acid in Plant/ Feed samples)\nIncludes sample preparation and Total Cyanide. ",110,121]
[null,"SS-SING-147","Fluoride - Total by fusion\n",77,84.7]
[null,"SS-SING-132","General Metals -  ICPMS\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SS-SING-157","Glyphosate (Round Up) + AMPA Screen (All dried solids)\n",280,308]
[null,"SS-SING-158","Herbicides Phenoxy Acid\n",220,242]
[null,"SS-SING-051","Hydrocarbons - BTEX - equivalent to TPH(C6-C10)\n",55,60.5]
[null,"SS-SING-020","Hydrocarbons - Polycyclic Aromatic (PAH)\n",71,78.099999999999994]
[null,"SS-SING-192","Hydrocarbons - Polycyclic Aromatic (PAH) by TCLP\nIncludes PAH by TCLP extraction.",130,143]
[null,"SS-SING-115","Hydrocarbons\nIncludes Hydrocarbons (C1-C5). Cost per analyte.",44,48.4]
[null,"SS-SING-023","Hydrocarbons - Total Petroleum - Speciated \nIncludes Speciated TPH (aromatic or aliphatic).",220,242]
[null,"SS-SING-052","Hydrocarbons - Total Petroleum - TPH (C10-C40)\n",55,60.5]
[null,"SS-SING-150","Lead - Total\nIncludes sample preparation, acid digest and analysis by ICPMS.",33,36.299999999999997]
[null,"SS-SING-024","Specific Metals - TCLP Extractable ICPMS\nPrice per element\nAluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Silver or  Zinc.",15,16.5]
[null,"SS-SING-133","Non-Standard Metals -  ICPMS\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SS-SING-053","Organo-chlorines (OC)  (Detection Limit - 0.1 ppm)\n",71,78.099999999999994]
[null,"SS-SING-056","Organo-chlorines (OC) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-054","Organo-phosphates (OP)  (Detection Limit - 0.1 ppm)\n",71,78.099999999999994]
[null,"SS-SING-057","Organo-phosphates (OP) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-159","Organotins (MBT, TBT, DBT)\n",285,313.5]
[null,"SS-SING-070","Paint Analysis for Lead\n",33,36.299999999999997]
[null,"SS-SING-224","PFAS in ASLP leachate – standard level 28 suite with detection to 0.01 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in ASLP (Australian Standard Leachate Procedure) leachate.\r\n",230,253]
[null,"SS-SING-216","PFAS in solid – standard level 28 suite with detection 0.01 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",190,209]
[null,"SS-SING-279","PFAS-28 Standard Level - TOF\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus any Total Organofluorine compounds.",230,253]
[null,"SS-SING-278","PFAS-28 Standard Level - TOPA\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus PFAS Precursor compounds.",360,396]
[null,"SS-SING-253","PFAS in solid – LOW level 28 suite with detection 0.0008-0.0016 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",210,231]
[null,"SS-SING-065","pH (1:5 water)\n",16,17.600000000000001]
[null,"SS-SING-142","Phenol - Total \n",66,72.599999999999994]
[null,"SS-SING-029","Phenolics - speciated phenols\n",99,108.9]
[null,"SS-SING-055","Polychlorinated Biphenyls (PCB)  (Detection Limit - 0.1 ppm)\n",71,78.099999999999994]
[null,"SS-SING-058","Polychlorinated Biphenyls (PCB) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-217","Semi-Volatile Organic Compounds (SVOC)\nSVOC includes Phenols.",285,313.5]
[null,"SS-SING-027","Silica - Total\nIncludes specialised NaOH high temperature fusion extraction of silicon.",135,148.5]
[null,"SS-SING-223","Silica Gel Clean-up TRH\nIncludes TRH C9-C40 Natural/ Petroleum differentiation – silica gel clean-up (removes all of the biogenic, more polar material leaving just the petrogenic based TRH).",120,132]
[null,"SS-SING-140","Synthetic Pyrethroids\n",135,148.5]
[null,"SS-SING-255","Fats, Oils and Grease of Solids - Hexane 1.5 hr soxlet extraction from wet weight solids\nIncludes separate moisture content for conversion of results to dry weight.",66,72.599999999999994]
[null,"SS-SING-126","Volatile Halogenated Compounds (VHC)\n",88,96.8]
[null,"SS-SING-026","Volatile Organic Compounds (VOC)\n",130,143]
[null,"SS-SING-288","PFAS Full Suite – 30 Trace Compounds (0.1 µg/kg)                                        \n",370,407]
[null,"SS-SING-289","TOPA – PFAS Full Suite – 30 Trace Compounds (0.1 µg/kg)                                  \n",435,478.5]
[null,"SS-SING-290","ASLP Leachate – PFAS Full Suite – 30 Trace Compounds (0.001-0.005 µg/L)                      \n",370,407]
[null,"SS-SING-291","TOF – Total OrganoFluorine                   \n",280,308]
[null,"SS-SING-285","Contamination Foreign Material Fraction Percentage – Modified RMS T276\nIncludes Fraction % (Rubber, plastic, bitumen, paper, cardboard, cloth, paint, glass, metal, Timber (engineered, painted, coated or treated)other vegetable matter). Includes photo per sample and each individual fraction.",150,165]
[]
[null,"WATER ASSESSMENT TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SPECIFIC WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-018","Effluent Monitoring\nIncludes pH, Total Suspended Solids (TSS); Biochemical Oxygen Demand (BOD); Total Oils and Grease (TOG); Total Nitrogen (TN), Total Phosphorus (TP); Nitrate, Nitrite, Phosphate, Ammonium; Faecal Coliforms.",210,231]
[null,"SW-PACK-058","Gas Contamination Monitoring for Dissolved Gases\nIncludes Acetylene, Butane, Ethane, Ethene, Methane and Propane.",155,170.5]
[null,"SW-PACK-056","Gas Contamination Water Quality Monitoring\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Total Alkalinity, Total Suspended Solids (TSS); Total Petroleum Hydrocarbons (TPH C10-C40), BTEX (Equivalent TPH C6-C10); Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",180,198]
[null,"SW-PACK-015","Wastewater Monitoring\nIncludes pH, Total Suspended Solids (TSS); Biochemical Oxygen Demand (BOD); Total Oils and Grease (TOG).",104,114.4]
[null,"SW-PACK-079","Water Contamination Assessment\nIncludes Metals (Total Available Al, As, Cd, Cr, Cu, Fe Pb, Mn, Hg, Ni, Se, Ag, Zn), PAH, TPH, BTEX, and speciated Phenolics.",240,264]
[null,"SW-PACK-071","Water quality for concrete mixes under AS1379 \nIncludes pH, EC, TDS (by calc), Total Suspended Solids, Total Oils and Grease, Sugars (Biological Oxygen Demand), Chloride, Sodium and Sulfate.",155,170.5]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","RESIDUE WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-072","Complete Waters Residue Screen \nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue).",240,264]
[null,"SW-PACK-009","Pesticide Screen 1a\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).",77,84.7]
[null,"SW-PACK-010","Pesticide Screen 1b\nIncludes Organo-chlorines (OC), Organo-phosphates (OP) and Polychlorinated biphenyls (PCB).",99,108.9]
[null,"SW-PACK-024","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Organo-phosphates (OP).",140,154]
[null,"SW-PACK-027","Pesticide Screen 2b - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",155,170.5]
[null,"SW-PACK-059","Pesticide Screen 3 - In Oil (Detection est. <10ppm)\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).\r\nNote: 25 mL required.",165,181.5]
[null,"SW-PACK-075","Pesticides/ Residue Screen – In Oil (Detection 0.1ppm) \nIncludes Organo-chlorines (OC), Organo-phosphates (OP) and a Multi-residue scan.\r\nNote: 25 mL required.",200,220]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","METAL WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-031","Basic Metals Scan - As Supplied (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",60,66]
[null,"SW-PACK-040","Basic Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-030","Basic Metals Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",71,78.099999999999994]
[null,"SW-PACK-029","Basic Metals Scan - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-043","Extra Metals Scan - As Supplied (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",60,66]
[null,"SW-PACK-044","Extra Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-045","Extra Metals Scan - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-046","Extra Metals Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",71,78.099999999999994]
[null,"SW-PACK-060","Saline Water Metals (Low Level) > 20 mS/cm (As Supplied) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",88,96.8]
[null,"SW-PACK-061","Saline Water Metals (Low Level) > 20 mS/cm (Dissolved) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",93,102.3]
[null,"SW-PACK-062","Saline Water Metals (Low Level) > 20 mS/cm (Total Available/Acid Soluble) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",93,102.3]
[null,"SW-PACK-063","Saline Water Metals (Low Level) > 20 mS/cm (Total Recoverable) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",99,108.9]
[null,"SW-PACK-051","Special - Metals and Salts Combo - As Supplied (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",120,132]
[null,"SW-PACK-052","Special - Metals and Salts Combo - Dissolved (filtered then acidified) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",130,143]
[null,"SW-PACK-053","Special - Metals and Salts Combo - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",130,143]
[null,"SW-PACK-054","Special - Metals and Salts Combo - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",135,148.5]
[null,"SW-PACK-067","Speciated Arsenic\nIncludes toxic arsenic species AsV and AsIII determination using HPLC-ICPMS (Total Arsenic analysis also included) 1% of volume HCl preservation in PP.",385,423.5]
[null,"SW-PACK-068","Speciated Chromium\nIncludes toxic hexavalent chromium species CrVI and CrIII determination using HPLC-ICPMS (Total Chromium analysis also included) 1M NaOH preservation (approx.. 3 Drops/30ml to adjust pH to 8-9.5) in PP.",385,423.5]
[null,"SW-PACK-066","Speciated Mercury\nIncludes toxic mercury species Methyl Mercury and Hg2+ determination using HPLC-ICPMS. (Total Mercury analysis also included) 1% of volume HCl preservation in glass jar.",385,423.5]
[null,"SW-PACK-074","Metals Screen in Oil - Total Acid Digestible (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.\r\nNote: 25 mL required to complete testing.",99,108.9]
[]
[]
[null,"ITEM CODE","WATER PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PREP-003","Filtered/Dissolved Metals\nImmediate filtration through 0.45 µm filter followed by acidification with Nitric acid. It is particularly important where waters are high in suspended clay matter, where Iron and Aluminium may be present.",5,5.5]
[null,"SW-PREP-006","Saline Waters Instrument Setup (per batch)\n",110,121]
[null,"SW-PREP-002","Total Available/Acid Soluble Metals\nAcidification with Nitric acid.  Used on nearly all environmental waters, acid sulfate waters, groundwater and surface waters (According to ANZECC guidelines).  Also used for clean waters, drinking waters, when acidified in the field and when requested.",5,5.5]
[null,"SW-PREP-001","Total Recoverable Metals\nNitric Acid digest. Used on high sludge/solid waters and when requested.",16,17.600000000000001]
[]
[null,null,null,null,"Sample Preparation may be required unless a Discounted Testing Suite is selected."]
[null,"ITEM CODE","INDIVIDUAL WATER TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-142","Absorbance (Wavelength 440nm – Filtered 0.22 micron)\n",22,24.2]
[null,"SW-SING-012","Biochemical Oxygen Demand (BOD) - Total\n",49,53.9]
[null,"SW-SING-013","Chemical Oxygen Demand (COD)\n",49,53.9]
[null,"SW-SING-030","Chromium VI - Hexavalent \nSpeciation by a screening colourimetric technique which may be subject to matrix interference. Refer to separate analysis codes for speciation using HPLC-ICPMS analysis.",39,42.9]
[null,"SW-SING-056","Conductivity - Electrical\n",11,12.1]
[null,"SW-SING-029","Cyanide - Total\n",55,60.5]
[null,"SW-SING-102","General Metals - As Supplied (external prep)\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-103","General Metals - Dissolved\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-104","General Metals - Total Available/Acid Soluble\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-105","General Metals - Total Recoverable\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-133","Non-Standard Metals -  ICPMS\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-116","Glyphosate (Round Up)\n",190,209]
[null,"SW-SING-098","Herbicides Phenoxy Acid\n",190,209]
[null,"SW-SING-062","Hydrocarbons - BTEX (Equivalent to TPH C6-C10)\n",55,60.5]
[null,"SW-SING-008","Hydrocarbons - Polycyclic Aromatic Hydrocarbons (PAH)\n",71,78.099999999999994]
[null,"SW-SING-063","Hydrocarbons - Total Petroleum (TPH C10-C40)\n",55,60.5]
[null,"SW-SING-112","Methane\n",120,132]
[null,"SW-SING-106","Non-Standard Metals - As Supplied\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-107","Non-Standard Metals - Dissolved\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-108","Non-Standard Metals - Total Available/Acid Soluble\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-109","Non-Standard Metals - Total Recoverable\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-064","Organo-chlorines (OC)\n",71,78.099999999999994]
[null,"SW-SING-113","Organo-chlorines (OC) - In Oil\nNote: 25 mL required.",135,148.5]
[null,"SW-SING-143","Chemical Oxygen Demand - Filtered (COD-F)\nFiltered GFC 1.2micron equivalent",55,60.5]
[null,"SW-SING-096","Organo-chlorines (OC) - Low Level\n",99,108.9]
[null,"SW-SING-065","Organo-phosphates (OP)\n",71,78.099999999999994]
[null,"SW-SING-114","Organo-phosphates (OP) - In Oil\nNote: 25 mL required.",135,148.5]
[null,"SW-SING-097","Organo-phosphates (OP) - Low Level \n",99,108.9]
[null,"SW-SING-117","Organotins (MBT, TBT, DBT)\n",285,313.5]
[null,"SW-SING-058","Oxygen - Dissolved (DO)\n",11,12.1]
[null,"SW-SING-121","PFAS in water – standard level 28 suite with detection 0.01 - 0.05 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in water.",165,181.5]
[null,"SW-SING-134","PFAS in water – LOW level 28 suite with detection 0.0002 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in water.",190,209]
[null,"SW-SING-055","pH\n",11,12.1]
[null,"SW-SING-038","Phenol - Total \n",66,72.599999999999994]
[null,"SW-SING-026","Phenolics - Speciated Phenols\n",99,108.9]
[null,"SW-SING-066","Polychlorinated Biphenyls (PCB)\n",71,78.099999999999994]
[null,"SW-SING-099","Polychlorinated Biphenyls (PCB) - Low Level \n",99,108.9]
[null,"SW-SING-057","Salinity\n",11,12.1]
[null,"SW-SING-111","Semi-Volatile Organic Compounds (SVOC)\nSVOC includes Phenols.",240,264]
[null,"SW-SING-141","Silica Gel Clean-up TRH\nIncludes TRH C9-C40 Natural/ Petroleum differentiation – silica gel clean-up (removes all of the biogenic, more polar material leaving just the petrogenic based TRH).",120,132]
[null,"SW-SING-122","Silica - Total\nIncludes specialised NaOH high temperature fusion extraction of silicon as per dry weight. ",165,181.5]
[null,"SW-SING-011","Total Oils and Grease (TOG) - Hexane extractable\n",55,60.5]
[null,"SW-SING-003","Total Suspended Solids (TSS)\n",22,24.2]
[null,"SW-SING-037","Trihalomethanes (THM)\n",66,72.599999999999994]
[null,"SW-SING-095","Volatile Halogenated Compounds (VHC)\n",99,108.9]
[null,"SW-SING-094","Volatile Organic Compounds (VOC)\nVOC includes BTEX.",130,143]
[]
[null,"PHYSICAL PARAMETERS ANALYTICAL SERVICES"]
[null,"PHYSICAL PARAMETER TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","PHYSICAL PARAMETER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-138","Atterberg Limits\nIncludes Liquid Limit, Plastic Limit, Plastic Index and Shrinkage Limit.\r\nNote: 1kg of sample required.",190,209]
[null,"SS-PACK-125","RUSLE Soil Erodibility Factor\nIncludes texture grading through ISSS Hydrometer and 0.1, 0.2 and 2.0 mm Sieve analysis, Organic Matter by calculation from LECO Total Organic Carbon, Emerson Dispersion Class using the Emerson Aggregate Test and determination of K Factor. \r\nClient must provide field assessment of Soil Structure and Permeability using RUSLE classes for K Factor calculation.\r\n",240,264]
[]
[null,null,null,null,"Individual tests may require sample preparation."]
[null,"ITEM CODE","PARTICLE SIZE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-194","Gravel Content\nIncludes sieving > 2 mm stones and organic material.",22,24.2]
[null,"SS-PACK-155","Biochar Particle Size Analysis - Dry Sieving\nDry sieving for fractions > 2 mm, 1-2 mm, 500 µm-1 mm, 250-500 µm, 125-250 µm, 63-125 µm, < 63 µm.",99,108.9]
[null,"SS-SING-123","Particle Size Grading under AS4454\nIncludes percentage mass retained on 5 mm and 16 mm sieve. Note: 2 kg of sample is required to complete testing.",33,36.299999999999997]
[null,"SS-SING-184","Particles Size Grading - Large particles under AS4419:2003\nIncludes percentage mass retained on 10 mm, 20 mm, 50 mm and 75 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-226","Particles Size Grading - Large particles under AS4419:2018\nIncludes percentage mass retained on 2 mm, 5 mm, 20 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-244","Particles Size Grading for Structural Support under AS4419:2018\nIncludes percentage mass passing on 63.0 mm, 53.0 mm, 37.5 mm, 26.5 mm, 19.0 mm, 13.2 mm, 4.75 mm fractions. Note: 2 kg of sample is required to complete testing.",66,72.599999999999994]
[null,"SS-SING-227","Top Dress - Particles under AS4419:2018\nIncludes percentage mass retained of organics particles on 2 mm, 5 mm, 8 mm sieve. Also mass retained of mineral particles on 2 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-243","Particle Size Analysis for Wetlands under AS4419:2018\nParticle size of sediment and soil by hydrometer and sieve. Percentage mass retained on sieve. Includes > 2 mm, 1.0–2.0 mm, 0.5–1.0 mm, 0.25–0.5 mm, 0.1–0.25 mm, 50 µm–0.1 mm, 2–50 µm, < 2 µm fractions.  Note: 500 g of sample is required to complete testing.      ",120,132]
[null,"SS-SING-254","Particle Size Analysis - Dry Sieving (FMSBS 2015)\nDry sieving for fractions >2.0 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm.",82,90.2]
[null,"SS-SING-011","Particle Size Analysis - Dry Sieving\nDry sieving for fractions > 2 mm, 1-2 mm, 500 µm-1 mm, 250-500 µm, 125-250 µm, 63-125 µm, < 63 µm.",82,90.2]
[null,"SS-SING-198","Particle Size Analysis - Wet Sieving\nWet sieving for fractions > 2 mm, 1-2 mm, 500 µm-1 mm, 250-500 µm, 125-250 µm, 63-125 µm, < 63 µm.",165,181.5]
[null,"SS-SING-012","Particle Size Analysis - ISSS Hydrometer\nParticle size of sediment and soil by hydrometer. Includes > 2 mm, > 20 µm, 20–2 mm, 2–20 µm and < 2 µm fractions.",99,108.9]
[null,"SS-PACK-126","Particle Size Analysis – ISSS Hydrometer plus 0.2 and 2.0 mm Sieving\nIncludes particle sizing of soils and sediments for ISSS classification: < 2 µm, 2–20 µm and 20 µm¬–2 mm by hydrometer; 0.2–2.0 mm and > 2 mm by sieving.\r\n",110,121]
[null,"SS-SING-236","Particle Size Analysis – ISSS and USDA Hydrometer\nParticle size of sediment and soil by hydrometer. Includes > 2 mm, > 50 µm, > 20 µm, 50 µm–2 mm, 2–50 µm, 2–20 µm and < 2 µm fractions.",130,143]
[null,"SS-SING-235","Particle Size Analysis – USDA Hydrometer\nParticle size of sediment and soil by hydrometer. Includes > 2 mm, > 50 µm, 50 µm–2 mm, 2–50 µm and < 2 µm fractions.",120,132]
[null,"SS-SING-146","Particle Size Analysis - Laser Diffraction\nParticle size analysis using a Malvern Mastersizer 3000. Span 0.01 to 3000 µm. Size classes dictated by client requirements. Includes organic and acid digestion of organic matter and shell, as required.\r\nPrice dependent upon application and sample amounts.",180,198]
[null,"SS-SING-237","Laser Diffraction – Methylated Spirits\nIncludes dry or wet sieving at 2 mm followed by digestion and dispersion as required. Particle size distribution from 2000 to 0.01 µm. Size classes dictated by clients requirements.\r\nPrice dependent upon application and sample amounts.\r\n",190,209]
[null,"FA-PACK-013","Particle Size Analysis – Laser Diffraction – Fine Fertiliser\nLaser Diffraction Particle Size Analysis including 2000 to 0.01 µm. Size fractions include < 0.01 mm, 0.01-0.02 mm, 0.02-0.03 mm, 0.03-0.04 mm, 0.04-0.05 mm, 0.05-0.06 mm, 0.06-0.07 mm, 0.07-0.08 mm, 0.08-0.09 mm, 0.09-0.1 mm, 0.1-0.125 mm, 0.125-0.25 mm, 0.25-0.5 mm, 0.5-1.0 mm, > 1.0 mm fractions.\r\nPrice dependent upon application and sample amounts.",190,209]
[null,"FA-PACK-012","Particle Size Analysis – Dry Sieving – Coarse Fertiliser\nDry sieving Particle Size Analysis including  > 1 mm, 0.85-1 mm, 0.3-0.85 mm, < 0.3 mm fractions.",55,60.5]
[null,"SS-SING-245","Vermicast Sieve Test under AS4454:2012\nIncludes percentage mass retained on 1.18 mm sieve. Note: 1 kg of sample is required to complete testing.",44,48.4]
[]
[null,null,null,null,"Individual tests may require sample preparation."]
[null,"ITEM CODE","DISPERSION AND AGGREGATION TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-167","Dispersibility under AS4419\n",44,48.4]
[null,"SS-SING-215","Dispersion Percent\nIncludes Dispersion Percent and ISSS Hydrometer particle size analysis.\r\n",120,132]
[null,"SS-SING-205","Emerson Aggregate Stability Test for Wastewater\nThis modified Emerson aggregate test (MEAT alternative) is the best option for assessment of aggregate stability for land application areas. Unlike MEAT results, the classes determined by this test can be directly related to those of the Emerson Aggregate Test.",33,36.299999999999997]
[null,"SS-SING-025","Emerson Aggregate Test (EAT)\nProvides an Emerson Dispersion Class",49,53.9]
[null,"SS-SING-085","Emerson Dispersion Index (Loveday and Pyle, 1973)\n",49,53.9]
[null,"SS-SING-015","Modified Emerson Aggregate Test (MEAT)\n",49,53.9]
[null,"SS-SING-206","R1 and R2 Dispersion Ratio\n",120,132]
[null,"SS-SING-196","Slaking and Clouding - Test Methods Q161 and Q162\n",33,36.299999999999997]
[null,"SS-SING-286","R1 Dispersion Index - additional extra option to PSA\nIncludes R1 Dispersion Index. ONLY available when selected with hydrometer particle size techniques.",52,57.2]
[]
[null,null,null,null,"Individual tests may require sample preparation."]
[null,"ITEM CODE","WATER HOLDING AND PERMEABILITY TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-021","AFP and WHC under AS3743:2003\nIncludes Air-Filled Porosity (AFP) and Water Holding Capacity (WHC). Note: 2 kg of sample is required to complete testing.",55,60.5]
[null,"SS-SING-120","Air-filled Porosity (AFP) under AS3743\nNote: 2 kg of sample is required to complete testing.",27,29.7]
[null,"SS-SING-229","Water repellence of soil under AS4419:2018\nIncludes water repellence of soil and if required, further testing to ethanol repellence of soil. Note: 200 g of sample is required to complete testing.",15,16.5]
[null,"SS-SING-156","Permeability under AS4419:2003\nNote: 2 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-230","Permeability under AS4419:2018\nThis includes 8, 16 and 32 drops. Note: 1 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-231","Saturated Hydraulic Conductivity under ASTM F1815 - 11\nNote: 1 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-013","Soil Water Retention Curve - Estimation by surrogate methods \nPurely soil materials. Not suitable for mine tailings. Includes estimation of soil hydraulic properties comprising Field Capacity, Permanent Wilting Point, Saturated Hydraulic Conductivity and van Genuchten Soil Moisture Curve parameters. Required: field soil Bulk Density or target Bulk Density, or if unknown then a simple statement of intended land use (eg. horticulture, pasture,  MEDLI etc). The method uses USDA hydrometer particle size analysis and pedotransfer software.",165,181.5]
[null,"SS-SING-207","Soil Water Retention Curve - in-situ soil cores - Ceramic Plate & Dewpoint Potentiometer\nIncludes data for three points on the Soil Water Retention Curve: wet-end soil water content at 1 kPa and 10 kPa (Field Capacity) and dry-end soil water content at Air-Dryness (100 MPa). A ceramic plate and hanging water column is used for the wet end, while the dry end is measured using a dew point potentiometer (Decagon WP4-T). Soil water content at 33 kPa (Field Capacity) and 1500 kPa (Permanent Wilting Point) can be included with selection of SS-SING-247.\r\nNote: In-situ soil cores of 30–50 mm height and no more than 75 mm diameter are required.",275,302.5]
[null,"SS-SING-210","Soil Water Content at Field Capacity and Air-dryness\nApplicable to soils supporting native vegetation. Includes soil water content at 1 kPa, 10 kPa (Field Capacity) and 100 MPa (Air-dryness). Equipment used: ceramic plate and hanging water column for the 1 kPa and 10 kPa points, and a dew point potentiometer (WP4C) for the 100 MPa point. Required: 500 g loose soil (or 1 kg inclusive of both tests when chosen in combination with SS-SING-247), and a target Bulk Density value for each sample, preferably plus a simple statement of intended land use eg. pasture, horticulture, greens,  land remediation etc.",385,423.5]
[null,"SS-SING-247","Soil Water Content at Field Capacity and Permanent Wilting Point\nIncludes soil water content at 33 kPa (Field Capacity) and 1500 kPa (Permanent Wilting Point).  Equipment used: ceramic plate and hanging water column for the 33 kPa point and dew point potentiometer (WP4C) for the 1500 kPa point. \nRequired: 500 g loose soil (or 1 kg inclusive of both tests when chosen in combination with SS-SING-210), and a target Bulk Density value for each sample, preferably plus a simple statement of intended land use eg. pasture, horticulture, greens,  land remediation etc.",155,170.5]
[null,"SS-SING-256","Soil Water Retention Curve - 6 point curve \nIncludes soil water content at 1 kPa, 3 kPa, 10 kPa (Field Capacity upper limit), 33 kPa (Field Capacity lower limit), 1500 kPa (Permanent Wilting Point) and 100 MPa (Air-dryness). Equipment used:  ceramic plate and hanging water column for 1 kPa, 3 kPa, 10 kPa and 33 kPa points, and a dew point potentiometer (WP4C) for the 1500 kPa and 100 MPa points. \nRequired: 1 kg loose soil and a target Bulk Density value for each sample, preferably plus a simple statement of intended land use eg. pasture, horticulture, greens,  land remediation etc.",180,198]
[null,"SS-SING-121","Water Holding Capacity (WHC) under AS3743\nNote: 2 kg of sample is required to complete testing.",27,29.7]
[null,"SS-SING-275","Water Holding Capacity under AS4419:2018\nNote: 500g of sample is required to complete testing.",27,29.7]
[null,"SS-SING-197","Water repellence of soil - Test Method Q160\n",16,17.600000000000001]
[null,"SS-SING-182","Wettability under AS4419\n\r\n",22,24.2]
[null,"SS-SING-072","Wettability under AS4454/AS3743\n",22,24.2]
[]
[]
[null,"ITEM CODE","MOISTURE CONTENT TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-221","Air Dry Moisture Content - ADMC (%) at 105°C.\nMoisture content of an air-dry (40°C) sample, further dried to 105°C (oven-dry equivalent).",11,12.1]
[null,"SS-SING-225","Dry Matter Content (%) at 105°C\nProportion of moisture and oven-dry solid in ‘as received’ sample (105°C). ",11,12.1]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-SING-233","Moisture Content - As Received (%) at 40°C \nMoisture content as a per cent of air-dry equivalent soil (40°C).",11,12.1]
[null,"SS-SING-222","Moisture Content - As Received (%) Gravimetric at 105°C\nSoil moisture as a per cent of dry mass at 105°C (oven-dry equivalent).",11,12.1]
[null,"SS-PREP-007","Total Dry Weight - Air dry basis\nMass of the sample dried at 40°C.\r\n",6,6.6]
[null,"SS-PREP-017","Total Dry Weight - Oven dry basis\nMass of the sample dried at 105°C. Used to calculate bulk density when cores are supplied.",11,12.1]
[]
[]
[null,"ITEM CODE","BULK DENSITY TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-021","Bulk Density - Lab Based\nBulk Density – Lab based compacting of a supplied loose soil/sediment to a set volume, to simulate equivalent field conditions – note for the most accurate method use field bulk density rings of known volume with SS-PREP-017 for total oven dry weight.  ",11,12.1]
[null,"SS-SING-183","Bulk Density under AS4419\nLab based bulk density on landscape soils. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-139","Bulk Density under AS4454/AS3743\nLab based bulk density on compost and potting mix. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-274","Bulk Density under AS4419:2018 \nThis includes 8, 16 and 32 drops. Note 1kg of sample is required to complete testing.",66,72.599999999999994]
[]
[]
[null,"ITEM CODE","COLOUR AND TEXTURE\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-218","Colour (Munsell Soil Colour Classification)  \n",8,8.8000000000000007]
[null,"SS-SING-086","Texture – Full under AS 1547:2012",27,29.7]
[null,"SS-SING-164","Texture - Full under AS4419\n",27,29.7]
[null,"SS-SING-208","Texture - Full (NCST, 2009)\nThis method is used for acid sulfate soil action criteria.",27,29.7]
[]
[null,null,null,null,"Individual tests may require sample preparation."]
[null,"ITEM CODE","PHYSICAL CONTAMINANTS TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-127","Contamination Foreign Material Fraction Percentage\nIncludes Fraction % (metal, plaster, rubber, plastic, paper, cloth, paint, wood, other vegetable matter).",44,48.4]
[null,"SS-SING-228","Physical Contaminants under AS4419:2018\nApplies to soil types as identified by AS4419:2018. Includes contamination with glass, metal, rigid plastics, light flexible film plastics. Note: 2 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-245","Vermicast Sieve Test under AS4454:2012\nIncludes percentage mass retained on 1.18 mm sieve. Note: 1 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-122","Visible Contaminants under AS4454\nApplies to composts from agricultural or source separated organics. Includes contamination with glass, metal, rigid plastics, stones, lumps of clay, light flexible film plastics. Note: 2 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-285","Contamination Foreign Material Fraction Percentage – Modified RMS T276\nIncludes Fraction % (Rubber, plastic, bitumen, paper, cardboard, cloth, paint, glass, metal, Timber (engineered, painted, coated or treated)other vegetable matter). Includes photo per sample and each individual fraction.",150,165]
[]
[null,"OTHER SOLID ANALYTICAL SERVICES"]
[null,"GENERAL SOLIDS TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SOLIDS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-015","Aggressivity Assessment\nIncludes Moisture, Basic Texture; pH, EC, Resistivity (calculation), Soluble Chloride, Sulfate.",77,84.7]
[null,"SS-PACK-163","Biochar Totals Analysis Plus \nIncludes Moisture Content, Bulk Density; Ash Content and Loss on Ignition (750°C); pH, EC (1:10 water); Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC); Hydrogen, Oxygen Calc., H/Corg and O/Corg Calc; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Acid Neutralising Capacity (ANC). Note: 500 g of sample is required to complete testing.",470,517]
[null,"SS-PACK-053","Concrete Quality Analysis\nIncludes concrete crushing, Chloride and Sulfate.",88,96.8]
[null,"SS-PACK-034","Micronutrients - 12A1 - DTPA Extractable \nIncludes Iron, Copper, Zinc, Manganese.",44,48.4]
[null,"SS-PACK-073","Incubation - Slab\nThis method is used to assess the effectiveness of a soil's Acid Neutralising Capacity (ANC). The incubation is maintained and pH-INC taken fortnightly until the soil pH changes by at least 0.5 pH unit to below 4, or for at least 8 weeks until pH-INC is stable.",200,220]
[null,"SS-PACK-088","LECO - Total Carbon and Total Sulfur\nIncludes Total Carbon (TC) and Total Sulfur (TS) (LECO SC832).",38,41.8]
[null,"SS-PACK-022","Excavated Natural Material (ENM) Classification 2012  (replaced by SS-PACK-051)\nIncludes pH, EC (water 1:5); Foreign Material; Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury; Polycyclic Aromatic Hydrocarbons (PAH); Total Petroleum Hydrocarbons (C10-C36), BTEX (C6-C9), Volatile Halogen Compounds (VHC).",330,363]
[null,"SS-PACK-019","Nutrients - KCl Extractable\nIncludes Nitrate, Ammonium, Phosphate.",55,60.5]
[null,"SS-PACK-033","Nutrients - Water Extractable\nIncludes Nitrate, Phosphate, Ammonium.",55,60.5]
[null,"SS-PACK-036","Mehlich III  Exchangeable Cations\nIncludes Mehlich III Extractable Sodium, Potassium, Calcium, Magnesium, Phosphorus.",44,48.4]
[null,"SS-PACK-037","Mehlich III Exchangeable Cations and Micronutrients\nIncludes Mehlich III Extractable Sodium, Potassium, Calcium, Magnesium, Phosphorus, Sulfur, Aluminium, Iron, Copper, Zinc, Manganese, Boron.",66,72.599999999999994]
[null,"SS-PACK-141","Microbial Biomass Assessment - Compost \nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-140","Microbial Biomass Assessment - Soil\nIncludes biomasses of 12 microbial groups relevant for soil quality, health and function. ",285,313.5]
[null,"SS-PACK-038","Micronutrients - 12C2 - Hot 0.01M CaCl2 Extractable\nIncludes Plant available Boron, Silica.",33,36.299999999999997]
[null,"SS-PACK-039","Morgan Soluble Salt Extract\nIncludes Calcium, Magnesium, Potassium, Phosphorus.",44,48.4]
[null,"SS-PACK-010","pH and EC\nIncludes soil pH and EC (1:5 water).",27,29.7]
[null,"SS-PACK-003","Septic Disposal Soil Assessment\nIncludes moisture, pH(CaCl2), EC, Total Dissolved Salts (TDS) (calculation); Exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium, Hydrogen, Exchangeable Sodium Percentage, Cation Exchange Capacity; Phosphorus Sorption Capacity; Emerson Aggregate Stability Test for Wastewater.",180,198]
[null,"SS-PACK-143","Soil Testing for Biochar Application\nIncludes Moisture, pH, EC (1:5 water); Total Organic Carbon (TOC), Total Nitrogen (TN), TC/TN Ratio; Available Nitrogen (Nitrate); Soluble Chloride; Total Metals (Sb, As, Be, B, Cd, Co, Cu, Cr, Pb, Mn, Mo, Ni, Se, Sn, V, Zn, S, P, Hg); Soluble Cations (Ca, Mg, K, Na). Note: 300 g of sample is required to complete testing.",225,247.5]
[null,"SS-PACK-035","SOUR Test\nIncludes Moisture, Volatile Solids Concentration,  Specific Oxygen Uptake Rate (SOUR) with an incubation of 20oC.",110,121]
[null,"SS-PACK-164","Sulfate to Chloride Ratio\nIncludes Sulfate and Chloride (1:5 water) and Sulfate/Chloride Ratio.\r\n",55,60.5]
[null,"SS-PACK-110","Total NPK Analysis\nIncludes Total Nitrogen, Total Phosphorus, Total Potassium.",66,72.599999999999994]
[null,"SS-PACK-203","Solids Leachable SAR Analysis\nIncludes Sodium Absorption Ratio (SAR) of Solids (1:10 water leach of solid material and analysis of dissolved salts (Na, Ca, Mg)).",50,55]
[]
[null,null,null,null,"SS-PREP-010"]
[null,"ITEM CODE","SOLIDS PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-024","Ash Analysis Preparation\nIncludes moisture (105°C) and ash content(550°C) whereby ash is analysed.",33,36.299999999999997]
[null,"SS-PREP-021","Bulk Density - Lab Based\nBulk Density – Lab based compacting of a supplied loose soil/sediment to a set volume, to simulate equivalent field conditions – note for the most accurate method use field bulk density rings of known volume with SS-PREP-017 for total oven dry weight.  ",11,12.1]
[null,"SS-PREP-015","Exchangeable Cation Pre-treatment for Soluble Salts\nIncludes pre-treatment with aqueous ethanol and aqueous glycerol to remove soluble salts. Recommended on soils with EC > 0.3 dS/m.",11,12.1]
[null,"SS-PREP-020","Exchangeable Cation Suppression of Carbonates \nIncludes pre-treatment with aqueous ethanol and aqueous glycerol to remove soluble salts then extraction with 1M Alcoholic NH4Cl to suppress solid phase carbonates. Testing according to Method 15C1 with other agricultural tests.",44,48.4]
[null,"SS-PREP-014","Fertiliser Handling Charge\n",55,60.5]
[null,"SS-PREP-016","Fizz Test for Carbonates \nThis method is used to indicate the presence of carbonates.",3,3.3]
[null,"SS-PREP-027","Freeze Drying of solid samples (ie. marine organisms, flesh)\nUsed for tissue or marine samples not suitable for oven drying.",26,28.6]
[null,"SS-PREP-002","Hotblock Digest\nIncludes total Aqua-Regia or Nitric Acid digestion of solid samples.",13,14.3]
[null,"SS-PREP-013","Biosecurity Handling Charge\n",110,121]
[null,"SS-PREP-003","Leaching\nIncludes 1:10 solid/water leaching with filtration.",8,8.8000000000000007]
[null,"SS-PREP-009","Leaf Washing\nPlease advise with samples.",11,12.1]
[null,"SS-PREP-025","Medicinal Cannabis and Hemp Handling Fee\n",84,92.4]
[null,"SS-PREP-008","Microwave Digest\n",22,24.2]
[null,"SS-PREP-028","Pore Water Extraction of sediment sample\n(ie. centrifuge of 50ml subsamples of sediment to extract available pore water or alternative backup option of water added and extracted)",22,24.2]
[null,"SS-PREP-019","Repacking to Target Bulk Density\n",115,126.5]
[null,"SS-PREP-004","Sample Compositing\nIncludes sample compositing and storage of individual samples for at least 2 months to allow for individual testing if required. Charge per individual sample used in the composite.",4,4.4000000000000004]
[null,"SS-PREP-023","Sample Compositing for Soil Carbon Subsoils (30-100cm)\nIncludes compositing charge for composite subsoil samples tested under 2018 CFI methodology.",38,41.8]
[null,"SS-PREP-022","Sample Compositing for Soil Carbon Topsoils (0-30cm)\nIncludes compositing charge for composite topsoil samples tested under 2018 CFI methodology.",16,17.600000000000001]
[null,"SS-PREP-001","Sample Preparation\nIncludes drying and ring mill grinding.",11,12.1]
[null,"SS-PREP-026","Sample Preparation - Crushing/grinding only \nIncludes crushing/grinding when samples are supplied already dried.",6,6.6]
[null,"SS-PREP-012","Sample Storage of Fresh Samples\nIncludes sample storage of supplied samples (1st month storage is free) for up to 12 months at $10.00 per month.",11,12.1]
[null,"SS-PREP-018","Saturated Paste Extract\nIncludes extraction of saturated paste (14A3). Please select required analytical parameters from the waters codes.",77,84.7]
[null,"SS-PREP-005","TCLP Extractions\nToxicity Characteristic Leaching Procedure.",49,53.9]
[null,"SS-PREP-007","Total Dry Weight - Air dry basis\nMass of the sample dried at 40°C.\r\n",6,6.6]
[null,"SS-PREP-017","Total Dry Weight - Oven dry basis\nMass of the sample dried at 105°C. Used to calculate bulk density when cores are supplied.",11,12.1]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL SOLIDS TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-090","Acid Neutralising Capacity (ANC-BT)\nThis method is used to measure Acid Neutralising Capacity (ANC-BT) where pH-KCl > 6.5.",33,36.299999999999997]
[null,"SS-SING-201","Acid Neutralising Capacity by Total Inorganic Carbon (C-IN)\nThis method is used to measure Acid Neutralising Capacity (ANC) where the pH-KCl > 6.5.\r\n\r\n",49,53.9]
[null,"SS-SING-251","Aluminium - 1 M KCl\nIncludes exchangeable aluminium by 1 M KCl.",22,24.2]
[null,"SS-SING-149","Arsenic - Total\nIncludes sample preparation / acid digest and analysis by ICPMS.",33,36.299999999999997]
[null,"SS-SING-063","Asbestos Identification (Not Quantifiable)\nIdentification in building material, soil, compost and dust.",77,84.7]
[null,"SS-SING-161","Asbestos Identification and Quantification in Soil\nIdentification and quantification in soil (using AS4964-2004 or WA/NEPM) (% ACM, % Friable).",88,96.8]
[null,"SS-SING-021","Ash Content by Combustion\nIncludes moisture content and ash content by combustion.",33,36.299999999999997]
[null,"SS-SING-155","Ash Content by Combustion - Routine and Acid Insoluble\nIncludes standard Ash content by combustion then treatment of filter with hydrochloric acid and re-ashing.",38,41.8]
[null,"SS-SING-134","Boron - 12C2 - Hot 0.01M CaCl2 Extractable",27,29.7]
[null,"SS-SING-160","Brix Reading\n",11,12.1]
[null,"SS-SING-038","Chloride - Water Extractable",33,36.299999999999997]
[null,"SS-SING-153","Cyanide - Free\n",49,53.9]
[null,"SS-SING-148","Cyanide - Total\n",66,72.599999999999994]
[null,"SS-SING-225","Dry Matter Content (%) at 105°C\nProportion of moisture and oven-dry solid in ‘as received’ sample (105°C). ",11,12.1]
[null,"SS-SING-064","Electrical Conductivity (1:5 water)\n",16,17.600000000000001]
[null,"SS-SING-273","Extractable Sulfate Sulfur (10% HCl extractable)\nIncludes extraction of soil using 10% HCl following method BS1377 and analysis by ICPOES.",26,28.6]
[null,"SS-SING-067","Fluoride - Water Extractable",66,72.599999999999994]
[null,"SS-SING-147","Fluoride - Total by fusion\n",77,84.7]
[null,"SS-SING-022","Iodine - NaOH Extraction\n",110,121]
[null,"SS-SING-150","Lead - Total\nIncludes sample preparation, acid digest and analysis by ICPMS.",33,36.299999999999997]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-SING-233","Moisture Content - As Received (%) at 40°C \nMoisture content as a per cent of air-dry equivalent soil (40°C).",11,12.1]
[null,"SS-SING-068","Neutralising Value\nIncludes Acid Neutralising Capacity -  Carbonate.",33,36.299999999999997]
[null,"SS-SING-138","Organic Matter \nIncludes Total Organic Carbon and organic matter by calculation.",33,36.299999999999997]
[null,"SS-SING-070","Paint Analysis for Lead\n",33,36.299999999999997]
[null,"SS-SING-069","Paramagnetism\n",11,12.1]
[null,"SS-SING-216","PFAS in solid – standard level 28 suite with detection 0.01 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",190,209]
[null,"SS-SING-279","PFAS-28 Standard Level - TOF\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus any Total Organofluorine compounds.",230,253]
[null,"SS-SING-278","PFAS-28 Standard Level - TOPA\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus PFAS Precursor compounds.",360,396]
[null,"SS-SING-253","PFAS in solid – LOW level 28 suite with detection 0.0008-0.0016 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",210,231]
[null,"SS-SING-084","Phosphorus Buffer Index (PBI) - Colwell corrected\nIncludes Phosphorus Buffer Index (PBI) and is corrected using Colwell Phosphorus.",44,48.4]
[null,"SS-SING-083","Potassium - 18C1 - BSES 1M HNO3",33,36.299999999999997]
[null,"SS-SING-076","Potassium - Colwell \n",27,29.7]
[null,"SS-SING-136","Protein (Crude)\nIncludes Total Nitrogen (TN) and Crude Protein (Calculation).",33,36.299999999999997]
[null,"SS-SING-131","Redox Potential\nTested on 'as supplied' sample.",33,36.299999999999997]
[null,"SS-SING-028","Scanning Electron Microscopy (SEM) - Sample Feasibility Assessment\nIncludes sample preparation and instrument setup. A quote for analysis is provided following Sample Feasibility Assessment.",400,440]
[null,"SS-PACK-047","Salts – Water Soluble\nIncludes water soluble Sodium, Calcium, Magnesium, Potassium. ",38,41.8]
[null,"SS-SING-199","Scanning Electron Microscopy (SEM) - Imaging and X-ray analysis\nImaging, X-ray analysis or both. Price is sample dependent; a quote can be provided following SEM Sample Feasibility Assessment (SS-SING-028).",310,341]
[null,"SS-SING-080","Silicon - 13D1 - BSES 0.005M H2SO4",22,24.2]
[null,"SS-SING-078","Silicon - 0.01M CaCl2 Extractable",22,24.2]
[null,"SS-SING-135","Silicon - 12C2 - Hot 0.01M CaCl2 Extractable",27,29.7]
[null,"SS-SING-081","Sulfur - KCl-40 \n",22,24.2]
[null,"SS-SING-082","Sulfur - MCP\n",22,24.2]
[null,"SS-SING-124","Sulfur - Morgan Soluble Extract",22,24.2]
[null,"SS-SING-144","Total Sulfur (TS) by LECO\n",22,24.2]
[null,"SS-SING-010","X-ray Diffraction (XRD) Identification - excluding clay minerals\nIncludes identification of minerals and mineral assemblages.  Price dependent upon application and sample amounts. Price does NOT include clay identification.",165,181.5]
[null,"SS-SING-200","X-ray Diffraction (XRD) Identification of Clay Minerals\nIncludes preparation and identification of clay minerals. All other minerals are removed during sample preparation. Price dependent upon application and sample amounts.",610,671]
[null,"SS-SING-031","X-ray Fluorescence (XRF) \nIncludes total elemental concentration of elements with atomic weight greater than Oxygen. Price dependent upon application and sample amounts. Price includes Total Carbon (TC) and Total Nitrogen (TN).",200,220]
[null,"SS-SING-079","Zinc - BSES HCl\n",22,24.2]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIOSOLID SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"BS-PACK-001","Contaminated Grade Assessment\nIncludes Total Dry Solids Concentration, Metals Analysis Arsenic, Cadmium, Chromium, Copper, Lead, Mercury, Nickel, Selenium, Zinc; Low Level (Organo-chlorines Pesticides (OC), Polychlorinated biphenyls (PCB)).",250,275]
[null,"BS-PACK-004","Enteric Viruses Determination\nIncludes Reovirus, Enterovirus, Adenovirus (viruses per 10 g).",460,506]
[null,"BS-PACK-006","Enteric Viruses Determination plus Helminth Ova\nIncludes Reovirus, Enterovirus, Adenovirus (viruses per 10 g) plus Helminth Ova.",550,605]
[null,"BS-PACK-002","Nutrient Determination\nIncludes Moisture Content; Total Nitrogen (TN), Total Phosphorus, Total Kjeldahl Nitrogen (TKN) (by calculation); and available Nutrients (1:10 KCL extractable Nitrate, Ammonium).",99,108.9]
[null,"BS-PACK-005","SOUR Test\nIncludes Moisture, Volatile Solids Concentration, Specific Oxygen Uptake Rate (SOUR) with an incubation of 20oC.",110,121]
[null,"BS-PACK-003","Stabilisation Confirmation\nIncludes Moisture, Microbial Assessment (E.Coli, Faecal Coliforms, and Salmonella sp.), Volatile Solids Concentration, Specific Oxygen Uptake Rate (SOUR).",220,242]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","CARBON SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-020","Carbon Stability\nIncludes Total Carbon (TC), Labile Carbon.",55,60.5]
[null,"SS-PACK-011","LECO - Total Carbon and Total Nitrogen\nIncludes Total Carbon (TC) and Total Nitrogen (TN), TC/TN Ratio.",33,36.299999999999997]
[null,"SS-PACK-088","LECO - Total Carbon and Total Sulfur\nIncludes Total Carbon (TC) and Total Sulfur (TS) (LECO SC832).",38,41.8]
[null,"SS-PACK-012","LECO - Total Carbon, Total Nitrogen and Total Sulfur\nIncludes Total Carbon (TC) and Total Nitrogen (TN), Total Sulfur (TS), TC/TN Ratio.",49,53.9]
[null,"SS-PACK-174","Inorganic (Carbonate) Carbon by LECO\nIncludes Total Carbon (TC), Total Organic Carbon (TOC).",60,66]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL CARBON TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-018","Carbon - Labile - Blair 0.333M KMnO4\n",22,24.2]
[null,"SS-SING-062","Carbon - Organic by Walkley Black\n",44,48.4]
[null,"SS-SING-061","Carbon - Total Organic by LECO\n",33,36.299999999999997]
[null,"SS-SING-059","Inorganic (Carbonate) Carbon by LECO\nIncludes Total Carbon (TC), Total Organic Carbon (TOC).",49,53.9]
[null,"SS-SING-060","Total Carbon by LECO\n",22,24.2]
[null,"SS-SING-138","Organic Matter \nIncludes Total Organic Carbon and organic matter by calculation.",33,36.299999999999997]
[]
[null,"EXCHANGEABLE CATIONS TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","EXCHANGEABLE CATIONS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-073","Incubation - Slab\nThis method is used to assess the effectiveness of a soil's Acid Neutralising Capacity (ANC). The incubation is maintained and pH-INC taken fortnightly until the soil pH changes by at least 0.5 pH unit to below 4, or for at least 8 weeks until pH-INC is stable.",200,220]
[null,"SS-PACK-028","Exchangeable Acidity - 15G1 - 1 M KCl\nIncludes exchangeable acidity (Hydrogen + Aluminium) by 1 M KCl.\r\n\r\n",33,36.299999999999997]
[null,"SS-PACK-074","Exchangeable Cations - 15A1 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. No pre-treatment for soluble salts.\r\n\r\n\r\n",44,48.4]
[null,"SS-PACK-075","Exchangeable Cations - 15A2 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-029","Exchangeable Cations - 15A3 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium. \r\n\r\n\r\n",60,66]
[null,"SS-PACK-076","Exchangeable Cations - 15B1 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. No pre-treatment for soluble salts.\r\n\r\n\r\n\r\n\r\n",44,48.4]
[null,"SS-PACK-077","Exchangeable Cations - 15B2 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-078","Exchangeable Cations - 15B3 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium.\r\n\r\n\r\n\r\n\r\n\r\n",60,66]
[null,"SS-PACK-027","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.\r\n\r\n\r\n ",77,84.7]
[null,"SS-PACK-026","Exchangeable Cations - 15D1 - 1 M NH4OAc\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-041","Exchangeable Cations - 15D3 - 1 M NH4OAc\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0. No pre-treatment for soluble salts.\r\n\r\n\r\n",44,48.4]
[null,"SS-PACK-001","Exchangeable Cations - 15D3 - 1 M NH4OAc plus Acidity (15G1)\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0 and exchangeable acidity (Hydrogen + Aluminium) by 1 M KCl.\r\n\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-205","Exchangeable Cations - 15D1 - 1 M NH4OAc plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.",74,81.400000000000006]
[null,"SS-PACK-206","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl  plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.",95,104.5]
[null,"SS-PACK-207","Exchangeable Cations - 15B3 - 1 M NH4Cl plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium.",74,81.400000000000006]
[]
[null,"METALS TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","METALS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-004","Basic Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Aluminium, Arsenic, Beryllium, Boron, Cadmium, Chromium, Cobalt, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",77,84.7]
[null,"SS-PACK-043","Extra Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Antimony, Barium, Bismuth, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",77,84.7]
[null,"SS-PACK-050","Hair Tissue Mineral Analysis (HTMA) - Human and Animal\nIncludes Antimony, Aluminium, Arsenic, Barium, Beryllium, Bismuth, Boron, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium and Zinc.\r\nData only (no interpretation), Nitric Acid digest, minimum of 0.5 g of hair required which is equivalent to one heaped tablespoon. Collect from nape as close as possible to scalp as this reflects new growth.  Provide sample double bagged to avoid contamination when opened at the laboratory.",88,96.8]
[null,"SS-PACK-044","Salts Scan - Total Acid Extractable (ICPMS)\nIncludes Calcium, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",49,53.9]
[null,"SS-PACK-046","Special - Metals and Salts Combo - Total Acid Extractable (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",135,148.5]
[null,"SS-PACK-069","Speciated Arsenic\nIncludes toxic arsenic species AsV and AsIII determination using HPLC-ICPMS (Total Arsenic analysis also included). ",330,363]
[null,"SS-PACK-070","Speciated Chromium\nIncludes toxic hexavalent chromium species CrVI and CrIII determination using HPLC-ICPMS (Total Chromium analysis also included).",330,363]
[null,"SS-PACK-068","Speciated Mercury\nIncludes toxic mercury species Methyl Mercury and Hg2+ determination using HPLC-ICPMS. (Total Mercury analysis also included).",330,363]
[null,"SS-PACK-031","Specific - Rare Earth - Total Acid Extractable (ICPMS) \nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",104,114.4]
[null,"SS-PACK-161","Specific - ASLP Extractable (ICPMS) \nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride, Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-032","Specific - TCLP Extractable (ICPMS) \nIncludes Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-162","Specific - SPLP Extractable (ICPMS) \nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride, Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-053","Concrete Quality Analysis\nIncludes concrete crushing, Chloride and Sulfate.",88,96.8]
[null,"SS-PACK-045","Total Acid Extractable - Heavy Metals  (ICPMS)\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",55,60.5]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL METALS TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-132","General Metals -  ICPMS\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SS-SING-133","Non-Standard Metals -  ICPMS\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SS-SING-024","Specific Metals - TCLP Extractable ICPMS\nPrice per element\nAluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Silver or  Zinc.",15,16.5]
[]
[null,"MICROBIAL AND NITROGEN TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","MICROBIAL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-185","Cryptosporidium and Giardia \nNote: 500 g of sample is required to complete testing.",940,1034]
[null,"SS-PACK-192","Food Microbiology (ie. Macadamia kernel)\nIncludes E.Coli, Total Coliforms, Salmonella and Total Plate Count.",115,126.5]
[null,"SS-PACK-176","General Plant Pathogen Scan\nNote: 500 g of sample is required to complete testing.",385,423.5]
[null,"SS-PACK-184","General Plant Pathogen Scan Plus\nGeneral plant pathogen scan including Phytophthora, Pythium, Rhizoctonia and Fusarium.\r\n\r\nNote: 500 g of sample is required to complete testing.",550,605]
[null,"SS-PACK-141","Microbial Biomass Assessment - Compost \nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-166","Microbial Biomass Assessment - Soil with high Organics\nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-140","Microbial Biomass Assessment - Soil\nIncludes biomasses of 12 microbial groups relevant for soil quality, health and function. ",285,313.5]
[null,"SS-PACK-167","MIC-01: Basic Analysis of Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Total fungi (moulds), Gram negative bacteria, Filamentous actinomycetes, Yeasts. ",99,108.9]
[null,"SS-PACK-168","MIC-02: Extended Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Filamentous actinomycetes, Actinobacteria, Gram negative bacteria, Filamentous fungi (Moulds), Yeasts, Lactic acid bacteria, Total Anaerobes (includes facultative anaerobes), Sulfite Reducing Anaerobes.",210,231]
[null,"SS-PACK-059","Pathogens\nIncludes Moisture, Ecoli, Faecal Coliforms, Salmonella.",155,170.5]
[null,"SS-PACK-175","Phytophthora and Pythium\nNote: 500 g of sample is required to complete testing.",165,181.50000000000003]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL MICROBIAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-047","Aerobic Plate Count\n",44,48.4]
[null,"SS-SING-265","Bacillus cereus\n",135,148.5]
[null,"SS-SING-044","E.Coli\n",44,48.4]
[null,"SS-SING-266","Clostridium perfringens\n",82,90.2]
[null,"SS-SING-267","Campylobacter\n",165,181.5]
[null,"SS-SING-043","Faecal Coliforms\n",44,48.4]
[null,"SS-SING-203","Helminth Ova\n",285,313.5]
[null,"SS-SING-046","Listeria\n",66,72.599999999999994]
[null,"SS-SING-269","Nematodes\n",110,121]
[null,"SS-SING-045","Salmonella\n",66,72.599999999999994]
[null,"SS-SING-195","SOLVITA - Compost Emissions Maturity Test\nIncludes measurement of carbon dioxide and ammonia gas released from compost due to biological activity.",66,72.599999999999994]
[null,"SS-SING-209","SOLVITA - Soil CO2 Burst\nIncludes measurement of carbon dioxide released from soil due to biological activity.",66,72.599999999999994]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","NITROGEN SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-019","Nutrients - KCl Extractable\nIncludes Nitrate, Ammonium, Phosphate.",55,60.5]
[null,"SS-PACK-033","Nutrients - Water Extractable\nIncludes Nitrate, Phosphate, Ammonium.",55,60.5]
[null,"SS-PACK-204","Nitrogen - Water Extractable\nIncludes Nitrate, Nitrite, Ammonium.",55,60.5]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL NITROGEN TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-048","Ammonium - Water Extractable",33,36.299999999999997]
[null,"SS-SING-049","Nitrate - Water Extractable\n",33,36.299999999999997]
[null,"SS-SING-050","Total Nitrogen by LECO\n",22,24.2]
[]
[null,"PHOSPHORUS TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","PHOSPHORUS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-019","Nutrients - KCl Extractable\nIncludes Nitrate, Ammonium, Phosphate.",55,60.5]
[null,"SS-PACK-033","Nutrients - Water Extractable\nIncludes Nitrate, Phosphate, Ammonium.",55,60.5]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL PHOSPHORUS TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-191","MEDLI Adsorption Isotherm Parameters\nModelling (6 concentrations of Phosphorus), Colwell Phosphorus. ",110,121]
[null,"SS-SING-042","Phosphorus - Available by 1M KCl extract\n",22,24.2]
[null,"SS-SING-041","Phosphorus - Morgan Soluble Extract",22,24.2]
[null,"SS-SING-035","Phosphorus - Bray 1 \nIncludes plant available Phosphorous for acid soils.",22,24.2]
[null,"SS-SING-036","Phosphorus - Bray 2\nIncludes plant available and acid soluble forms of Phosphorous.",22,24.2]
[null,"SS-SING-040","Phosphorus - 9G2 - BSES 0.005M H2SO4",22,24.2]
[null,"SS-SING-248","Phosphorus - Citrate Soluble \nIncludes 2% Citrate Soluble Phosphorus.",44,48.4]
[null,"SS-SING-033","Phosphorus - Colwell\nIncludes Phosphorus for alkaline soils.",22,24.2]
[null,"SS-SING-264","Phosphorus – Formic Acid Soluble\nIncludes Formic Acid Soluble Phosphorus.",66,72.599999999999994]
[null,"SS-SING-034","Phosphorus - Olsen\nIncludes Olsen Phosphorous - a measure of the intensity of Phosphorus.",22,24.2]
[null,"SS-SING-032","Phosphorus - Total Acid Extractable (includes preparation)\n",44,48.4]
[null,"SS-SING-037","Phosphorus Buffer Index (PBI)\n",22,24.2]
[null,"SS-SING-084","Phosphorus Buffer Index (PBI) - Colwell corrected\nIncludes Phosphorus Buffer Index (PBI) and is corrected using Colwell Phosphorus.",44,48.4]
[null,"SS-SING-087","Phosphorus Sorption - 40ppm (as mg P/kg)",27,29.7]
[null,"SS-SING-039","Phosphorus Sorption Capacity\nIncludes 1 day preliminary trial, 7 day sorption capacity trial (Ryden and Pratt, 1980), In situ Phosphorous and calculations. ",88,96.8]
[null,"SS-SING-249","Phosphorus - Water Soluble \nIncludes Water Soluble Phosphorus.",22,24.2]
[]
[null,"STABLE ISOTOPES TESTING"]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL STABLE ISOTOPE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-118","Biomarker and Specific Compounds - 13C and / or 15N Isotopes\nPrice dependent upon application and sample amounts.",0,0]
[null,"SS-SING-116","Carbonate Analysis - 'as supplied' - 13C & 18O Isotopes\nWithout pre-concentration.",66,72.599999999999994]
[null,"SS-SING-257","Carbonate Analysis - 13C and 18O Isotopes\nNo pre-concentration, sample preparation included.",155,170.5]
[null,"SS-SING-114","Dissolved Gas Analysis\nIncludes N2/Ar non-isotope ratio measurement.",44,48.4]
[null,"SS-SING-109","Dissolved inorganic carbon in water - 13C isotopes\n",68,74.8]
[null,"SS-SING-112","Dissolved Nitrogen\nIncludes Dissolved N2 - ratio masses 29/28 and 30/28.",82,90.2]
[null,"SS-SING-113","Dissolved Nitrous Oxide\n",140,154]
[null,"SS-SING-110","Dissolved organic carbon in water - 13C isotopes \n",89,97.9]
[null,"SS-SING-260","Hydrogen and Oxygen in Bulk Solids - 2H and 18O Isotopes\nIncludes % H and % O - consult for sample suitability.",135,148.5]
[null,"SS-SING-261","Hydrogen and Oxygen Content in Bulk Solids - No Isotopes\n",66,72.599999999999994]
[null,"SS-SING-258","Hydrogen in Bulk Solids - 2H Isotopes\nIncludes % H - consult for sample suitability.",66,72.599999999999994]
[null,"SS-SING-242","Organic Carbon in Bulk Solids - 13C Isotopes\nIncludes acid treatment to remove inorganic carbon. % C also provided.",77,84.7]
[null,"SS-SING-117","Nitrogen Gas\nWithout pre-concentration.",49,53.9]
[null,"SS-SING-259","Oxygen in Bulk Solids - 18O Isotopes\nIncludes % O - consult for sample suitability.",66,72.599999999999994]
[null,"SS-SING-108","Total Carbon and Total Nitrogen in Filters - 13C and 15N Isotopes\nFilters (25 mm or smaller GFF quartz preferred) (charge per analyte, sample preparation included).",99,108.9]
[null,"SS-SING-106","Total Carbon in filters - 13C isotopes \n",99,108.9]
[null,"SS-SING-105","Total Carbon and Total Nitrogen in Bulk Solids - 13C and 15N Isotopes\nAlso includes % TC and % TN. ",77,84.7]
[null,"SS-SING-103","Total Carbon in Bulk Solids - 13C Isotopes\nAlso includes % TC.",66,72.599999999999994]
[null,"SS-SING-104","Total Nitrogen in Bulk Solids - 15N Isotopes\nAlso includes % TN. ",66,72.599999999999994]
[null,"SS-SING-107","Total Nitrogen in filters – 15N isotopes \n",99,108.9]

{"sheet":"Waters","index":3,"n_rows":223,"n_cols":5,"rows_kept":223,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[null,"WATERS ANALYTICAL SERVICES"]
[null,"WATER TESTING"]
[]
[null,null,null,null,"Metals as Total Available / Acid Soluble unless requested otherwise. All packs have preparation and digest/extract charge included."]
[null,"ITEM CODE","SPECIFIC WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-002","Water Quality - Basic \nFor drinking and domestic use.  Includes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms, E.Coli Bacteria.",77,84.7]
[null,"SW-PACK-003","Water Quality - Comprehensive\nFor drinking and domestic use. Includes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms and E.Coli Bacteria; Nitrate; Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Manganese, Nickel, Lead, Zinc, Mercury.",120,132]
[null,"SW-PACK-004","Irrigation Suitability - Basic\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Iron and Manganese; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride; Turbidity, Total Alkalinity, Water Hardness (calculation), Saturation Index; Sodium Absorption Ratio (SAR).",88,96.8]
[null,"SW-PACK-005","Irrigation and Livestock Suitability – Comprehensive\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms and E.Coli Bacteria; Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Manganese, Nickel, Lead, Zinc; Nitrate, Ammonium, Phosphate; Sodium, Potassium, Calcium, Magnesium, Chloride, Sulfate, Sodium Absorption Ratio (SAR).",165,181.5]
[null,"SW-PACK-015","Wastewater Monitoring\nIncludes pH, Total Suspended Solids (TSS); Biochemical Oxygen Demand (BOD); Total Oils and Grease (TOG).",104,114.4]
[null,"SW-PACK-016","Acid Sulfate Waters\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Titratable Acidity; Dissolved Iron and Aluminium; Sulfate, Chloride, Sulfate: Chloride Ratio.",77,84.7]
[null,"SW-PACK-021","Aggressivity Assessment\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Resistivity (Calculation), Soluble Chloride, Sulfate.",49,53.9]
[null,"SW-PACK-007","Agricultural Stock Use\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Water Hardness; Total Alkalinity; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury; Nitrate, Ammonium, Phosphate; Faecal Coliforms.",135,148.5]
[null,"SW-PACK-041","Aquaculture Monitoring Suite\nIncludes pH, Total Suspended Solids (TSS), Biochemical Oxygen Demand (BOD), Total Nitrogen (TN), Total Phosphorus (TP).",99,108.9]
[null,"SW-PACK-001","Bacteria\nIncludes Total Coliforms and E.Coli.",49,53.9]
[null,"SW-PACK-025","Dust Analysis\nAs per Total Suspended Solids (TSS) and Method AS 3580.10.1.8.2.2-1991.",27,29.7]
[null,"SW-PACK-022","Dust Ashing Analysis\nIncludes Volatile Suspended Solids (VSS), Total Suspended Solids (TSS), Total Dissolved Solids (TDS).",71,78.099999999999994]
[null,"SW-PACK-018","Effluent Monitoring\nIncludes pH, Total Suspended Solids (TSS); Biochemical Oxygen Demand (BOD); Total Oils and Grease (TOG); Total Nitrogen (TN), Total Phosphorus (TP); Nitrate, Nitrite, Phosphate, Ammonium; Faecal Coliforms.",210,231]
[null,"SW-PACK-012","Environmental Monitoring 1a\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Suspended Solids (TSS); Nitrate, Nitrite, Phosphate, Ammonium; Total Nitrogen (TN), Total Phosphorus (TP).",110,121]
[null,"SW-PACK-013","Environmental Monitoring 1b (EPA Suite)\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Suspended Solids (TSS); Nitrate, Nitrite, Phosphate, Ammonium; Total Nitrogen and Total Phosphorus; Biochemical Oxygen Demand (BOD).",140,154]
[null,"SW-PACK-017","Environmental Monitoring 2\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Suspended Solids (TSS); Total Nitrogen and Total Phosphorus; Nitrate, Nitrite, Phosphate, Ammonium; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride; Bicarbonate Alkalinity, Water Hardness (calculation); Sodium Absorption Ratio (SAR).",200,220]
[null,"SW-PACK-058","Gas Contamination Monitoring for Dissolved Gases\nIncludes Acetylene, Butane, Ethane, Ethene, Methane and Propane.",155,170.5]
[null,"SW-PACK-056","Gas Contamination Water Quality Monitoring\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Total Alkalinity, Total Suspended Solids (TSS); Total Petroleum Hydrocarbons (TPH C10-C40), BTEX (Equivalent TPH C6-C10); Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",180,198]
[null,"SW-PACK-080","General Plant Pathogen Scan Plus\nGeneral plant pathogen water scan including Phytophthora, Pythium, Rhizoctonia and Fusarium.\r\n\r\nNote: 1 L of sample is required to complete testing.",550,605]
[null,"SW-PACK-078","Liquid Compost Analysis\nIncludes pH, EC; TOC, TN; NO3, NH4, PO4; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Salmonella, Ecoli, Faecal Coliforms. Note: 1 L of sample required as well as 200 mL Bacto sample.",310,341]
[null,"SW-PACK-026","Liquid - Fertiliser Totals\nIncludes acid digestion then ICP analysis for Phosphorus; Sodium, Potassium, Calcium, Magnesium, Sulfur; Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron. Also includes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Nitrogen (TN).",200,220]
[null,"SW-PACK-057","Liquid - Hydroponic Availables\nIncludes 0.45 um filter then ICP analysis for Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride; Available Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron. Also includes pH, EC; Total Nitrogen (TN), Phosphorus (TP).",140,154]
[null,"SW-PACK-070","MRTS - FORM I - Non-potable Water Testing and Assessment Report\nIncludes pH, EC; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride, Sodium Absorption Ratio (SAR); Bicarbonate / Carbonate Alkalinity;  Salmonella, Ecoli, Total Coliforms.",165,181.5]
[null,"SW-PACK-020","Nutrients - Dissolved\nIncludes Nitrate, Nitrite, Phosphate, Ammonium.",49,53.9]
[null,"SW-PACK-019","Nutrients - Total \nIncludes Total Nitrogen (TN), Total Phosphorus (TP).",55,60.5]
[null,"SW-PACK-042","Petroleum Hydrocarbons\nIncludes Total Petroleum Hydrocarbons (TPH C10-C40), BTEX (Equivalent TPH C6-C10).",88,96.8]
[null,"SW-PACK-023","Renal RO Analysis\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Sodium, Potassium, Calcium, Magnesium, Chloride, Sulfate, Water Hardness (calculation), Nitrate, Nitrite, Phosphate, Ammonium; Fluoride, Barium; Available Metals (Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury).",140,154]
[null,"SW-PACK-077","Plant pathogens in water\nIncludes Phytophthora and Pythium.",165,181.5]
[null,"SW-PACK-076","Public Pools Microbiological Monitoring\nMicrobiological analysis of Total Plate Count (ie. Heterotrophic colony count), Ecoli and Pseudomonas aeruginosa\r\n(250ml bacto sample container with thiosulfate preservative- do not rinse container).",110,121]
[null,"SW-PACK-014","Salts Suite\nIncludes pH, EC, Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride; Total Alkalinity, Water Hardness (calculation); Sodium Absorption Ratio (SAR).",77,84.7]
[null,"SW-PACK-028","Volatile Fatty Acids (VFA)\nIncludes Volatile Fatty Acids (VFA), pH, Alkalinity.",66,72.599999999999994]
[null,"SW-PACK-079","Water Contamination Assessment\nIncludes Metals (Total Available Al, As, Cd, Cr, Cu, Fe Pb, Mn, Hg, Ni, Se, Ag, Zn), PAH, TPH, BTEX, and speciated Phenolics.",240,264]
[null,"SW-PACK-071","Water quality for concrete mixes under AS1379 \nIncludes pH, EC, TDS (by calc), Total Suspended Solids, Total Oils and Grease, Sugars (Biological Oxygen Demand), Chloride, Sodium and Sulfate.",155,170.5]
[null,"SW-PACK-055","Water Analysis - Basic\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Total Suspended Solids (TSS).",33,36.299999999999997]
[null,"SW-PACK-073","Water Source Identification\nIncludes pH, EC, TDS (Calc), turbidity, nitrate, nitrite, ammonia, phosphate, fluoride, Total and free residual chlorine and Ecoli bacteria (used to indicate if water is sourced from town reticulation, sewage, recycling, ground, surface or rain water – comments provided on email of results).",155,170.5]
[]
[]
[null,"ITEM CODE","WATERS PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PREP-005","As Supplied - Research Samples/External Preparation\n",0,0]
[null,"SW-PREP-003","Filtered/Dissolved Metals\nImmediate filtration through 0.45 µm filter followed by acidification with Nitric acid. It is particularly important where waters are high in suspended clay matter, where Iron and Aluminium may be present.",5,5.5]
[null,"SW-PREP-006","Saline Waters Instrument Setup (per batch)\n",110,121]
[null,"SW-PREP-007","Total Acid Digestible Metals\nNitric Acid digest. Used on oils, liquid fertilisers and when requested.",33,36.299999999999997]
[null,"SW-PREP-002","Total Available/Acid Soluble Metals\nAcidification with Nitric acid.  Used on nearly all environmental waters, acid sulfate waters, groundwater and surface waters (According to ANZECC guidelines).  Also used for clean waters, drinking waters, when acidified in the field and when requested.",5,5.5]
[null,"SW-PREP-001","Total Recoverable Metals\nNitric Acid digest. Used on high sludge/solid waters and when requested.",16,17.600000000000001]
[]
[null,null,null,null,"All packs have preparation and digest/extract charge included. Saline waters that request low level metals require (SW-PREP-006)."]
[null,"ITEM CODE","METAL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-031","Basic Metals Scan - As Supplied (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",60,66]
[null,"SW-PACK-040","Basic Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-029","Basic Metals Scan - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-030","Basic Metals Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",71,78.099999999999994]
[null,"SW-PACK-043","Extra Metals Scan - As Supplied (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",60,66]
[null,"SW-PACK-044","Extra Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-045","Extra Metals Scan - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-046","Extra Metals Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",71,78.099999999999994]
[null,"SW-PACK-074","Metals Screen in Oil - Total Acid Digestible (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.\r\nNote: 25 mL required to complete testing.",99,108.9]
[null,"SW-PACK-060","Saline Water Metals (Low Level) > 20 mS/cm (As Supplied) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",88,96.8]
[null,"SW-PACK-061","Saline Water Metals (Low Level) > 20 mS/cm (Dissolved) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",93,102.3]
[null,"SW-PACK-062","Saline Water Metals (Low Level) > 20 mS/cm (Total Available/Acid Soluble) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",93,102.3]
[null,"SW-PACK-063","Saline Water Metals (Low Level) > 20 mS/cm (Total Recoverable) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",99,108.9]
[null,"SW-PACK-039","Salts Scan - As Supplied (ICPMS)\nIncludes Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",33,36.299999999999997]
[null,"SW-PACK-036","Salts Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",38,41.8]
[null,"SW-PACK-037","Salts Scan - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",38,41.8]
[null,"SW-PACK-038","Salts Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",44,48.4]
[null,"SW-PACK-051","Special - Metals and Salts Combo - As Supplied (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",120,132]
[null,"SW-PACK-052","Special - Metals and Salts Combo - Dissolved (filtered then acidified) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",130,143]
[null,"SW-PACK-053","Special - Metals and Salts Combo - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",130,143]
[null,"SW-PACK-054","Special - Metals and Salts Combo - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",135,148.5]
[null,"SW-PACK-067","Speciated Arsenic\nIncludes toxic arsenic species AsV and AsIII determination using HPLC-ICPMS (Total Arsenic analysis also included) 1% of volume HCl preservation in PP.",385,423.5]
[null,"SW-PACK-068","Speciated Chromium\nIncludes toxic hexavalent chromium species CrVI and CrIII determination using HPLC-ICPMS (Total Chromium analysis also included) 1M NaOH preservation (approx.. 3 Drops/30ml to adjust pH to 8-9.5) in PP.",385,423.5]
[null,"SW-PACK-066","Speciated Mercury\nIncludes toxic mercury species Methyl Mercury and Hg2+ determination using HPLC-ICPMS. (Total Mercury analysis also included) 1% of volume HCl preservation in glass jar.",385,423.5]
[null,"SW-PACK-047","Specific - Rare Earth - As Supplied (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",82,90.2]
[null,"SW-PACK-048","Specific - Rare Earth - Dissolved (filtered then acidified) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",88,96.8]
[null,"SW-PACK-049","Specific - Rare Earth - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",88,96.8]
[null,"SW-PACK-050","Specific - Rare Earth - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",93,102.3]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL METAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-102","General Metals - As Supplied (external prep)\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-103","General Metals - Dissolved\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-104","General Metals - Total Available/Acid Soluble\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-105","General Metals - Total Recoverable\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-133","General Metals - Total Acid Digestable\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",16,17.600000000000001]
[null,"SW-SING-106","Non-Standard Metals - As Supplied\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-107","Non-Standard Metals - Dissolved\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-108","Non-Standard Metals - Total Available/Acid Soluble\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-109","Non-Standard Metals - Total Recoverable\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[]
[null,null,null,null,"All packs have preparation and digest/extract charge included."]
[null,"ITEM CODE","RESIDUE SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-072","Complete Waters Residue Screen \nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue).",240,264]
[null,"SW-PACK-009","Pesticide Screen 1a\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).",77,84.7]
[null,"SW-PACK-010","Pesticide Screen 1b\nIncludes Organo-chlorines (OC), Organo-phosphates (OP) and Polychlorinated biphenyls (PCB).",99,108.9]
[null,"SW-PACK-024","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Organo-phosphates (OP).",140,154]
[null,"SW-PACK-027","Pesticide Screen 2b - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",155,170.5]
[null,"SW-PACK-059","Pesticide Screen 3 - In Oil (Detection est. <10ppm)\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).\r\nNote: 25 mL required.",165,181.5]
[null,"SW-PACK-075","Pesticides/ Residue Screen – In Oil (Detection 0.1ppm) \nIncludes Organo-chlorines (OC), Organo-phosphates (OP) and a Multi-residue scan.\r\nNote: 25 mL required.",200,220]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL RESIDUE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-116","Glyphosate (Round Up)\n",190,209]
[null,"SW-SING-098","Herbicides Phenoxy Acid\n",190,209]
[null,"SW-SING-062","Hydrocarbons - BTEX (Equivalent to TPH C6-C10)\n",55,60.5]
[null,"SW-SING-008","Hydrocarbons - Polycyclic Aromatic Hydrocarbons (PAH)\n",71,78.099999999999994]
[null,"SW-SING-063","Hydrocarbons - Total Petroleum (TPH C10-C40)\n",55,60.5]
[null,"SW-SING-064","Organo-chlorines (OC)\n",71,78.099999999999994]
[null,"SW-SING-113","Organo-chlorines (OC) - In Oil\nNote: 25 mL required.",135,148.5]
[null,"SW-SING-096","Organo-chlorines (OC) - Low Level\n",99,108.9]
[null,"SW-SING-065","Organo-phosphates (OP)\n",71,78.099999999999994]
[null,"SW-SING-114","Organo-phosphates (OP) - In Oil\nNote: 25 mL required.",135,148.5]
[null,"SW-SING-097","Organo-phosphates (OP) - Low Level \n",99,108.9]
[null,"SW-SING-117","Organotins (MBT, TBT, DBT)\n",285,313.5]
[null,"SW-SING-121","PFAS in water – standard level 28 suite with detection 0.01 - 0.05 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in water.",165,181.5]
[null,"SW-SING-134","PFAS in water – LOW level 28 suite with detection 0.0002 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in water.",190,209]
[null,"SW-SING-038","Phenol - Total \n",66,72.599999999999994]
[null,"SW-SING-026","Phenolics - Speciated Phenols\n",99,108.9]
[null,"SW-SING-066","Polychlorinated Biphenyls (PCB)\n",71,78.099999999999994]
[null,"SW-SING-099","Polychlorinated Biphenyls (PCB) - Low Level \n",99,108.9]
[null,"SW-SING-111","Semi-Volatile Organic Compounds (SVOC)\nSVOC includes Phenols.",240,264]
[null,"SW-SING-037","Trihalomethanes (THM)\n",66,72.599999999999994]
[null,"SW-SING-095","Volatile Halogenated Compounds (VHC)\n",99,108.9]
[null,"SW-SING-094","Volatile Organic Compounds (VOC)\nVOC includes BTEX.",130,143]
[]
[]
[null,"ITEM CODE","INDIVIDUAL MICROBIAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-039","Bacteria - Faecal Coliforms\n",38,41.8]
[null,"SW-SING-040","Bacteria - Total Coliforms\n",38,41.8]
[null,"SW-SING-041","E.Coli - 24h Incubation\n",44,48.4]
[null,"SW-SING-042","Enterococci\n",49,53.9]
[null,"SW-SING-036","Legionella\n",110,121]
[null,"SW-SING-043","Listeria\n",66,72.599999999999994]
[null,"SW-SING-044","Pseudomonas\n",49,53.9]
[null,"SW-SING-045","Salmonella\n",66,72.599999999999994]
[null,"SW-SING-046","Total Plate Count\n",49,53.9]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL NITROGEN TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-047","Ammonium\n",22,24.2]
[null,"SW-SING-048","Nitrate\n",22,24.2]
[null,"SW-SING-049","Nitrite\n",22,24.2]
[null,"SW-SING-050","NOx\n",22,24.2]
[null,"SW-SING-051","Total Kjeldahl Nitrogen (TKN)\nIncludes Total Nitrogen and NOx.",44,48.4]
[null,"SW-SING-052","Total Nitrogen (TN)\n",33,36.299999999999997]
[null,"SW-SING-118","Total Nitrogen by LECO\n",33,36.299999999999997]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL GENERAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-142","Absorbance (Wavelength 440nm – Filtered 0.22 micron)\n",22,24.2]
[null,"SW-SING-031","Acidity (Titratable)\nIncludes pH.",19,20.9]
[null,"SW-SING-022","Algae - Basic ID and Count (Blue Green Algae only) by Microscopic Identification\n",120,132]
[null,"SW-SING-123","Algae - Full ID and Count by Microscopic Identification\n",180,198]
[null,"SW-SING-075","Alkalinity - Bicarbonate\n",19,20.9]
[null,"SW-SING-076","Alkalinity - Carbonate\n",19,20.9]
[null,"SW-SING-077","Alkalinity - Total\n",19,20.9]
[null,"SW-SING-110","Biochemical Oxygen Demand (BOD) - Dissolved\n",49,53.9]
[null,"SW-SING-012","Biochemical Oxygen Demand (BOD) - Total\n",49,53.9]
[null,"SW-SING-078","Carbon - Dissolved Organic (DOC)\n",55,60.5]
[null,"SW-SING-079","Carbon - Total Organic (TOC)\n",55,60.5]
[null,"SW-SING-119","Carbon - Total Organic (TOC) by LECO\n",55,60.5]
[null,"SW-SING-013","Chemical Oxygen Demand (COD)\n",49,53.9]
[null,"SW-SING-143","Chemical Oxygen Demand - Filtered (COD-F)\nFiltered GFC 1.2micron equivalent",55,60.5]
[null,"SW-SING-080","Chloride - Available\n",19,20.9]
[null,"SW-SING-081","Chlorine - Free\n",19,20.9]
[null,"SW-SING-082","Chlorine - Total Residual\nIncludes Total Residual Chlorine and Free Chlorine.",39,42.9]
[null,"SW-SING-017","Chlorophyll 'a' and Algal Biomass\n",59,64.900000000000006]
[null,"SW-SING-030","Chromium VI - Hexavalent \nSpeciation by a screening colourimetric technique which may be subject to matrix interference. Refer to separate analysis codes for speciation using HPLC-ICPMS analysis.",39,42.9]
[null,"SW-SING-073","Colour - Apparent\n",15,16.5]
[null,"SW-SING-074","Colour - True\n",15,16.5]
[null,"SW-SING-056","Conductivity - Electrical\n",11,12.1]
[null,"SW-SING-029","Cyanide - Total\n",55,60.5]
[null,"SW-SING-083","Fluoride\n",33,36.299999999999997]
[null,"SW-SING-116","Glyphosate (Round Up)\n",190,209]
[null,"SW-SING-084","Hardness\n",19,20.9]
[null,"SW-SING-124","Insoluble Matter – Liquid Fertilisers\nIncludes insoluble matter mg/L.",33,36.299999999999997]
[null,"SW-SING-027","Iodine - Total \n",66,72.599999999999994]
[null,"SW-SING-085","Moisture (105°C)\n",22,24.2]
[null,"SW-SING-058","Oxygen - Dissolved (DO)\n",11,12.1]
[null,"SW-SING-115","Particle Size Analysis - Laser Diffraction\nParticle size analysis using a Malvern Mastersizer 3000. Span 0.01 to 3000 µm. Size classes dictated by client requirements.\r\nPrice dependent upon application and sample amounts.",190,209]
[null,"SW-SING-055","pH\n",11,12.1]
[null,"SW-SING-054","Phosphorus - Available Orthophosphate\n",22,24.2]
[null,"SW-SING-053","Phosphorus - Total (TP)\nAutoclave digestion and analysis by FIA.",33,36.299999999999997]
[null,"SW-SING-059","Redox\n",11,12.1]
[null,"SW-SING-057","Salinity\n",11,12.1]
[null,"SW-SING-141","Silica Gel Clean-up TRH\nIncludes TRH C9-C40 Natural/ Petroleum differentiation – silica gel clean-up (removes all of the biogenic, more polar material leaving just the petrogenic based TRH).",120,132]
[null,"SW-SING-122","Silica - Total\nIncludes specialised NaOH high temperature fusion extraction of silicon as per dry weight. ",165,181.5]
[null,"SW-SING-120","Specific Gravity - Hydrometer method\nIncludes specific gravity and temperature on sample volumes greater than 200 mL.",22,24.2]
[null,"SW-SING-035","Specific Gravity - Volumetric method\nIncludes specific gravity and temperature on samples with small volumes.",22,24.2]
[null,"SW-SING-067","Sulfide - Dissolved\n",33,36.299999999999997]
[null,"SW-SING-068","Sulfide - Total\n",33,36.299999999999997]
[null,"SW-SING-100","Sulfite - Dissolved\n",24,26.4]
[null,"SW-SING-101","Sulfite - Total\n",24,26.4]
[null,"SW-SING-028","Surfactant - MBAS\n",55,60.5]
[null,"SW-SING-021","Tannin/Lignin\n",66,72.599999999999994]
[null,"SW-SING-060","Temperature\n",11,12.1]
[null,"SW-SING-061","Total Dissolved Salts (TDS) (calculation)\n",11,12.1]
[null,"SW-SING-034","Total Dissolved Solids (TDS)\nIncludes filtering and TDS by evaporation.",33,36.299999999999997]
[null,"SW-SING-118","Total Nitrogen by LECO\n",33,36.299999999999997]
[null,"SW-SING-011","Total Oils and Grease (TOG) - Hexane extractable\n",55,60.5]
[null,"SW-SING-033","Total Solids\n",33,36.299999999999997]
[null,"SW-SING-003","Total Suspended Solids (TSS)\n",22,24.2]
[null,"SW-SING-069","Turbidity\n",13,14.3]
[null,"SW-SING-070","UV Absorbency\n",27,29.7]
[null,"SW-SING-072","UV Transmission - Filtered\n",27,29.7]
[null,"SW-SING-071","UV Transmission - Unfiltered\n",27,29.7]
[null,"SW-SING-005","Volatile Suspended Solids (VSS)\n",38,41.8]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL STABLE ISOTOPE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-136","Total Inorganic Carbon (TIC) - 13C Isotopes\nIncludes both saline and non-saline waters. ",55,60.5]
[null,"SW-SING-137","Total Organic Carbon (TOC) - 13C Isotopes\nIncludes both saline and non-saline waters. ",88,96.8]
[null,"SW-SING-125","Total Inorganic and Organic (TIC and TOC) - 13C Isotopes\nIncludes both saline and non-saline waters. ",135,148.5]
[null,"SW-SING-128","Dissolved Nitrogen - 15N Isotopes\nIncludes Dissolved N2 isotope testing - ratio masses 29/28.",82,90.2]
[null,"SW-SING-129","Dissolved Nitrous Oxide - 15N Isotopes\n",140,154]
[null,"SW-SING-135","Nitrate Stable Isotope Analysis - 15N & 18O Isotopes\nIncludes Delta 15N and delta 18O of nitrate fresh and saline water samples (includes nitrate analysis to confirm minimum 0.14mg/L N required for isotope analysis).",165,181.5]
[null,"SW-SING-130","Dissolved Gas Analysis\nIncludes N2/Ar non-isotope ratio measurement.",55,60.5]
[null,"SW-SING-138","Hydrogen Isotopes in Water - 2H Isotopes\n",63,69.3]
[null,"SW-SING-140","Hydrogen and Oxygen Isotopes in Water - 2H and 18O Isotopes\n",110,121]
[null,"SW-SING-139","Oxygen Isotopes in Water - 18O Isotopes\n",63,69.3]

{"sheet":"Acid sulfate soil","index":4,"n_rows":71,"n_cols":5,"rows_kept":71,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[null,"ACID SULFATE ANALYTICAL TESTING"]
[null,"SOIL TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"AS-PACK-007","Acid Sulfate pH-F and pH-FOX Testing\nIncludes moisture content, drying and ring mill grinding. Field based technique modified for lab use. Results should be used in conjunction with field descriptions to indicate which samples require further laboratory testing.",22,24.2]
[null,"AS-PACK-008","Acid Sulfate Soil Net Acidity - S-CR (National Guidance 2018)\nIncludes Net Acidity and liming rate with analysis of Reduced Inorganic Sulfur (Chromium Reducible Sulfur; S-CR), KCl extractable pH (pH-KCl), Actual Acidity (Titratable Actual Acidity; TAA) where pH-KCl < 6.5, Retained Acidity (Net Acid Soluble Sulfur; S-NAS) where pH-KCl < 4.5 and Acid Neutralising Capacity (ANC-BT) where pH-KCl => 6.5.",99,108.9]
[null,"AS-PACK-013","Acid Sulfate Soil Net Acidity - S-POS (National Guidance 2018)\nIncludes Net Acidity and liming rate with analysis of Reduced Inorganic Sulfur (Peroxide Oxidisable Sulfur; S-POS), KCl extractable pH (pH-KCl), Actual Acidity (Titratable Actual Acidity; TAA) where pH-KCl < 6.5, Retained Acidity (Net Acid Soluble Sulfur; S-NAS) where pH-KCl < 4.5 and Acid Neutralising Capacity (ANC-BT) where pH-KCl => 6.5.",140,154]
[null,"AS-PACK-011","Acid Sulfate Soil Net Acidity for Treatment Verification (National Guidance 2018)\nIncludes Net Acidity and liming rate with analysis of Reduced Inorganic Sulfur (Chromium Reducible Sulfur; S-CR), KCl extractable pH (pH-KCl), Actual Acidity (Titratable Actual Acidity; TAA) where pH-KCl < 6.5 and Acid Neutralising Capacity (ANC-BT). \r\nClient must provide pre-liming ANC-BT.\r\nRoutine TAT of 3 days with a reduced surcharge of 50% for 24 h TAT (limited to 15 samples).\r\n",110,121]
[null,"AS-PACK-004","Acid Volatile Sulfide and Reduced Inorganic Sulfur\nIncludes Acid Volatile Sulfide (S-AV) and Chromium Reducible Sulfur (S-CR).",135,148.5]
[null,"AS-PACK-001","Actual and Potential Acidity\nIncludes analysis of Reduced Inorganic Sulfur (Chromium Reducible Sulfur; S-CR), KCl extractable pH (pH-KCl), Actual Acidity (Titratable Actual Acidity; TAA) where pH-KCl < 6.5. If Net Acidity and Liming Rate are required AS-PACK-008 should be used instead of AS-PACK-001.",77,84.7]
[null,"SS-PACK-054","Incubation - Chip Tray\nThis method is used to assess the effectiveness of a soil's Acid Neutralising Capacity (ANC). Includes pH-F before and pH-INC after 9 weeks incubation, with further incubation to 19 weeks where 4 <= pH-INC <= 6.5.",66,72.599999999999994]
[null,"SS-PACK-073","Incubation - Slab\nThis method is used to assess the effectiveness of a soil's Acid Neutralising Capacity (ANC). The incubation is maintained and pH-INC taken fortnightly until the soil pH changes by at least 0.5 pH unit to below 4, or for at least 8 weeks until pH-INC is stable.",200,220]
[null,"AS-PACK-012","Sulfate to Chloride Ratio\nIncludes Sulfate and Chloride (1:1 water) and Sulfate/Chloride Ratio.\r\n",55,60.5]
[]
[]
[null,"ITEM CODE","SOIL PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-010","Acid Sulfate Soil - Sample Preparation - Required for all individual testing\nIncludes 80°C moisture content, drying and ring mill grinding. Required for all samples analysed on a dry weight basis.  ",11,12.1]
[null,"SS-PREP-016","Fizz Test for Carbonates \nThis method is used to indicate the presence of carbonates.",3,3.3]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-PREP-017","Total Dry Weight - Oven dry basis\nMass of the sample dried at 105°C. Used to calculate bulk density when cores are supplied.",11,12.1]
[]
[null,null,null,null,"All samples require Sample Preparation (SS-PREP-010) unless a discounted testing suite is selected."]
[null,"ITEM CODE","INDIVIDUAL SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-090","Acid Neutralising Capacity (ANC-BT)\nThis method is used to measure Acid Neutralising Capacity (ANC-BT) where pH-KCl > 6.5.",33,36.299999999999997]
[null,"SS-SING-201","Acid Neutralising Capacity by Total Inorganic Carbon (C-IN)\nThis method is used to measure Acid Neutralising Capacity (ANC) where the pH-KCl > 6.5.\r\n\r\n",49,53.9]
[null,"SS-SING-250","Acid Sulfate Soil Field pH-W and pH-FOX\nIncludes pH-W and pH-FOX on raw sample, as supplied. Results should be used in conjunction with field descriptions to indicate which samples require further laboratory testing.",11,12.1]
[null,"SS-SING-089","Acid Volatile Sulfide (AVS)\nThis method measures Acid Volatile Sulfides (S-AV). All samples should be frozen on collection and transported in an esky with freezer bricks.",55,60.5]
[null,"SS-SING-088","Chromium Reducible Sulfur (CRS)\nThis method measures Reduced Inorganic Sulfur (S-CR) and is not subject to interferences by sulfate minerals and organic matter.",55,60.5]
[null,"SS-SING-064","Electrical Conductivity (1:5 water)\n",16,17.600000000000001]
[null,"SS-SING-246","Elemental Sulfur\nThis includes Elemental Sulfur (S-E). 100% surcharge for single samples to cover setup costs.",155,170.5]
[null,"SS-SING-093","Net Acid Soluble Sulfur (S-NAS)\nThis method estimates Retained Acidity where pH-KCl < 4.5.",33,36.299999999999997]
[null,"SS-SING-095","Titratable Actual Acidity (TAA)\nThis method measures Actual Acidity. Titratable Actual Acidity (TAA) titrated to pH 6.5.",33,36.299999999999997]
[null,"SS-SING-097","Titratable Actual Acidity (TAA) and KCl Extractable Sulfur (S-KCl)\n",38,41.8]
[null,"SS-SING-101","pH and Sulfate (1:1 water)\nThis method is used for classification of actual acid sulfate soil materials.",33,36.299999999999997]
[null,"SS-SING-202","pH - KCl extractable (pH-KCl)\nThis method is used to determine what further testing is required for Net Acidity calculations: Titratable Actual Acidity (TAA; pH-KCl < 6.5), Net Acid Soluble Sulfur (S-NAS; pH-KCl < 4.5), Acid Neutralising Capacity (ANC-BT or C-IN; pH-KCl => 6.5).\r\n",22,24.2]
[null,"SS-SING-098","Sulfur - KCl Extractable\nThis method is used to measure sulfur concentration after Titratable Actual Acidity (TAA) analysis.",11,12.1]
[null,"SS-SING-163","Peroxide Oxidisable Sulfur (S-POS)\nThis method estimates Reduced Inorganic Sulfur. It can include interferences from sulfate minerals and organic matter.",93,102.3]
[null,"SS-SING-208","Texture - Full (NCST, 2009)\nThis method is used for acid sulfate soil action criteria.",27,29.7]
[]
[null,"ROCK TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","ROCK SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"AS-PACK-010","Acid Sulfate Rock with Chromium Reducible Sulfur\nIncludes Net Acid Producing Potential (NAPP), NAG pH and Net Acid Generation (NAG) (single addition peroxide acidity), Acid Neutralising Capacity (ANC-BT) and Reduced Inorganic Sulfur (S-CR) (combined in NAPP equation).",120,132]
[null,"AS-PACK-006","Acid Sulfate Rock with Total Sulfur\nIncludes Net Acid Producing Potential (NAPP), NAG pH and Net Acid Generation (NAG) (single addition peroxide acidity), Acid Neutralising Capacity (ANC-BT) and Total Sulfur (combined in NAPP equation).",99,108.9]
[]
[]
[null,"ITEM CODE","ROCK PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-010","Acid Sulfate Soil - Sample Preparation - Required for all individual testing\nIncludes 80°C moisture content, drying and ring mill grinding. Required for all samples analysed on a dry weight basis.  ",11,12.1]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[]
[null,null,null,null,"All samples require Sample Preparation (SS-PREP-010) unless a discounted testing suite is selected."]
[null,"ITEM CODE","INDIVIDUAL ROCK TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-090","Acid Neutralising Capacity (ANC-BT)\nThis method is used to measure Acid Neutralising Capacity (ANC-BT) where pH-KCl > 6.5.",33,36.299999999999997]
[null,"SS-SING-201","Acid Neutralising Capacity by Total Inorganic Carbon (C-IN)\nThis method is used to measure Acid Neutralising Capacity (ANC) where the pH-KCl > 6.5.\r\n\r\n",49,53.9]
[null,"SS-SING-088","Chromium Reducible Sulfur (CRS)\nThis method measures Reduced Inorganic Sulfur (S-CR) and is not subject to interferences by sulfate minerals and organic matter.",55,60.5]
[null,"SS-SING-102","Net Acid Generation (NAG)\nThis method is used to determine the Net Acid Generation (NAG) of rock material. Includes NAGpH.",55,60.5]
[null,"SS-SING-144","Total Sulfur (TS) by LECO\n",22,24.2]
[]
[null,"WATER TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-016","Acid Sulfate Waters\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Titratable Acidity; Dissolved Iron and Aluminium; Sulfate, Chloride, Sulfate: Chloride Ratio.",77,84.7]
[null,"SW-PACK-029","Basic Metals Scan - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-040","Basic Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-044","Extra Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-045","Extra Metals Scan - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-048","Specific - Rare Earth - Dissolved (filtered then acidified) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",88,96.8]
[null,"SW-PACK-049","Specific - Rare Earth - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",88,96.8]

{"sheet":"Agricultural","index":5,"n_rows":211,"n_cols":5,"rows_kept":211,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[null,"AGRICULTURAL ANALYTICAL SERVICES"]
[null,"SOIL TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","ROUTINE SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"RA-PACK-001","Agricultural - Albrecht/Reams\nIncludes pH and EC (1:5 water); Available Calcium, Magnesium, Potassium, Ammonium, Nitrate, Phosphate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), Organic Matter, TC/TN Ratio; Basic Colour, Basic Texture.",120,132]
[null,"RA-PACK-002","Agricultural - Albrecht/Reams plus Totals\nIncludes pH and EC (1:5 water); Available Calcium, Magnesium, Potassium, Ammonium, Nitrate, Phosphate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Basic Colour, Basic Texture; Total Sodium, Potassium, Calcium, Magnesium, Sulfur,  Phosphorus, Silicon, Cobalt, Molybdenum, Selenium, Zinc, Manganese, Iron, Copper, Boron and Aluminium.",180,198]
[null,"RA-PACK-003","Agricultural - Albrecht/Reams plus Totals and Heavy Metals\nIncludes pH and EC (1:5 water); Available Calcium, Magnesium, Potassium, Ammonium, Nitrate, Phosphate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Basic Colour, Basic Texture; Total Sodium, Potassium, Calcium, Magnesium, Sulfur, Phosphorus, Silicon, Cobalt, Molybdenum, Selenium, Zinc, Manganese, Iron, Copper, Boron and Aluminium; Heavy Metals Silver, Arsenic, Lead, Chromium, Nickel, Cadmium, Mercury.",200,220]
[null,"RA-PACK-014","Agricultural - Standard C\nIncludes pH and EC (1:5 water); pH (1:5 CaCl); Available (Ammonium, Nitrate, Sulfur); Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Colwell Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Basic Colour, Basic Texture.",110,121]
[null,"RA-PACK-015","Agricultural - Sugarcane Reefwise\nIncludes pH and EC (1:5 water); pH (1:5 CaCl); Available Ammonium, Nitrate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Nitric Acid Extractable Potassium; Colwell Phosphorus, Phosphorous Buffer Index (PBI), BSES Phosphorus, Silicon; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; HCl Extractable Zinc; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Organic Carbon (W-B); Basic Colour, Basic Texture.",155,170.5]
[null,"RA-PACK-017","Agricultural Basic Home\nIncludes pH and EC (1:5 water); Exchangeable Sodium, Potassium, Calcium, Magnesium, Cation Exchange Capacity; Bray I Phosphorus; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter.",66,72.599999999999994]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","OTHER SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"RA-PACK-004","Agricultural - Standard A-1\nIncludes pH and EC (1:5 water); Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Bray I Phosphorus; Total Carbon (TC), Total Nitrogen (TN), Organic Matter; Basic Colour, Basic Texture.",82,90.2]
[null,"RA-PACK-018","Agricultural - Standard A-2\nIncludes pH and EC (1:5 water); Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Colwell Phosphorus; Total Carbon (TC), Total Nitrogen (TN), Organic Matter; Basic Colour, Basic Texture.",82,90.2]
[null,"RA-PACK-013","Agricultural - Standard B\nIncludes pH and EC (1:5 water); Available Ammonium, Nitrate, Sulfur; Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Hydrogen, Cation Exchange Capacity; Bray I and II Phosphorus; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Basic Colour, Basic Texture.",99,108.9]
[null,"RA-PACK-041","Agricultural Sugar Cane Basic  \nIncludes Basic Texture, Basic Colour, Organic Carbon (W/B), pH/EC (H2O), pH (CaCl2), EC-SE (Calculation), Phosphorus (Colwell, BSES), Phosphorus Buffer Index, Potassium (Nitric), Exchangeable Cations (Ammonium Acetate), Aluminium (KCl), Sulfur (MCP), and Silicon (BSES, CaCl2).",135,148.5]
[null,"RA-PACK-043","Agricultural Sugar Cane Full  \nIncludes Basic Texture, Basic Colour, Organic Carbon (W/B), pH/EC (H2O), pH (CaCl2), EC-SE (Calculation), Phosphorus (Colwell, BSES), Phosphorus Buffer Index, Potassium (Nitric), Exchangeable Cations (Ammonium Acetate), Aluminium (KCl), Sulfur (MCP), Silicon (BSES, CaCl2), Zinc (HCl), Iron/Copper/Zinc/Manganese (DTPA), Chloride (H2O), Ammonium/Nitrate (KCl) and Buffer pH.",180,198]
[null,"RA-PACK-042","Agricultural Sugar Cane Standard  \nIncludes Basic Texture, Basic Colour, Organic Carbon (W/B), pH/EC (H2O), pH (CaCl2), EC-SE (Calculation), Phosphorus (Colwell, BSES), Phosphorus Buffer Index, Potassium (Nitric), Exchangeable Cations (Ammonium Acetate), Aluminium (KCl), Sulfur (MCP), Silicon (BSES, CaCl2), Zinc (HCl) and Iron/Copper/Zinc/Manganese (DTPA).",155,170.5]
[null,"SS-PACK-113","Haney – Basic Carbon and Nitrogen\nIncludes Water extractable Nitrate/Ammonium, Total Water extractable Nitrogen and Organic Carbon, Inorganic Nitrogen (Calc), Organic Nitrogen (Calc), Water extractable Organic Carbon: Organic Nitrogen Ratio (Calc).",66,72.599999999999994]
[null,"SS-PACK-114","Haney – Basic Nutrients\nIncludes Haney (H3A) extractable Nitrate, Ammonium, Calcium, Magnesium, Potassium, Sodium, Phosphorus, Sulfur, Zinc, Manganese, Iron, Copper, Aluminium.",55,60.5]
[null,"SS-PACK-115","Haney – Basic Soil Health\nIncludes Solvita CO2 respiration, Water extractable Nitrate, Ammonium; Total Water extractable Nitrogen and Organic Carbon; Inorganic Nitrogen (Calc), Organic Nitrogen (Calc), Water extractable Organic Carbon: Organic Nitrogen Ratio (Calc) and Haney Soil Health Score (Calc).",110,121]
[null,"SS-PACK-116","Haney – Routine Soil Health\nIncludes Solvita CO2 respiration, Water extractable Nitrate, Ammonium; Total Water extractable Nitrogen and Organic Carbon; Inorganic Nitrogen (Calc), Organic Nitrogen (Calc), Water extractable Organic Carbon: Organic Nitrogen Ratio (Calc) and Haney Soil Health Score (Calc). Haney (H3A) extractable Nitrate, Ammonium, Calcium, Magnesium, Potassium, Sodium, Phosphorus, Sulfur, Zinc, Manganese, Iron, Copper, Aluminium.",165,181.5]
[null,"SS-PACK-117","Haney – Total Soil Health\nIncludes Solvita CO2 respiration, Water extractable Nitrate, Ammonium; Total Water extractable Nitrogen and Organic Carbon; Inorganic Nitrogen (Calc), Organic Nitrogen (Calc), Water extractable Organic Carbon: Organic Nitrogen Ratio (Calc) and Haney Soil Health Score (Calc). Haney (H3A) extractable Nitrate, Ammonium, Calcium, Magnesium, Potassium, Sodium, Phosphorus, Sulfur, Zinc, Manganese, Iron, Copper, Aluminium. Also includes pH, EC; Total Carbon, Total Nitrogen, estimated Organic Matter and Labile Carbon.",220,242]
[null,"RA-PACK-019","Macadamia Soil Testing\nIncludes pH and EC (1:5 water); Available (Sulfur); Exchangeable Sodium, Potassium, Calcium, Magnesium, Hydrogen, Aluminium, Cation Exchange Capacity; Colwell Phosphorus, Phosphorus Buffer Index; Available Micronutrients Zinc, Manganese, Iron, Copper, Boron, Silicon; Total Carbon (TC), Total Nitrogen (TN), TC/TN Ratio, Organic Matter; Basic Colour, Basic Texture.",110,121]
[null,"NT-PACK-005","Mehlich III Basic\nIncludes pH and EC (1:5 water); Chloride Estimate, Extractable Mehlich III Phosphorus, Sodium, Potassium, Calcium, Magnesium, Cation Exchange Capacity, Exchangeable Sodium Percentage.",60,66]
[null,"SS-PACK-037","Mehlich III Exchangeable Cations and Micronutrients\nIncludes Mehlich III Extractable Sodium, Potassium, Calcium, Magnesium, Phosphorus, Sulfur, Aluminium, Iron, Copper, Zinc, Manganese, Boron.",66,72.599999999999994]
[null,"NT-PACK-001","Mehlich III Standard\nIncludes pH and EC (1:5 water); Available Calcium, Magnesium, Potassium, Ammonium, Nitrate, Phosphate, Sulfur; Mehlich III Extractable Sodium, Potassium, Calcium, Magnesium, Hydrogen/Aluminium (calculation) Cation Exchange Capacity; Mehlich III Extractable Phosphorus, Bray II Phosphorus; Total Nitrogen (TN), Total Carbon (TC), Organic Matter; Available Micronutrients Iron, Copper, Zinc, Manganese, Silicon, Boron; Paramagnetism; Basic Colour and Basic Texture.",110,121]
[null,"SS-PACK-140","Microbial Biomass Assessment - Soil\nIncludes biomasses of 12 microbial groups relevant for soil quality, health and function. ",285,313.5]
[null,"SS-PACK-167","MIC-01: Basic Analysis of Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Total fungi (moulds), Gram negative bacteria, Filamentous actinomycetes, Yeasts. ",99,108.9]
[null,"SS-PACK-168","MIC-02: Extended Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Filamentous actinomycetes, Actinobacteria, Gram negative bacteria, Filamentous fungi (Moulds), Yeasts, Lactic acid bacteria, Total Anaerobes (includes facultative anaerobes), Sulfite Reducing Anaerobes.",210,231]
[null,"SS-PACK-014","Pesticide Screen 1b\nIncludes Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",110,121]
[null,"SS-PACK-175","Phytophthora and Pythium\nNote: 500 g of sample is required to complete testing.",165,181.50000000000003]
[null,"RA-PACK-007","Reef Wise Pack - 1\nIncludes Colwell Phosphorus; Phosphorous Buffer Index (PBI); BSES Extractable Phosphorous; Organic Carbon (W-B).",66,72.599999999999994]
[null,"RA-PACK-016","Reef Wise Pack - 2\nIncludes Colwell Phosphorus; Phosphorus Buffer Index (PBI); BSES Extractable Phosphorus, Silicon; CaCl2 Extractable Silicon; HNO3 Extractable Potassium; HCl Extractable Zinc; Organic Carbon (W-B).",82,90.2]
[null,"SS-PACK-118","Residue Screen - Extended (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",310,341]
[null,"SS-PACK-119","Residue Screen - Complete + Glyphosate (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue) + Glyphosate Screens.",470,517]
[null,"SS-PACK-182","Soil/ Sediment Contamination Assessment\nIncludes Metals (Total Available Al, As, Cd, Cr, Cu, Fe Pb, Mn, Hg, Ni, Se, Ag, Zn), PAH, TPH, BTEX, and speciated Phenolics.",240,264]
[null,"SS-PACK-052","Soluble Nitrogen - Soil\nIncludes KCl extractable Nitrate and Ammonium.",44,48.4]
[null,"SS-PACK-045","Total Acid Extractable - Heavy Metals  (ICPMS)\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",55,60.5]
[null,"RA-PACK-009","Total Acid Extractable Cobalt, Molybdenum, Selenium\n",33,36.299999999999997]
[null,"RA-PACK-012","Total Acid Extractable Cobalt, Molybdenum, Selenium, Phosphorus\n",44,48.4]
[null,"RA-PACK-008","Total Acid Extractable Elements\nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Phosphorus, Silicon, Cobalt, Molybdenum, Selenium, Zinc, Manganese, Iron, Copper, Boron, Aluminium.",88,96.8]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-013","Biosecurity Handling Charge\n",110,121]
[null,"SS-SING-038","Chloride - Water Extractable",33,36.299999999999997]
[null,"SS-SING-218","Colour (Munsell Soil Colour Classification)  \n",8,8.8000000000000007]
[null,"SS-SING-085","Emerson Dispersion Index (Loveday and Pyle, 1973)\n",49,53.9]
[null,"SS-PREP-015","Exchangeable Cation Pre-treatment for Soluble Salts\nIncludes pre-treatment with aqueous ethanol and aqueous glycerol to remove soluble salts. Recommended on soils with EC > 0.3 dS/m.",11,12.1]
[null,"SS-PREP-020","Exchangeable Cation Suppression of Carbonates \nIncludes pre-treatment with aqueous ethanol and aqueous glycerol to remove soluble salts then extraction with 1M Alcoholic NH4Cl to suppress solid phase carbonates. Testing according to Method 15C1 with other agricultural tests.",44,48.4]
[null,"SS-SING-204","Fertility Report - Ferti-Tech Soil /Leaf Report Preparation\n",52,57.2]
[null,"SS-SING-071","Fertility Report - Keycrobe Soil /Leaf Report Preparation\n",52,57.2]
[null,"SS-SING-234","Fertility Report - Vital Soils Report Preparation\n",52,57.2]
[null,"SS-SING-262","Microbiometer – Soil biomass measurement\nIncludes estimates of Total Bacteria, Fungi and Fungi:Bacteria ratio. This test should only be done in conjunction with SS-Pack-167 or SS-Pack-168.",33,36.299999999999997]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-SING-066","pH (1:5 CaCl2)\n",16,17.600000000000001]
[null,"SS-SING-034","Phosphorus - Olsen\nIncludes Olsen Phosphorous - a measure of the intensity of Phosphorus.",22,24.2]
[null,"SS-SING-032","Phosphorus - Total Acid Extractable (includes preparation)\n",44,48.4]
[null,"SS-SING-037","Phosphorus Buffer Index (PBI)\n",22,24.2]
[null,"SS-SING-076","Potassium - Colwell \n",27,29.7]
[null,"SS-PREP-018","Saturated Paste Extract\nIncludes extraction of saturated paste (14A3). Please select required analytical parameters from the waters codes.",77,84.7]
[null,"SS-SING-027","Silica - Total\nIncludes specialised NaOH high temperature fusion extraction of silicon.",135,148.5]
[null,"SS-SING-209","SOLVITA - Soil CO2 Burst\nIncludes measurement of carbon dioxide released from soil due to biological activity.",66,72.599999999999994]
[null,"SS-SING-086","Texture – Full under AS 1547:2012",27,29.7]
[null,"SS-PREP-007","Total Dry Weight - Air dry basis\nMass of the sample dried at 40°C.\r\n",6,6.6]
[]
[null,"SOIL CARBON TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SOIL CARBON SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-179","Total Organic Carbon (TOC) on Topsoils under 2021 CFI Methodology\nIn CFI methodology topsoil refers to the 0 - 30 cm layer, however this should be selected on individual depth layers up to 30cm in total. \r\nIncludes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on the air-dry soil.",63,69.3]
[null,"SS-PACK-180","Total Organic Carbon (TOC) on Subsoils under 2021 CFI Methodology\nIn CFI methodology subsoil refers to the 30+cm layer however this should be selected on a depth layer of 30-100cm only. \r\nIncludes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on the air-dry soil.",94,103.4]
[null,"SS-PACK-181","Total Organic Carbon (TOC) on Core segments under 2021 CFI Methodology\nTo be selected on core segments or soil layers 0-5cm or 0-10cm. Includes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on air-dry soil.",47,51.7]
[null,"SS-PACK-193","Total Organic Carbon on Topsoils modified from 2021 CFI Methodology – not ERF registered projects\nIn CFI methodology topsoil refers to the 0-30 cm layer, however, this should be selected on individual depth layers up to 30cm in total.                                                                                                                                                                                                                                                                                                           \r\nModified method includes representative sub-sampling and analysis on reduced mass. Includes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on the air-dry soil.",57,62.7]
[null,"SS-PACK-194","Total Organic Carbon on Subsoils modified from 2021 CFI Methodology – not ERF registered projects\nIn CFI methodology subsoil refers to the 30+cm layer, however, this should be selected on a depth layer of 30-100cm only.                                                                                                                                                                                                                                                                                                            \r\nModified method includes representative sub-sampling and analysis on reduced mass. Includes Total Organic Carbon by LECO, gravel content, air-dry mass and gravimetric water content on the air-dry soil.",89,97.9]
[null,"SS-PACK-187","Carbon - Total Organic by LECO plus Gravimetric Moisture\nIncludes gravimetric moisture and TOC by LECO combustion.",52,57.2]
[null,"SS-PACK-174","Inorganic (Carbonate) Carbon by LECO\nIncludes Total Carbon (TC), Total Organic Carbon (TOC).",60,66]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL SOIL CARBON TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-018","Carbon - Labile - Blair 0.333M KMnO4",22,24.2]
[null,"SS-SING-062","Carbon - Organic by Walkley Black\n",44,48.4]
[null,"SS-SING-061","Carbon - Total Organic by LECO\n",33,36.299999999999997]
[null,"SS-SING-276","Carbon - Total Organic by LECO plus PREP\nIncludes sample preparation and TOC by LECO combustion.",42,46.2]
[null,"SS-PREP-023","Sample Compositing for Soil Carbon Subsoils (30-100cm)\nIncludes compositing charge for composite subsoil samples tested under 2018 CFI methodology.",38,41.8]
[null,"SS-PREP-022","Sample Compositing for Soil Carbon Topsoils (0-30cm)\nIncludes compositing charge for composite topsoil samples tested under 2018 CFI methodology.",16,17.600000000000001]
[]
[null,"FERTILISER TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","FERTILISER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"FA-PACK-003","Fertiliser - Liquid  Analysis\nIncludes pH, EC, Total Dissolved Salts (TDS) (by calc.); Total Nitrogen, Total Phosphorus; Sodium, Potassium, Calcium, Magnesium, Sulfur; Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper and Boron.",220,242]
[null,"FA-PACK-001","Fertiliser - Solid  Analysis\nIncludes Moisture, pH, EC; Total Nitrogen (TN), Total Carbon (TC); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Sulfur, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron.",220,242]
[null,"FA-PACK-009","Gypsum Assessment - Fertiliser\nIncludes Moisture Content, Calcium, Magnesium, Sodium and Sulfur.",135,148.5]
[null,"FA-PACK-015","LECO - Total Carbon and Total Nitrogen - Fertiliser\nIncludes Total Carbon (TC) and Total Nitrogen (TN), TC/TN Ratio.",66,72.599999999999994]
[null,"FA-PACK-014","Lime Assessment - Basic Fertiliser\nIncludes Moisture Content, Calcium, Magnesium, Acid Neutralising Capacity (ANC-BT) and Neutralising Value.",140,154]
[null,"FA-PACK-010","Lime Assessment - Coarse Fertiliser\nIncludes Moisture Content, Calcium, Magnesium, Acid Neutralising Capacity (ANC-BT), Neutralising Value and Dry Sieving Particle Size Analysis including > 1 mm, 0.85-1 mm, 0.3-0.85 mm, < 0.3 mm fractions.",180,198]
[null,"FA-PACK-011","Lime Assessment – Fine Fertiliser \nIncludes Moisture Content, Calcium, Magnesium, Acid Neutralising Capacity (ANC-BT), Neutralising Value and Laser Diffraction Particle Size Analysis including < 0.01 mm, 0.01-0.02 mm, 0.02-0.03 mm, 0.03-0.04 mm, 0.04-0.05 mm, 0.05-0.06 mm, 0.06-0.07 mm, 0.07-0.08 mm, 0.08-0.09 mm, 0.09-0.1 mm, 0.1-0.125 mm, 0.125-0.25 mm, 0.25-0.5 mm, 0.5-1.0 mm, > 1.0 mm fractions.",285,313.5]
[null,"FA-PACK-007","NPK Analysis - Fertiliser\nIncludes Total Nitrogen, Total Phosphorus, Total Potassium.",135,148.5]
[null,"FA-PACK-012","Particle Size Analysis – Dry Sieving – Coarse Fertiliser\nDry sieving Particle Size Analysis including  > 1 mm, 0.85-1 mm, 0.3-0.85 mm, < 0.3 mm fractions.",55,60.5]
[null,"FA-PACK-013","Particle Size Analysis – Laser Diffraction – Fine Fertiliser\nLaser Diffraction Particle Size Analysis including 2000 to 0.01 µm. Size fractions include < 0.01 mm, 0.01-0.02 mm, 0.02-0.03 mm, 0.03-0.04 mm, 0.04-0.05 mm, 0.05-0.06 mm, 0.06-0.07 mm, 0.07-0.08 mm, 0.08-0.09 mm, 0.09-0.1 mm, 0.1-0.125 mm, 0.125-0.25 mm, 0.25-0.5 mm, 0.5-1.0 mm, > 1.0 mm fractions.\r\nPrice dependent upon application and sample amounts.",190,209]
[null,"FA-PACK-008","Soluble Nitrogen - Fertiliser\nIncludes water extractable nitrate and ammonium on fertilisers ",88,96.8]
[null,"FA-PACK-005","Soluble Phosphorus I - Fertiliser \nIncludes Total Phosphorus, Total Soluble Phosphorus, Water Soluble Phosphorus, 2% Citrate Soluble Phosphorus.",110,121]
[null,"FA-PACK-006","Soluble Phosphorus II - Fertiliser \nIncludes Total Phosphorus, Total Soluble Phosphorus, Water Soluble Phosphorus, 2% Citrate Soluble Phosphorus and 2% Formic Acid Soluble Phosphorus.",155,170.5]
[null,"FA-PACK-002","Total Acid Extractable - Heavy Metals  (ICPMS) - Fertiliser\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",88,96.8]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL FERTILISER TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-238","Chloride – Fertiliser \nIncludes water soluble chloride on fertilisers.",66,72.599999999999994]
[null,"SS-PREP-014","Fertiliser Handling Charge\n",55,60.5]
[null,"SS-SING-067","Fluoride - Water Extractable",66,72.599999999999994]
[null,"SW-SING-124","Insoluble Matter – Liquid Fertilisers\nIncludes insoluble matter mg/L.",33,36.299999999999997]
[null,"SS-SING-240","Insoluble Matter – Solid Fertilisers\nIncludes insoluble matter mg/kg.",44,48.4]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-SING-233","Moisture Content - As Received (%) at 40°C \nMoisture content as a per cent of air-dry equivalent soil (40°C).",11,12.1]
[null,"SS-SING-193","Solubility - Fertiliser\nIncludes maximum solubility at 20°C.",44,48.4]
[null,"SW-SING-120","Specific Gravity - Hydrometer method\nIncludes specific gravity and temperature on sample volumes greater than 200 mL.",22,24.2]
[null,"SW-SING-035","Specific Gravity - Volumetric method\nIncludes specific gravity and temperature on samples with small volumes.",22,24.2]
[null,"SW-SING-149","Silicon – 2M NaOH extraction – Liquid Fertilisers\n",65,71.5]
[]
[null,"PLANT TISSUE AND GRAIN TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","PLANT TISSUE AND GRAIN SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"PA-PACK-001","Plant Testing\nIncludes Total Nitrogen (TN), Total Carbon (TC), Total Sulfur (TS); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron.",55,60.5]
[null,"PA-PACK-008","Plant Testing - Comprehensive\nIncludes Total Nitrogen (TN), Total Carbon (TC), Total Sulfur (TS); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron, Aluminium, Selenium, Chloride, Nitrate Nitrogen, Ammonium Nitrogen.",99,108.9]
[null,"PA-PACK-004","Plant Testing with Leaf Washing\nIncludes Total Nitrogen (TN), Total Carbon (TC), Total Sulfur (TS); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron, Leaf Washing.",66,72.599999999999994]
[null,"PA-PACK-002","Plant Testing with Report\nIncludes Total Nitrogen (TN), Total Carbon (TC), Total Sulfur (TS); Sodium, Potassium, Calcium, Magnesium, Phosphorus, Silicon, Cobalt, Molybdenum, Zinc, Manganese, Iron, Copper, Boron; Fertility Report.",93,102.3]
[null,"SS-PACK-118","Residue Screen - Extended (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",310,341]
[null,"PA-PACK-006","Sap Analysis\nIncludes Moisture, pH, EC, Total Nitrogen; Nitrate, Ammonium; Chloride; Calcium, Magnesium, Sodium, Potassium, Phosphorus, Sulfur, Boron, Copper, Iron, Manganese, Zinc, Aluminium, Molybdenum, Cobalt and Silicon; Brix.. Data Only (no interpretation).",88,96.8]
[null,"PA-PACK-005","Soluble Nitrogen\nIncludes Nitrate and Ammonium.",44,48.4]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL PLANT TISSUE AND GRAIN TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-271","Carbohydrates - Cold Water Soluble\n(% in plant leaf or organic material)",63,69.3]
[null,"SS-SING-277","Carbohydrates - Total Non-structural\n(% in plant leaf or organic material)",66,72.599999999999994]
[null,"SS-SING-160","Brix Reading\n",11,12.1]
[null,"SS-SING-270","Chloride – Plants\nIncludes water soluble chloride on plants.",33,36.299999999999997]
[null,"SS-SING-263","Chlorophyll 'a' Concentration \nIncludes 90% acetone extraction- requires air dry and grinding into powder.",66,72.599999999999994]
[null,"SS-SING-225","Dry Matter Content (%) at 105°C\nProportion of moisture and oven-dry solid in ‘as received’ sample (105°C). ",11,12.1]
[null,"SS-SING-204","Fertility Report - Ferti-Tech Soil /Leaf Report Preparation\n",52,57.2]
[null,"SS-SING-071","Fertility Report - Keycrobe Soil /Leaf Report Preparation\n",52,57.2]
[null,"SS-SING-022","Iodine - NaOH Extraction\n",110,121]
[null,"SS-PREP-009","Leaf Washing\nPlease advise with samples.",11,12.1]
[null,"SS-SING-136","Protein (Crude)\nIncludes Total Nitrogen (TN) and Crude Protein (Calculation).",33,36.299999999999997]
[null,"SS-SING-272","Starch Content (% in plant leaf or organic material)\n",84,92.4]
[]
[null,"FEED AND PRODUCE TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","FEED SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-107","Feed Package - Cereal Grain (NIR- Near-Infrared Analysis)\nFor oat, barley, wheat and triticale grains. \r\nIncludes Dry Matter/Moisture, Crude Protein, Acid Detergent Fibre, Neutral Detergent Fibre, Dry Matter Digestibility, Dry Organic Matter Digestibility and Metabolisable Energy, Starch and Sugar, Fat for oats. \r\n",110,121]
[null,"SS-PACK-109","Feed Package - Horse (NIR- Near-Infrared Analysis)\nFor hay, fresh cut pasture and cereal grains, includes Horse Digestible Energy. \r\nIncludes Dry Matter/Moisture, Crude Protein, Acid Detergent Fibre, Neutral Detergent Fibre, Dry Matter Digestibility, Dry Organic Matter Digestibility and Metabolisable Energy and Horse Digestible Energy.\r\n\r\n",110,121]
[null,"SS-PACK-108","Feed Package - Pelleted (NIR- Near-Infrared Analysis)\nFor pelleted and mixed feeds.\r\nIncludes Dry Matter/Moisture, Crude Protein, Acid Detergent Fibre, Neutral Detergent Fibre, Dry Matter Digestibility, Dry Organic Matter Digestibility and Metabolisable Energy, Fat and Ash. \r\n",110,121]
[null,"SS-PACK-106","Feed Package - Quality (NIR- Near-Infrared Analysis)\nFor hay, fresh cut pasture, straw, pasture silage and maize silage. \r\nIncludes Dry Matter/Moisture, Crude Protein, Acid Detergent Fibre, Neutral Detergent Fibre, Dry Matter Digestibility, Dry Organic Matter Digestibility and Metabolisable Energy. Depending on fodder type can include: Water Soluble Carbohydrates, Starch and Sugar, Fat and Ash. \r\n",110,121]
[null,"SS-PACK-145","Soluble Nitrogen - Feed\nIncludes Nitrate and Ammonium.",44,48.4]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL FEED TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-239","Cyanide (Total Prussic Acid in Plant/ Feed samples)\nIncludes sample preparation and Total Cyanide. ",110,121]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","PRODUCE SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-084","Produce Metals 1 (NATA Subcontracted)\nIncludes Cadmium and Lead.",104,114.4]
[null,"SS-PACK-085","Produce Metals 2 (NATA Subcontracted)\nIncludes Cadmium, Lead and Mercury.",120,132]
[null,"SS-PACK-083","Produce MRL - CR006 (C3/C5 Extended Residue)\nIncludes Standard Residue Screen - Analysis of Pesticides (Organo-chlorines (OC), Organo-phosphates (OP)), Herbicides, Phenols, Carbamates, Acaricides, Synthetic Pyrethroids, Fungicides, Other.",385,423.5]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL PRODUCE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-214","Produce - Single Metal\nIncludes Cadmium or Lead or Mercury. Includes preparation.",88,96.8]
[null,"SS-SING-211","Produce Bacto 1\nIncludes Produce Ecoli.",49,53.9]
[null,"SS-SING-212","Produce Bacto 2\nIncludes Produce Salmonella.",66,72.599999999999994]
[null,"SS-SING-213","Produce Bacto 3\nIncludes Produce Listeria.",60,66]
[null,"SS-SING-287","Produce Bacto 4\nIncludes Produce Faecal Coliforms.",49,53.9]
[]
[null,"COMPOST, BIOCHAR AND HAIR TESTING"]
[]
[null,null,null,null,"Basic Compost Testing Only. See Compost and Lanscape Soils Price List for comprehensive list."]
[null,"ITEM CODE","COMPOST SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-004","Compost Available Nutrients\nIncludes pH and EC; Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 200 g of sample is required.",135,148.5]
[null,"CA-PACK-001","Compost Total Nutrients\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se). Note: 200 g of sample is required.",110,121]
[null,"CA-PACK-019","Compost Total and Available Nutrients\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se); Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 300 g of sample is required.",210,231]
[null,"CA-PACK-020","Compost Total and Available Nutrients plus Heavy Metals\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag; Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 300 g of sample is required.  ",240,264]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIOCHAR SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-163","Biochar Totals Analysis Plus \nIncludes Moisture Content, Bulk Density; Ash Content and Loss on Ignition (750°C); pH, EC (1:10 water); Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC); Hydrogen, Oxygen Calc., H/Corg and O/Corg Calc; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Acid Neutralising Capacity (ANC). Note: 500 g of sample is required to complete testing.",470,517]
[null,"SS-PACK-143","Soil Testing for Biochar Application\nIncludes Moisture, pH, EC (1:5 water); Total Organic Carbon (TOC), Total Nitrogen (TN), TC/TN Ratio; Available Nitrogen (Nitrate); Soluble Chloride; Total Metals (Sb, As, Be, B, Cd, Co, Cu, Cr, Pb, Mn, Mo, Ni, Se, Sn, V, Zn, S, P, Hg); Soluble Cations (Ca, Mg, K, Na). Note: 300 g of sample is required to complete testing.",225,247.5]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","HAIR SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-050","Hair Tissue Mineral Analysis (HTMA) - Human and Animal\nIncludes Antimony, Aluminium, Arsenic, Barium, Beryllium, Bismuth, Boron, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium and Zinc.\r\nData only (no interpretation), Nitric Acid digest, minimum of 0.5 g of hair required which is equivalent to one heaped tablespoon. Collect from nape as close as possible to scalp as this reflects new growth.  Provide sample double bagged to avoid contamination when opened at the laboratory.",88,96.8]
[]
[null,"AGRICULTURAL WATER TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","AGRICULTURAL WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-007","Agricultural Stock Use\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation); Water Hardness; Total Alkalinity; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury; Nitrate, Ammonium, Phosphate; Faecal Coliforms.",135,148.5]
[null,"SW-PACK-005","Irrigation and Livestock Suitability – Comprehensive\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms and E.Coli Bacteria; Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Manganese, Nickel, Lead, Zinc; Nitrate, Ammonium, Phosphate; Sodium, Potassium, Calcium, Magnesium, Chloride, Sulfate, Sodium Absorption Ratio (SAR).",165,181.5]
[null,"SW-PACK-004","Irrigation Suitability - Basic\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Iron and Manganese; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride; Turbidity, Total Alkalinity, Water Hardness (calculation), Saturation Index; Sodium Absorption Ratio (SAR).",88,96.8]
[null,"SW-PACK-024","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Organo-phosphates (OP).",140,154]
[null,"SW-PACK-002","Water Quality - Basic \nFor drinking and domestic use.  Includes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms, E.Coli Bacteria.",77,84.7]
[null,"SW-PACK-003","Water Quality - Comprehensive\nFor drinking and domestic use. Includes pH, EC, Total Dissolved Salts (TDS) (calculation), Water Hardness, Total Alkalinity, Turbidity, Total Coliforms and E.Coli Bacteria; Nitrate; Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Manganese, Nickel, Lead, Zinc, Mercury.",120,132]
[]
[null,null,null,null,"No additional charges if a suite is selected."]
[null,"ITEM CODE","INDIVIDUAL AGRICULTURAL WATER TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-022","Algae - Basic ID and Count (Blue Green Algae only) by Microscopic Identification\n",120,132]
[null,"SW-SING-123","Algae - Full ID and Count by Microscopic Identification\n",180,198]

{"sheet":"Compost","index":6,"n_rows":294,"n_cols":5,"rows_kept":294,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[null,"COMPOST AND LANDSCAPE SOIL ANALYTICAL SERVICES"]
[null,"COMPOST TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS4454 COMPOST PRODUCT SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-011","Mature Compost Analysis under AS4454\nIncludes Bulk Density; Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Bioassay; Plant Propagules, Nitrogen Drawdown Index, Specific Oxygen Uptake Rate, Solvita; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms. Acid Neutralising Capacity required if pH > 8.0. Note: 4 kg of sample required.",660,726]
[null,"CA-PACK-003","Composted Product Analysis under AS4454\nIncludes Bulk Density; Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Bioassay; Plant Propagules, Nitrogen Drawdown Index; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms. Acid Neutralising Capacity required if pH > 8.0. Note: 4 kg of sample required.",500,550]
[null,"CA-PACK-023","Pasteurized Product Analysis under AS4454\nIncludes Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; PO4; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Plant Propagules; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms. Acid Neutralising Capacity required if pH > 8.0. Note: 4 kg of sample required.",350,385]
[null,"CA-PACK-024","Raw Mulch Analysis under AS4454\nIncludes pH, EC; TOC, TN, TC/TN Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Plant Propagules; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls). Acid Neutralising Capacity required if pH > 8.0. Note: 4 kg of sample required.",200,220]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS4454 COMPOST BASIC SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-005","Compost Soluble Nutrients plus Carbon & Nitrogen under AS4454\nIncludes Moisture, pH, EC; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio. Note: 200 g of sample is required to complete testing. \r\n",99,108.9]
[null,"CA-PACK-013","LECO - Total Carbon, Total Nitrogen under AS4454/AS3743/AS4419\nIncludes Total Carbon (TC) and Total Nitrogen (TN), TC/TN Ratio. Note: 200 g of sample is required to complete testing.",38,41.8]
[null,"CA-PACK-014","Nutrients - Water Extractable under AS4454\nIncludes Moisture, Nitrate, Phosphate, Ammonium (1:5 water). Note: 200 g of sample is required to complete testing.\r\n",55,60.5]
[null,"CA-PACK-010","pH and EC under AS4454\nIncludes Moisture, pH and EC. Note: 200 g of sample is required to complete testing.",44,48.4]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","BASIC COMPOST SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-020","Compost Total and Available Nutrients plus Heavy Metals\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag; Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 300 g of sample is required.  ",240,264]
[null,"CA-PACK-019","Compost Total and Available Nutrients\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se); Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 300 g of sample is required.",210,231]
[null,"CA-PACK-001","Compost Total Nutrients\nIncludes Moisture, pH, EC; TC, TN, TC/TN Ratio, Organic Matter; Total (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se). Note: 200 g of sample is required.",110,121]
[null,"CA-PACK-004","Compost Available Nutrients\nIncludes pH and EC; Soluble (Ca, Mg, K, P), Dissolved (NH4, NO3, S); Exchangeable (Ca, Mg, Na, K, H, Al, ECEC); Bray I and II Phosphorus; Colwell Phosphorus; Available Micronutrients (Fe, Cu, Mg, Zn, B, Si); TC, TN, TC/TN Ratio, Organic Matter. Note: 200 g of sample is required.",135,148.5]
[null,"CA-PACK-008","Compost Water Soluble Nutrients\nIncludes Moisture; Nitrate, Ammonium; Chloride; Calcium, Magnesium, Sodium, Potassium, Phosphorus, Sulfur, Boron, Copper, Iron, Manganese, Zinc, Aluminium, Molybdenum and Cobalt. Note: 200 g of sample is required to complete testing.",99,108.9]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","OTHER COMPOST SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-189","The Compost Order 2016 - Monitoring\nThis order applies to compost. In this order, compost means any combination of mulch, garden organics, food waste, manure and paunch that has undergone composting.             Includes physical contaminants with glass, metal, rigid plastics, light flexible film plastics. Also includes Salmonella, Ecoli and Faecal Coliforms. Note: 2 kg of sample is required to complete testing. ",200,220]
[null,"SS-PACK-142","The Compost Order 2016 - Compliance\nThis order applies to compost. In this order, compost means any combination of mulch, garden organics, food waste, manure and paunch that has undergone composting.             Includes physical contaminants with glass, metal, rigid plastics, light flexible film plastics, treated timber and asbestos. Also includes Salmonella, Ecoli and Faecal Coliforms. Note: 2 kg of sample is required to complete testing. ",240,264]
[null,"SS-PACK-190","The Pasteurised Garden Organics Order 2016 - Monitoring\nThis order applies to pasteurised garden organics. In this order, pasteurised garden organics means mulch and/or garden organics that have undergone the process of pasteurisation as a minimum.                                      \r\nIncludes physical contaminants with glass, metal, rigid plastics and light flexible film plastics. Note: 2 kg of sample is required to complete testing. ",44,48.4]
[null,"SS-PACK-170","The Pasteurised Garden Organics Order 2016 - Compliance\nThis order applies to pasteurised garden organics. In this order, pasteurised garden organics means mulch and/or garden organics that have undergone the process of pasteurisation as a minimum.                                      \r\nIncludes physical contaminants with glass, metal, rigid plastics, light flexible film plastics, treated timber and asbestos. Also includes Salmonella, Ecoli and Faecal Coliforms and plant propagules. Note: 2 kg of sample is required to complete testing. ",285,313.5]
[null,"SS-PACK-169","The Mulch Order 2016 - Compliance\nThis order applies to mulch. In this order, mulch means plant material shredded and/or screened to a preferred particle size grading for particular applications.                                  Includes particle Size > 5 mm and < 16 mm, physical contaminants with glass, metal, rigid plastics, light flexible film plastics, polystyrene, treated timber and asbestos. Also includes Salmonella, Ecoli and Faecal Coliforms. Also includes chemical contaminants Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls) and heavy metals. Note: 2 kg of sample is required to complete testing. ",350,385]
[null,"SS-PACK-026","Exchangeable Cations - 15D1 - 1 M NH4OAc\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-035","SOUR Test\nIncludes Moisture, Volatile Solids Concentration,  Specific Oxygen Uptake Rate (SOUR) with an incubation of 20oC.",110,121]
[null,"SS-PACK-197","Landscape Soil Testing (A1 A2 A3 A4) under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC (Water) pH (CaCl2); Soluble Chloride; Exchangeable Cations (pH and EC dependant); Available (Fe, Cu, Mn, Zn, B); Available Phosphorus (Colwell); Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles (2-20 mm, > 20 mm); Particle Size Distribution ( > 2.0 mm, 1.0-2.0 mm, 0.5-1.0 mm, 0.25-0.5 mm, 0.1-0.25 mm, 0.05-0.1 mm, 0.002-0.05 mm, < 0.002 mm); Dispersibility; Permeability (@ 16 drops); Water Repellence; Physical Contaminants. Note: 4 kg of sample is required to complete testing.",690,759]
[null,"SS-PACK-202","QLD Compost Characteristics 2023\nIncludes Bulk Density; Moisture, pH, EC; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm; Totals (As, Cd, Cr, Cu, Pb, Hg, Ni, Se, Zn); Plant Propagules (21 days), Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms. (Does NOT include trace level PFAS, TOPA or ASLP leachable PFAS. These are additional charges). Note: 2 kg of sample required.",410,451]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL COMPOST TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-090","Acid Neutralising Capacity (ANC-BT)\nThis method is used to measure Acid Neutralising Capacity (ANC-BT) where pH-KCl > 6.5.",33,36.299999999999997]
[null,"SS-SING-168","Ammonium (1:5 water) under AS4454\nIncludes moisture, extractable ammonium.",33,36.299999999999997]
[null,"SS-SING-139","Bulk Density under AS4454/AS3743\nLab based bulk density on compost and potting mix. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-062","Carbon - Organic by Walkley Black\n",44,48.4]
[null,"SS-SING-061","Carbon - Total Organic by LECO\n",33,36.299999999999997]
[null,"SS-SING-177","Carbon - Organic Matter under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC), Organic Matter by calculation.",44,48.4]
[null,"SS-SING-175","Carbon - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Carbon (TC). ",33,36.299999999999997]
[null,"SS-SING-176","Carbon - Total Organic (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC). ",44,48.4]
[null,"SS-SING-172","Chloride (1:5 water) under AS4454\nIncludes moisture, soluble chloride. ",33,36.299999999999997]
[null,"SS-SING-180","EC (1:5 water) under AS4454\nIncludes moisture, EC (1:5 water).\r\n",27,29.7]
[null,"SS-SING-170","Nitrate (1:5 water) under AS4454\nIncludes moisture, extractable nitrate.",33,36.299999999999997]
[null,"SS-SING-174","Nitrogen - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Nitrogen (TN). ",33,36.299999999999997]
[null,"SS-SING-119","Nitrogen Drawdown Index (NDI) under AS4454/AS4419\nNote: 2 kg of sample is required to complete testing.",104,114.4]
[null,"SS-SING-123","Particle Size Grading under AS4454\nIncludes percentage mass retained on 5 mm and 16 mm sieve. Note: 2 kg of sample is required to complete testing.",33,36.299999999999997]
[null,"SS-SING-178","pH (1:5 water) under AS4454\nIncludes moisture, pH (1:5 water).\r\n",27,29.7]
[null,"SS-SING-165","Phosphate (1:5 water) under AS4454\nIncludes moisture, extractable phosphate.",33,36.299999999999997]
[null,"SS-SING-145","Plant Growth Test (Bioassay) - TMECC 05.05-B\nIn-vitro germination and root elongation. Note: 1 L of sample is required to complete testing.",55,60.5]
[null,"SS-SING-189","Plant Growth Test (Bioassay) under AS4454\nUsed on fresh soils and composts.  Seedling emergence and relative root growth.  Note: 1 kg of sample is required to complete testing.",55,60.5]
[null,"SS-SING-219","Solids Energy Code (Calorific Value) \n",115,126.5]
[null,"SS-SING-245","Vermicast Sieve Test under AS4454:2012\nIncludes percentage mass retained on 1.18 mm sieve. Note: 1 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-137","Viable Plant Propagules under AS4454/AS3743\nNote: 1 kg of sample required to complete testing.",55,60.5]
[null,"SS-SING-122","Visible Contaminants under AS4454\nApplies to composts from agricultural or source separated organics. Includes contamination with glass, metal, rigid plastics, stones, lumps of clay, light flexible film plastics. Note: 2 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-072","Wettability under AS4454/AS3743\n",22,24.2]
[null,"SS-SING-292","AS4454:2012 Appendix K – Spent Mushroom Compost Classification       ",85,93.5]
[]
[null,"POTTING MIX TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS3743 POTTING MIX PRODUCT SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-007","Potting Mix and Growing Media - Premium under AS3743\nIncludes Moisture Content, Bulk Density, pH, EC (1:1.5 water); Chloride, Sodium, Calcium, Magnesium, Potassium, Phosphate, Nitrate, Ammonium, Sulfate, Iron, Copper, Manganese, Zinc, Boron; Air-Filled Porosity (AFP); Water Holding Capacity (WHC); Wettability; Plant Growth Bioassay (Toxicity Index), Nitrogen Drawdown Index (NDI). Note: 3 kg of sample is required to complete testing.\r\n\r\n",330,363]
[null,"CA-PACK-006","Potting Mix and Growing Media - Regular under AS3743\nIncludes Moisture Content, Bulk Density, pH, EC (1:1.5 water); Chloride, Sodium, Calcium, Magnesium, Potassium, Ammonium, Iron, Copper, Manganese, Zinc, Boron; Air-Filled Porosity (AFP), Water Holding Capacity (WHC); Wettability; Plant Growth Bioassay (Toxicity Index); Nitrogen Drawdown Index (NDI). Note: 3 kg of sample is required to complete testing.\r\n\r\n",300,330]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS3743 POTTING MIX BASIC SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-021","AFP and WHC under AS3743:2003\nIncludes Air-Filled Porosity (AFP) and Water Holding Capacity (WHC). Note: 2 kg of sample is required to complete testing.",55,60.5]
[null,"CA-PACK-017","Extractable Macronutrients (Ammonium Acetate) under AS3743\nIncludes Calcium, Magnesium, Sodium, Potassium, Phosphorus, Sulfur (1:1.5). Note: 200 g of sample is required to complete testing.",44,48.4]
[null,"CA-PACK-018","Extractable Micronutrients (DTPA) under AS3743\nIncludes Sodium, Calcium, Magnesium, Potassium, Phosphorus, Sulfur, Iron, Copper, Manganese, Zinc, Boron (1:1.5). Note: 200 g of sample is required to complete testing.",44,48.4]
[null,"CA-PACK-015","Nutrients - Water Extractable under AS3743\nIncludes Nitrate, Ammonium (1:1.5 water). Note: 200 g of sample is required to complete testing.\r\n ",44,48.4]
[null,"CA-PACK-016","pH and EC under AS3743\nIncludes pH and EC (1:1.5 water). Note: 200 g of sample is required to complete testing.",33,36.299999999999997]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL POTTING MIX TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-120","Air-filled Porosity (AFP) under AS3743\nNote: 2 kg of sample is required to complete testing.",27,29.7]
[null,"SS-SING-169","Ammonium (1:1.5 water) under AS3743\nIncludes extractable ammonium.",33,36.299999999999997]
[null,"SS-SING-139","Bulk Density under AS4454/AS3743\nLab based bulk density on compost and potting mix. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-177","Carbon - Organic Matter under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC), Organic Matter by calculation.",44,48.4]
[null,"SS-SING-175","Carbon - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Carbon (TC). ",33,36.299999999999997]
[null,"SS-SING-176","Carbon - Total Organic (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC). ",44,48.4]
[null,"SS-SING-173","Chloride (1:1.5 water) under AS3743\nIncludes soluble chloride. ",33,36.299999999999997]
[null,"SS-SING-181","EC (1:1.5 water) under AS3743\n\r\n",16,17.600000000000001]
[null,"SS-SING-171","Nitrate (1:1.5 water) under AS3743\nIncludes extractable nitrate.",33,36.299999999999997]
[null,"SS-SING-174","Nitrogen - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Nitrogen (TN). ",33,36.299999999999997]
[null,"SS-SING-188","Nitrogen Drawdown Index (NDI) under AS3743\nNote: 2 kg of sample is required to complete testing.",104,114.4]
[null,"SS-SING-179","pH (1:1.5 water) under AS3743\n",16,17.600000000000001]
[null,"SS-SING-166","Phosphate (1:1.5 water) under AS3743/AS4419\nIncludes extractable phosphate.",33,36.299999999999997]
[null,"SS-SING-190","Plant Growth Test (Bioassay) under AS3743/AS4419\nUsed on fresh soils and composts.  Seedling emergence and relative root growth.  Note: 1 kg of sample is required to complete testing.",55,60.5]
[null,"SS-SING-137","Viable Plant Propagules under AS4454/AS3743\nNote: 1 kg of sample required to complete testing.",55,60.5]
[null,"SS-SING-121","Water Holding Capacity (WHC) under AS3743\nNote: 2 kg of sample is required to complete testing.",27,29.7]
[null,"SS-SING-072","Wettability under AS4454/AS3743\n",22,24.2]
[]
[null,"LANDSCAPE SOIL TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS4419:2018 SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-120","Landscape Soils (On Grade) compliance under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles; Bioassay; Water Repellence; Physical Contaminants; Chemical Contaminants (Heavy Metals and Low Level (Pesticides, PCB)); Plant Propagules. Note: 4 kg of sample is required to complete testing.",550,605]
[null,"SS-PACK-127","Landscape Soils (On Grade) monitoring under AS4419:2018 \nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles; Bioassay; Water Repellence. Note: 4 kg of sample is required to complete testing.",350,385]
[null,"SS-PACK-121","Low Density Media (On Slab) compliance under AS4419:2018\nIncludes Bulk Density; pH and EC; Air-Filled Porosity; Water Holding Capacity; Available Phosphorus; Available Nitrogen (Ammonium), Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Nitrogen Drawdown Index; Physical Contaminants; Chemical Contaminants (Heavy Metals and Low Level (Pesticides, PCB)); Plant Propagules. Note: 4 kg of sample is required to complete testing.\r\n",460,506]
[null,"SS-PACK-128","Low Density Media (On Slab) monitoring under AS4419:2018\nIncludes Bulk Density; pH and EC; Air-Filled Porosity; Water Holding Capacity; Available Phosphorus; Available Nitrogen (Ammonium), Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Nitrogen Drawdown Index. Note: 3 kg of sample is required to complete testing.\r\n",260,286]
[null,"SS-PACK-122","Soils for Turf and Lawns compliance under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles; Dispersibility; Permeability; Water Repellence; Physical Contaminants; Chemical Contaminants (Heavy Metals and Low Level (Pesticides, PCB)); Plant Propagules. Note: 4 kg of sample is required to complete testing.",600,660]
[null,"SS-PACK-129","Soils for Turf and Lawns monitoring under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Ammonium plus Nitrate); Organic Matter (Total Organic Carbon); Large Particles; Dispersibility; Permeability; Water Repellence. Note: 3 kg of sample is required to complete testing.",400,440]
[null,"SS-PACK-123","Structural Support Soil and Wetlands compliance under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Nitrate); Organic Matter (Total Organic Carbon); Water Repellence; Permeability; Physical Contaminants; Chemical Contaminants (Heavy Metals and Low Level (Pesticides, PCB)); Plant Propagules. Note: 4 kg of sample is required to complete testing. Particle Size Analysis not included (SS-SING-243 Wetlands & SS-SING-244 Structural Support).",540,594]
[null,"SS-PACK-130","Structural Support Soil and Wetlands monitoring under AS4419:2018\nIncludes Bulk Density; Texture; pH and EC; Exchangeable Cations (pH and EC dependant); Available Phosphorus; Available Nitrogen (Nitrate); Organic Matter (Total Organic Carbon); Water Repellence; Permeability. Note: 3 kg of sample is required to complete testing.",340,374]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","AS4419 SOIL BASIC SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-013","LECO - Total Carbon, Total Nitrogen under AS4454/AS3743/AS4419\nIncludes Total Carbon (TC) and Total Nitrogen (TN), TC/TN Ratio. Note: 200 g of sample is required to complete testing.",38,41.8]
[null,"SS-PACK-131","pH and EC under AS4419:2018\nIncludes pH and EC (1:5 water) except low density soils. Note: 200 g of sample is required to complete testing.",27,29.7]
[null,"SS-PACK-146","pH and EC under AS4419:2018\nIncludes pH and EC (1:1.5 water) for low density soils. Note: 200 g of sample is required to complete testing.",33,36.299999999999997]
[null,"SS-PACK-191","Sportsturf Practical Drainage Suite under AS4419:2018\nIncludes Bulk Density (8, 16, 32 drops), Permeability (8, 16, 32 drops) and Water Holding Capacity. Note 1 kg of sample is required to complete testing.",140,154]
[null,"SS-PACK-132","Total Available Nitrogen under AS4419:2018\nIncludes KCl extractable Nitrate and Ammonium. Note 200 g of sample is required to complete testing.",27,29.7]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","OTHER SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-034","Micronutrients - 12A1 - DTPA Extractable \nIncludes Iron, Copper, Zinc, Manganese.",44,48.4]
[null,"SS-PACK-027","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.\r\n\r\n\r\n ",77,84.7]
[null,"SS-PACK-026","Exchangeable Cations - 15D1 - 1 M NH4OAc\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-001","Exchangeable Cations - 15D3 - 1 M NH4OAc plus Acidity (15G1)\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0 and exchangeable acidity (Hydrogen + Aluminium) by 1 M KCl.\r\n\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-205","Exchangeable Cations - 15D1 - 1 M NH4OAc plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.",74,81.400000000000006]
[null,"SS-PACK-206","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl  plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.",95,104.5]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-183","Bulk Density under AS4419\nLab based bulk density on landscape soils. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-274","Bulk Density under AS4419:2018 \nThis includes 8, 16 and 32 drops. Note 1kg of sample is required to complete testing.",66,72.599999999999994]
[null,"SS-SING-177","Carbon - Organic Matter under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC), Organic Matter by calculation.",44,48.4]
[null,"SS-SING-175","Carbon - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Carbon (TC). ",33,36.299999999999997]
[null,"SS-SING-176","Carbon - Total Organic (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC). ",44,48.4]
[null,"SS-SING-172","Chloride (1:5 water) under AS4454\nIncludes moisture, soluble chloride. ",33,36.299999999999997]
[null,"SS-SING-167","Dispersibility under AS4419\n",44,48.4]
[null,"SS-SING-180","EC (1:5 water) under AS4454\nIncludes moisture, EC (1:5 water).\r\n",27,29.7]
[null,"SS-SING-229","Water repellence of soil under AS4419:2018\nIncludes water repellence of soil and if required, further testing to ethanol repellence of soil. Note: 200 g of sample is required to complete testing.",15,16.5]
[null,"SS-SING-174","Nitrogen - Total (LECO) under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Nitrogen (TN). ",33,36.299999999999997]
[null,"SS-SING-119","Nitrogen Drawdown Index (NDI) under AS4454/AS4419\nNote: 2 kg of sample is required to complete testing.",104,114.4]
[null,"SS-SING-243","Particle Size Analysis for Wetlands under AS4419:2018\nParticle size of sediment and soil by hydrometer and sieve. Percentage mass retained on sieve. Includes > 2 mm, 1.0–2.0 mm, 0.5–1.0 mm, 0.25–0.5 mm, 0.1–0.25 mm, 50 µm–0.1 mm, 2–50 µm, < 2 µm fractions.  Note: 500 g of sample is required to complete testing.      ",120,132]
[null,"SS-SING-184","Particles Size Grading - Large particles under AS4419:2003\nIncludes percentage mass retained on 10 mm, 20 mm, 50 mm and 75 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-226","Particles Size Grading - Large particles under AS4419:2018\nIncludes percentage mass retained on 2 mm, 5 mm, 20 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-244","Particles Size Grading for Structural Support under AS4419:2018\nIncludes percentage mass passing on 63.0 mm, 53.0 mm, 37.5 mm, 26.5 mm, 19.0 mm, 13.2 mm, 4.75 mm fractions. Note: 2 kg of sample is required to complete testing.",66,72.599999999999994]
[null,"SS-SING-156","Permeability under AS4419:2003\nNote: 2 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-230","Permeability under AS4419:2018\nThis includes 8, 16 and 32 drops. Note: 1 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-178","pH (1:5 water) under AS4454\nIncludes moisture, pH (1:5 water).\r\n",27,29.7]
[null,"SS-SING-166","Phosphate (1:1.5 water) under AS3743/AS4419\nIncludes extractable phosphate.",33,36.299999999999997]
[null,"SS-SING-033","Phosphorus - Colwell\nIncludes Phosphorus for alkaline soils.",22,24.2]
[null,"SS-SING-034","Phosphorus - Olsen\nIncludes Olsen Phosphorous - a measure of the intensity of Phosphorus.",22,24.2]
[null,"SS-SING-228","Physical Contaminants under AS4419:2018\nApplies to soil types as identified by AS4419:2018. Includes contamination with glass, metal, rigid plastics, light flexible film plastics. Note: 2 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-190","Plant Growth Test (Bioassay) under AS3743/AS4419\nUsed on fresh soils and composts.  Seedling emergence and relative root growth.  Note: 1 kg of sample is required to complete testing.",55,60.5]
[null,"SS-SING-164","Texture - Full under AS4419\n",27,29.7]
[null,"SS-SING-227","Top Dress - Particles under AS4419:2018\nIncludes percentage mass retained of organics particles on 2 mm, 5 mm, 8 mm sieve. Also mass retained of mineral particles on 2 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-275","Water Holding Capacity under AS4419:2018\nNote: 500g of sample is required to complete testing.",27,29.7]
[null,"SS-SING-182","Wettability under AS4419\n\r\n",22,24.2]
[]
[null,"MAIN ROAD (MRTS AND R178) TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","MRTS SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-090","MRTS16 FORM C Topsoil Testing (2017)\nIncludes Bulk Density; Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC), Organic Matter; Wettability; pH and EC (1:5 water); Texture; Permeability; Extractable Phosphorus, Chloride; MCP Sulfur; Large Particles; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio Effective Cation Exchange Capacity; Water Repellence Class. Note: 4 kg of sample is required to complete testing.",330,363]
[null,"SS-PACK-067","MRTS16 FORM D Manufactured Site Topsoil Compliance Testing (2017)\nIncludes Total Organic Carbon (TOC), Organic Matter; pH and EC (1:5 water); Texture; Extractable Chloride; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Dispersion (Emerson Class); Water Repellence Class. Note: 1 kg of sample is required to complete testing.",210,231]
[null,"SS-PACK-093","MRTS16 FORM E Subsoil Testing (2017)\nIncludes Wettability; pH and EC (1:5 water); Texture; Extractable Chloride; MCP Sulfur; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Dispersion (Emerson Class); Water Repellence Class; Slaking Class; Clouding (Dispersion) Class. Note: 1 kg of sample is required to complete testing.",220,242]
[null,"SS-PACK-097","MRTS16 FORM F Drainage Basin Soil Testing (2017)\nIncludes Moisture Content; pH and EC (1:5 water); Extractable Chloride; MCP Sulfur; Dispersion (Emerson Class); Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Dispersion (Emerson Class); Slaking Class; Clouding (Dispersion) Class. Note: 1 kg of sample is required to complete testing.",210,231]
[null,"SS-PACK-100","MRTS16 FORM G Organic Soil Conditioner Testing (2017)\nIncludes Bulk Density; Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Bioassay; Plant Propagules, Nitrogen Drawdown Index, Specific Oxygen Uptake Rate, Solvita; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms; Legionella, Listeria; Asbestos; PFAS - Low Level. Acid Neutralising Capacity required if pH > 8.0. Note: 5 kg of sample required.",1160,1276]
[]
[]
[null,"ITEM CODE","MRTS WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-070","MRTS - FORM I - Non-potable Water Testing and Assessment Report\nIncludes pH, EC; Sodium, Potassium, Calcium, Magnesium, Sulfate, Chloride, Sodium Absorption Ratio (SAR); Bicarbonate / Carbonate Alkalinity;  Salmonella, Ecoli, Total Coliforms.",165,181.5]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","R178 SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-095","R178 FORM E1 Subsoil Testing (2017)\nIncludes Wettability; pH and EC (1:5 water); Texture; Extractable Phosphorus, Extractable Chloride; MCP Sulfur; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Water Repellence Class; Slaking Class; Clouding (Dispersion) Class. Note: 1 kg of sample is required to complete testing.",220,242]
[null,"SS-PACK-092","R178 FORM E2 Topsoil Testing - Site Won, Manufactured and Imported  (2017)\nIncludes Bulk Density; Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC), Organic Matter; Wettability; pH and EC (1:5 water); Texture; Permeability; Extractable Phosphorus, Chloride; MCP Sulfur; Large Particles; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio Effective Cation Exchange Capacity; Dispersion (Emerson Class); Water Repellence Class; Slaking Class; Clouding (Dispersion) Class. Note: 4 kg of sample is required to complete testing.",330,363]
[null,"SS-PACK-099","R178 FORM E3 Drainage Basin Soil Testing (2017)\nIncludes Moisture Content; pH and EC (1:5 water); Extractable Chloride; MCP Sulfur; Exchangeable Calcium, Magnesium, Sodium, Potassium, Aluminium, Calcium/Magnesium Ratio, Effective Cation Exchange Capacity; Dispersion (Emerson Class); Slaking Class; Clouding (Dispersion) Class. Note: 1 kg of sample is required to complete testing.",190,209]
[null,"SS-PACK-101","R178 FORM G1 Organic Soil Conditioner Testing (2017)\nIncludes Bulk Density; Moisture, pH, EC; Wettability; TOC, TN, TC/TN Ratio; NO3, NH4, PO4, NH4/NO3 Ratio; Particle Size > 5mm and < 16mm; Physical Contaminants - Glass, Metal, Rigid Plastics > 2mm, Light Plastics > 5mm, Stones and Clay > 5mm; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Bioassay; Plant Propagules, Nitrogen Drawdown Index, Specific Oxygen Uptake Rate, Solvita; Low Level Pesticides (Organo-chlorines, Polychlorinated Biphenyls); Salmonella, Ecoli, Faecal Coliforms; Legionella, Listeria; Asbestos. Acid Neutralising Capacity required if pH > 8.0. Note: 5 kg of sample required.",940,1034]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","OTHER SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-078","Exchangeable Cations - 15B3 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium.\r\n\r\n\r\n\r\n\r\n\r\n",60,66]
[null,"SS-PACK-027","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.\r\n\r\n\r\n ",77,84.7]
[null,"SS-PACK-207","Exchangeable Cations - 15B3 - 1 M NH4Cl plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium.",74,81.400000000000006]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL SOIL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-183","Bulk Density under AS4419\nLab based bulk density on landscape soils. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-177","Carbon - Organic Matter under AS4454/AS3743/AS4419\nIncludes moisture correction, Total Organic Carbon (TOC), Organic Matter by calculation.",44,48.4]
[null,"SS-SING-172","Chloride (1:5 water) under AS4454\nIncludes moisture, soluble chloride. ",33,36.299999999999997]
[null,"SS-SING-167","Dispersibility under AS4419\n",44,48.4]
[null,"SS-SING-025","Emerson Aggregate Test (EAT)\nProvides an Emerson Dispersion Class",49,53.9]
[null,"SS-SING-184","Particles Size Grading - Large particles under AS4419:2003\nIncludes percentage mass retained on 10 mm, 20 mm, 50 mm and 75 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-226","Particles Size Grading - Large particles under AS4419:2018\nIncludes percentage mass retained on 2 mm, 5 mm, 20 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-156","Permeability under AS4419:2003\nNote: 2 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-034","Phosphorus - Olsen\nIncludes Olsen Phosphorous - a measure of the intensity of Phosphorus.",22,24.2]
[null,"SS-SING-196","Slaking and Clouding - Test Methods Q161 and Q162\n",33,36.299999999999997]
[null,"SS-SING-082","Sulfur - MCP\n",22,24.2]
[null,"SS-SING-164","Texture - Full under AS4419\n",27,29.7]
[null,"SS-SING-197","Water repellence of soil - Test Method Q160\n",16,17.600000000000001]
[null,"SS-SING-182","Wettability under AS4419\n\r\n",22,24.2]
[]
[null,"CONTAMINATION TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","CONTAMINATION SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-004","Basic Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Aluminium, Arsenic, Beryllium, Boron, Cadmium, Chromium, Cobalt, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",77,84.7]
[null,"SS-PACK-055","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Polychlorinated Biphenyls (PCB).",135,148.5]
[null,"SS-PACK-056","Pesticide Screen 2b - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",140,154]
[null,"SS-PACK-118","Residue Screen - Extended (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",310,341]
[null,"SS-PACK-119","Residue Screen - Complete + Glyphosate (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue) + Glyphosate Screens.",470,517]
[null,"SS-PACK-045","Total Acid Extractable - Heavy Metals  (ICPMS)\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",55,60.5]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL CONTAMINATION TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-063","Asbestos Identification (Not Quantifiable)\nIdentification in building material, soil, compost and dust.",77,84.7]
[null,"SS-SING-157","Glyphosate (Round Up) + AMPA Screen (All dried solids)\n",280,308]
[null,"SS-SING-056","Organo-chlorines (OC) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-057","Organo-phosphates (OP) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-224","PFAS in ASLP leachate – standard level 28 suite with detection to 0.01 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in ASLP (Australian Standard Leachate Procedure) leachate.\r\n",230,253]
[null,"SS-SING-216","PFAS in solid – standard level 28 suite with detection 0.01 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",190,209]
[null,"SS-SING-253","PFAS in solid – LOW level 28 suite with detection 0.0008-0.0016 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",210,231]
[null,"SS-SING-278","PFAS-28 Standard Level - TOPA\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus PFAS Precursor compounds.",360,396]
[null,"SS-SING-279","PFAS-28 Standard Level - TOF\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus any Total Organofluorine compounds.",230,253]
[null,"SS-SING-058","Polychlorinated Biphenyls (PCB) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-140","Synthetic Pyrethroids\n",135,148.5]
[null,"SS-SING-288","PFAS Full Suite – 30 Trace Compounds (0.1 µg/kg)                                        \n",370,407]
[null,"SS-SING-289","TOPA – PFAS Full Suite – 30 Trace Compounds (0.1 µg/kg)                                  \n",435,478.5]
[null,"SS-SING-290","ASLP Leachate – PFAS Full Suite – 30 Trace Compounds (0.001-0.005 µg/L)                      \n",370,407]
[null,"SS-SING-291","TOF – Total OrganoFluorine                   \n",280,308]
[null,"SS-SING-285","Contamination Foreign Material Fraction Percentage – Modified RMS T276\nIncludes Fraction % (Rubber, plastic, bitumen, paper, cardboard, cloth, paint, glass, metal, Timber (engineered, painted, coated or treated)other vegetable matter). Includes photo per sample and each individual fraction.",150,165]
[]
[null,"BIOLOGICAL AND MICROBIAL TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","MICROBIAL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-185","Cryptosporidium and Giardia \nNote: 500 g of sample is required to complete testing.",940,1034]
[null,"SS-PACK-141","Microbial Biomass Assessment - Compost \nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-166","Microbial Biomass Assessment - Soil with high Organics\nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-140","Microbial Biomass Assessment - Soil\nIncludes biomasses of 12 microbial groups relevant for soil quality, health and function. ",285,313.5]
[null,"SS-PACK-167","MIC-01: Basic Analysis of Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Total fungi (moulds), Gram negative bacteria, Filamentous actinomycetes, Yeasts. ",99,108.9]
[null,"SS-PACK-168","MIC-02: Extended Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Filamentous actinomycetes, Actinobacteria, Gram negative bacteria, Filamentous fungi (Moulds), Yeasts, Lactic acid bacteria, Total Anaerobes (includes facultative anaerobes), Sulfite Reducing Anaerobes.",210,231]
[null,"SS-PACK-175","Phytophthora and Pythium\nNote: 500 g of sample is required to complete testing.",165,181.50000000000003]
[null,"SS-PACK-176","General Plant Pathogen Scan\nNote: 500 g of sample is required to complete testing.",385,423.5]
[null,"SS-PACK-059","Pathogens\nIncludes Moisture, Ecoli, Faecal Coliforms, Salmonella.",155,170.5]
[null,"SS-PACK-184","General Plant Pathogen Scan Plus\nGeneral plant pathogen scan including Phytophthora, Pythium, Rhizoctonia and Fusarium.\r\n\r\nNote: 500 g of sample is required to complete testing.",550,605]
[]
[null,null,null,null,"Unless otherwise indicated 200 g of sample is required."]
[null,"ITEM CODE","INDIVIDUAL MICROBIAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-047","Aerobic Plate Count\n",44,48.4]
[null,"SS-SING-265","Bacillus cereus\n",135,148.5]
[null,"SS-SING-266","Clostridium perfringens\n",82,90.2]
[null,"SS-SING-267","Campylobacter\n",165,181.5]
[null,"SS-SING-044","E.Coli\n",44,48.4]
[null,"SS-SING-043","Faecal Coliforms\n",44,48.4]
[null,"SS-SING-268","Legionella spp plus longbeachae\nIncludes Legionella spp plus longbeachae in solids.",140,154]
[null,"SS-SING-046","Listeria\n",66,72.599999999999994]
[null,"SS-SING-269","Nematodes\n",110,121]
[null,"SS-SING-045","Salmonella\n",66,72.599999999999994]
[null,"SS-SING-262","Microbiometer – Soil biomass measurement\nIncludes estimates of Total Bacteria, Fungi and Fungi:Bacteria ratio. This test should only be done in conjunction with SS-Pack-167 or SS-Pack-168.",33,36.299999999999997]
[null,"SS-SING-195","SOLVITA - Compost Emissions Maturity Test\nIncludes measurement of carbon dioxide and ammonia gas released from compost due to biological activity.",66,72.599999999999994]
[null,"SS-SING-209","SOLVITA - Soil CO2 Burst\nIncludes measurement of carbon dioxide released from soil due to biological activity.",66,72.599999999999994]
[]
[null,"BIOCHAR, FILTER MEDIA AND BIOSOLID TESTING"]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIOCHAR SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-163","Biochar Totals Analysis Plus \nIncludes Moisture Content, Bulk Density; Ash Content and Loss on Ignition (750°C); pH, EC (1:10 water); Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC); Hydrogen, Oxygen Calc., H/Corg and O/Corg Calc; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Acid Neutralising Capacity (ANC). Note: 500 g of sample is required to complete testing.",470,517]
[null,"SS-PACK-111","Biochar Totals Analysis\nIncludes Moisture Content, Bulk Density; Ash Content and Loss on Ignition (750°C); pH, EC (1:10 water); Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC), TC/TN Ratio, Organic Matter; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Acid Neutralising Capacity (ANC). Note: 200 g of sample is required to complete testing.",250,275]
[null,"SS-PACK-149","Biochar Ultimate Analysis\nIncludes Total Organic Carbon, Total Carbon, Total Nitrogen, Total Hydrogen and Ash Content. Oxygen Calc., H/Corg and O/Corg Calc. ",315,346.5]
[null,"SS-PACK-150","Biochar Density and Ashing\nIncludes moisture with % ash and volatiles.",77,84.7]
[null,"SS-PACK-153","Biochar Heavy Metals\nIncludes Pb, Cd, Hg, As, Cu, Ni, Zn and Cr.",88,96.8]
[null,"SS-PACK-154","Biochar Dioxin / Furans (<17 ng/kg) \n",1050,1155]
[null,"SS-PACK-155","Biochar Particle Size Analysis - Dry Sieving\nDry sieving for fractions > 2 mm, 1-2 mm, 500 µm-1 mm, 250-500 µm, 125-250 µm, 63-125 µm, < 63 µm.",99,108.9]
[null,"SS-PACK-156","Biochar Surface Area (Total and External)\n",330,363]
[null,"SS-PACK-143","Soil Testing for Biochar Application\nIncludes Moisture, pH, EC (1:5 water); Total Organic Carbon (TOC), Total Nitrogen (TN), TC/TN Ratio; Available Nitrogen (Nitrate); Soluble Chloride; Total Metals (Sb, As, Be, B, Cd, Co, Cu, Cr, Pb, Mn, Mo, Ni, Se, Sn, V, Zn, S, P, Hg); Soluble Cations (Ca, Mg, K, Na). Note: 300 g of sample is required to complete testing.",225,247.5]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIORETENTION FILTER MEDIA SUITES AND INDIVIDUAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-160","Bioretention Filter Media Analysis (FMSBS 2015)\nIncludes Moisture, pH, EC; Total Organic Carbon, Total Nitrogen, Organic Matter; Phosphate; Dry Sieving >2.0 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm; Bridging Criteria; Hydraulic Conductivity. Note: 3 kg of sample is required to complete testing.",330,363]
[null,"SS-PACK-171","Bioretention Transition Layer Analysis (FMSBS 2015)\nIncludes Dry Sieving >2.0 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm; Bridging Criteria; Hydraulic Conductivity. Note: 3 kg of sample is required to complete testing.",190,209]
[null,"SS-PACK-172","Bioretention Drainage Layer Analysis (FMSBS 2015)\nIncludes Dry Sieving > 5.0 mm, 3.4-5.0 mm, 2.0-3.4 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm; Bridging Criteria; Hydraulic  Conductivity. Note: 3 kg of sample is required to complete testing.",165,181.5]
[null,"SS-SING-231","Saturated Hydraulic Conductivity under ASTM F1815 - 11\nNote: 1 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-254","Particle Size Analysis - Dry Sieving (FMSBS 2015)\nDry sieving for fractions >2.0 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm.",82,90.2]
[]
[null,null,null,null,"All packs have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIOSOLIDS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"BS-PACK-001","Contaminated Grade Assessment\nIncludes Total Dry Solids Concentration, Metals Analysis Arsenic, Cadmium, Chromium, Copper, Lead, Mercury, Nickel, Selenium, Zinc; Low Level (Organo-chlorines Pesticides (OC), Polychlorinated biphenyls (PCB)).",250,275]
[null,"BS-PACK-004","Enteric Viruses Determination\nIncludes Reovirus, Enterovirus, Adenovirus (viruses per 10 g).",460,506]
[null,"BS-PACK-006","Enteric Viruses Determination plus Helminth Ova\nIncludes Reovirus, Enterovirus, Adenovirus (viruses per 10 g) plus Helminth Ova.",550,605]
[null,"BS-PACK-002","Nutrient Determination\nIncludes Moisture Content; Total Nitrogen (TN), Total Phosphorus, Total Kjeldahl Nitrogen (TKN) (by calculation); and available Nutrients (1:10 KCL extractable Nitrate, Ammonium).",99,108.9]
[null,"BS-PACK-005","SOUR Test\nIncludes Moisture, Volatile Solids Concentration, Specific Oxygen Uptake Rate (SOUR) with an incubation of 20oC.",110,121]
[null,"BS-PACK-003","Stabilisation Confirmation\nIncludes Moisture, Microbial Assessment (E.Coli, Faecal Coliforms, and Salmonella sp.), Volatile Solids Concentration, Specific Oxygen Uptake Rate (SOUR).",220,242]

{"sheet":"Contamination","index":7,"n_rows":215,"n_cols":5,"rows_kept":215,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[null,"CONTAMINATION ASSESSMENT ANALYTICAL SERVICES"]
[null,"SOIL ASSESSMENT TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SPECIFIC SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-015","Aggressivity Assessment\nIncludes Moisture, Basic Texture; pH, EC, Resistivity (calculation), Soluble Chloride, Sulfate.",77,84.7]
[null,"SS-PACK-154","Biochar Dioxin / Furans (<17 ng/kg) \n",1050,1155]
[null,"SS-PACK-186","EPA Resource Recover Order - Waste 2017\nAnalysis of solids for moisture content and dry weight analysis of pH, EC (1:5 water), Soluble Cations and Anions (1:5 water extraction with 0.2micron filtration for Na, K, Ca, Mg, Cl, NO3), TN, TOC (LECO), and metals (Aqua regia digest and ICPMS analysis of (S, P, Sb, As, Be, B, Cd, Co, Cu, Cr, Pb, Mn, Mo, Ni, Se, Sn, V, Zn, Hg) 200g dry weight equivalent of sample requested in a jar of plastic bag.",200,220]
[null,"SS-PACK-053","Concrete Quality Analysis\nIncludes concrete crushing, Chloride and Sulfate.",88,96.8]
[null,"SS-PACK-005","Contaminated Site Assessment 1a\nIncludes Basic Texture; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury, Boron, Cobalt, Beryllium; Pesticides (Organo-chlorines (OC), Organo-phosphates (OP)).",140,154]
[null,"SS-PACK-006","Contaminated Site Assessment 1b\nIncludes Basic Texture; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury, Boron, Cobalt, Beryllium; Pesticides (Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB)).",165,181.5]
[null,"SS-PACK-007","Contaminated Site Assessment 2a\nIncludes Basic Texture; Arsenic, Lead; Pesticides (Organo-chlorines (OC), Organo-phosphates (OP)).",120,132]
[null,"SS-PACK-147","Contaminated Site Assessment 2b\nIncludes Basic Texture; Arsenic, Lead; Pesticides (Organo-chlorines (OC)).",110,121]
[null,"SS-PACK-008","Contaminated Site Assessment 3\nIncludes Basic Texture; Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury, Boron, Cobalt, Beryllium; Pesticides (Organo-chlorines (OC)).",135,148.5]
[null,"SS-PACK-051","Excavated Natural Material (ENM) Classification 2014\nIncludes pH, EC (1:5 water); Foreign Material; Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury; Polycyclic Aromatic Hydrocarbons (PAH); Total Petroleum Hydrocarbons (C10-C40), BTEX (C6-C10).",285,313.5]
[null,"SS-PACK-177","Foundry Sand Analysis- RRO, 2014 \nIncludes pH, EC (1:5 water), Total Metals (Hg, Cd, Pb, As, Be, Cr, Cu, Mo, Ni, Se, Ag, Zn) and Total Fluoride (fusion method). \r\n\r\n",165,181.5]
[null,"SS-PACK-042","Health Investigation Level (HIL) Soil Assessment\nIncludes Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury, Beryllium, Boron, Cobalt; Polycyclic Aromatic Hydrocarbons (PAH), Total Petroleum Hydrocarbons (TPH), BTEX Hydrocarbons; Pesticides (Organo-chorines (OC)); Total Phenols; Total Cyanide.",350,385]
[null,"SS-PACK-023","Recovered Aggregate Exemption 2014 (suitable for waste aggregate, soil or concrete)\nIncludes EC; Mercury, Cadmium, Lead, Arsenic, Chromium, Copper, Nickel, Zinc; Fraction % (metal, plaster, rubber, plastic, paper, cloth, paint, wood, other vegetable matter).",120,132]
[null,"SS-PACK-065","Recovered Fines Order EPA 2014 Testing\nIncludes pH, EC (1:5 water); Foreign Material; Particle Size; Total Organic Carbon; Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury; Polycyclic Aromatic Hydrocarbons (PAH); Total Petroleum Hydrocarbons (C10-C36), BTEX (C6-C9); Pesticides (Organochlorine Pesticides (OC); Polychlorinated Biphenyls (PCB); Volatile Hydrocarbons (VHC).",550,605]
[null,"SS-PACK-104","Resource Recovery Exemption Analysis EPA 2017\nIncludes Moisture Content; pH, EC; Total Organic Carbon, Total Nitrogen, C/N Ratio; Soluble Cations (Sodium, Potassium, Calcium, Magnesium), Soluble Anions (Chloride, Nitrate); Totals (Antimony, Arsenic, Beryllium, Boron, Cadmium, Cobalt, Copper, Chromium, Lead, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Selenium, Sulfur, Tin, Vanadium, Zinc).",300,330]
[null,"SS-PACK-182","Soil/ Sediment Contamination Assessment\nIncludes Metals (Total Available Al, As, Cd, Cr, Cu, Fe Pb, Mn, Hg, Ni, Se, Ag, Zn), PAH, TPH, BTEX, and speciated Phenolics.",240,264]
[null,"SS-PACK-066","The Recovered Glass Sand Order 2014\nIncludes EC; Total Organic Carbon (TOC); Mercury, Cadmium, Lead, Arsenic, Chromium, Copper, Nickel, Zinc, Molybdenum; Fraction % (Plaster, clay lumps and other friable materials. Rubber, plastic, bitumen, paper, cloth, paint, wood and other vegetation matter).",150,165]
[null,"SS-PACK-080","Treated Drilling Mud Exemption 2014\nIncludes pH, EC (1:5 water); Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury; Polycyclic Aromatic Hydrocarbons (PAH); Total Petroleum Hydrocarbons (C10-C36), BTEX (C6-C9), Total Chlorinated Hydrocarbons (TCH).",310,341]
[null,"SS-PACK-105","Treated Grease Trap Waste Order EPA 2014 \nIncludes Moisture Content; pH, EC; Oil and Grease; Total Nitrogen; Totals (Arsenic, Cadmium, Chromium, Copper, Lead, Mercury, Nickel, Selenium and Zinc); Available Boron. ",200,220]
[null,"SS-PACK-148","Waste Material Biomethane Potential (BMP)\nIncludes BMP analysis using COD, Total Solids, Volatile solids (VS) and methane production normalised on a VS basis (includes assessment report with cumulative gas production graphs).\r\nNote: typically an 8 week production trial and limited sample numbers of 4 per batch) (estimated 2kg of sample solids/ sludge required for analysis.\r\n",1300,1430]
[null,"SS-PACK-198","Resource Recovery Plasterboard Order 2014 (suitable for recovered plasterboard)\nIncludes moisture content; pH (1:5 water); Metals (Mercury, Cadmium, Lead, Arsenic, Chromium, Copper, Molybdenum, Nickel, Selenium and Zinc); Nutrients/ salts (Calcium, Magnesium, Sodium and Sulfur); reporting Gypsum as % CaSO4.2H2O; and Soluble Chloride reported as % ClO2 (500g of sample requested).",170,187]
[null,"SS-PACK-201","Coffee Pod Analysis\nIncludes moisture content, coffee content, volatile content (plastic, lacquer, paint), aluminium content.",275,302.5]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","RESIDUE SOIL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-147","Contaminated Site Assessment 2b\nIncludes Basic Texture; Arsenic, Lead; Pesticides (Organo-chlorines (OC)).",110,121]
[null,"SS-PACK-030","Contaminated Site Assessment 4 - Dip Site Screening Analysis\nIncludes Total Arsenic and Organo-chlorines (OC). Designed for dip site assessments.",88,96.8]
[null,"SS-PACK-013","Pesticide Screen 1a\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).",88,96.8]
[null,"SS-PACK-014","Pesticide Screen 1b\nIncludes Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",110,121]
[null,"SS-PACK-055","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Polychlorinated Biphenyls (PCB).",135,148.5]
[null,"SS-PACK-056","Pesticide Screen 2b - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",140,154]
[null,"SS-PACK-017","Petroleum Compounds Assessment 1a\nIncludes Total Petroleum Hydrocarbons (TPHC10-C40), BTEX (equivalent to TPHC6- C10).",99,108.9]
[null,"SS-PACK-018","Petroleum Compounds Assessment 1b (Total and Speciated)\nIncludes Total Petroleum Hydrocarbons (TPHC10-C40), BTEX (equivalent to TPHC6- C10), Speciated Total Petroleum Hydrocarbons (aromatic and aliphatic).",310,341]
[null,"SS-PACK-118","Residue Screen - Extended (Compost, Plant leaf, stem, wood material, feed)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",310,341]
[null,"SS-PACK-119","Residue Screen - Complete + Glyphosate\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue) + Glyphosate Screens.",470,517]
[null,"SS-PACK-196","Residue Screen - Extended (Soil Only)\nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue)",200,220]
[null,"SS-PACK-208","Produce MRL - CR007 (Dithiocarbamates) \nProduce MRL - CR007 (Dithiocarbamates) \nIncludes Mancozeb(Dithane), Maneb, Metiram, Propineb, Zineb, Ferbam, Metham-sodium, Thiram, Ziram.",185,203.5]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","METAL SOLIDS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-004","Basic Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Aluminium, Arsenic, Beryllium, Boron, Cadmium, Chromium, Cobalt, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",77,84.7]
[null,"SS-PACK-188","Extra Elements related to Hair Analysis\nIncludes Caesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium and Zirconium.",190,209]
[null,"SS-PACK-043","Extra Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Antimony, Barium, Bismuth, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",77,84.7]
[null,"SS-PACK-046","Special - Metals and Salts Combo - Total Acid Extractable (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",135,148.5]
[null,"SS-PACK-045","Total Acid Extractable - Heavy Metals  (ICPMS)\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",55,60.5]
[null,"SS-PACK-153","Biochar Heavy Metals\nIncludes Pb, Cd, Hg, As, Cu, Ni, Zn and Cr.",88,96.8]
[null,"SS-PACK-161","Specific - ASLP Extractable (ICPMS) \nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride, Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-032","Specific - TCLP Extractable (ICPMS) \nIncludes Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-162","Specific - SPLP Extractable (ICPMS) \nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride, Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-069","Speciated Arsenic\nIncludes toxic arsenic species AsV and AsIII determination using HPLC-ICPMS (Total Arsenic analysis also included). ",330,363]
[null,"SS-PACK-070","Speciated Chromium\nIncludes toxic hexavalent chromium species CrVI and CrIII determination using HPLC-ICPMS (Total Chromium analysis also included).",330,363]
[null,"SS-PACK-068","Speciated Mercury\nIncludes toxic mercury species Methyl Mercury and Hg2+ determination using HPLC-ICPMS. (Total Mercury analysis also included).",330,363]
[]
[]
[null,"ITEM CODE","SOIL PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-002","Hotblock Digest\nIncludes total Aqua-Regia or Nitric Acid digestion of solid samples.",13,14.3]
[null,"SS-PREP-001","Sample Preparation\nIncludes drying and ring mill grinding.",11,12.1]
[null,"SS-PREP-005","TCLP Extractions\nToxicity Characteristic Leaching Procedure.",49,53.9]
[]
[null,null,null,null,"Sample Preparation may be required unless a Discounted Testing Suite is selected."]
[null,"ITEM CODE","INDIVIDUAL SOLIDS TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-149","Arsenic - Total\nIncludes sample preparation / acid digest and analysis by ICPMS.",33,36.299999999999997]
[null,"SS-SING-063","Asbestos Identification (Not Quantifiable)\nIdentification in building material, soil, compost and dust.",77,84.7]
[null,"SS-SING-161","Asbestos Identification and Quantification in Soil\nIdentification and quantification in soil (using AS4964-2004 or WA/NEPM) (% ACM, % Friable).",88,96.8]
[null,"SS-SING-162","Chromium VI - Hexavalent \nSpeciation by a screening colourimetric technique which may be subject to matrix interference. Refer to separate analysis codes for speciation using HPLC-ICPMS analysis.",39,42.9]
[null,"SS-SING-127","Contamination Foreign Material Fraction Percentage\nIncludes Fraction % (metal, plaster, rubber, plastic, paper, cloth, paint, wood, other vegetable matter).",44,48.4]
[null,"SS-SING-153","Cyanide - Free\n",49,53.9]
[null,"SS-SING-148","Cyanide - Total\n",66,72.599999999999994]
[null,"SS-SING-239","Cyanide (Total Prussic Acid in Plant/ Feed samples)\nIncludes sample preparation and Total Cyanide. ",110,121]
[null,"SS-SING-147","Fluoride - Total by fusion\n",77,84.7]
[null,"SS-SING-132","General Metals -  ICPMS\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SS-SING-157","Glyphosate (Round Up) + AMPA Screen (All dried solids)\n",280,308]
[null,"SS-SING-158","Herbicides Phenoxy Acid\n",220,242]
[null,"SS-SING-051","Hydrocarbons - BTEX - equivalent to TPH(C6-C10)\n",55,60.5]
[null,"SS-SING-020","Hydrocarbons - Polycyclic Aromatic (PAH)\n",71,78.099999999999994]
[null,"SS-SING-192","Hydrocarbons - Polycyclic Aromatic (PAH) by TCLP\nIncludes PAH by TCLP extraction.",130,143]
[null,"SS-SING-115","Hydrocarbons\nIncludes Hydrocarbons (C1-C5). Cost per analyte.",44,48.4]
[null,"SS-SING-023","Hydrocarbons - Total Petroleum - Speciated \nIncludes Speciated TPH (aromatic or aliphatic).",220,242]
[null,"SS-SING-052","Hydrocarbons - Total Petroleum - TPH (C10-C40)\n",55,60.5]
[null,"SS-SING-150","Lead - Total\nIncludes sample preparation, acid digest and analysis by ICPMS.",33,36.299999999999997]
[null,"SS-SING-024","Specific Metals - TCLP Extractable ICPMS\nPrice per element\nAluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Silver or  Zinc.",15,16.5]
[null,"SS-SING-133","Non-Standard Metals -  ICPMS\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SS-SING-053","Organo-chlorines (OC)  (Detection Limit - 0.1 ppm)\n",71,78.099999999999994]
[null,"SS-SING-056","Organo-chlorines (OC) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-054","Organo-phosphates (OP)  (Detection Limit - 0.1 ppm)\n",71,78.099999999999994]
[null,"SS-SING-057","Organo-phosphates (OP) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-159","Organotins (MBT, TBT, DBT)\n",285,313.5]
[null,"SS-SING-070","Paint Analysis for Lead\n",33,36.299999999999997]
[null,"SS-SING-224","PFAS in ASLP leachate – standard level 28 suite with detection to 0.01 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in ASLP (Australian Standard Leachate Procedure) leachate.\r\n",230,253]
[null,"SS-SING-216","PFAS in solid – standard level 28 suite with detection 0.01 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",190,209]
[null,"SS-SING-279","PFAS-28 Standard Level - TOF\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus any Total Organofluorine compounds.",230,253]
[null,"SS-SING-278","PFAS-28 Standard Level - TOPA\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus PFAS Precursor compounds.",360,396]
[null,"SS-SING-253","PFAS in solid – LOW level 28 suite with detection 0.0008-0.0016 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",210,231]
[null,"SS-SING-065","pH (1:5 water)\n",16,17.600000000000001]
[null,"SS-SING-142","Phenol - Total \n",66,72.599999999999994]
[null,"SS-SING-029","Phenolics - speciated phenols\n",99,108.9]
[null,"SS-SING-055","Polychlorinated Biphenyls (PCB)  (Detection Limit - 0.1 ppm)\n",71,78.099999999999994]
[null,"SS-SING-058","Polychlorinated Biphenyls (PCB) - Low Level (Detection Limit - 0.01 ppm)\n",110,121]
[null,"SS-SING-217","Semi-Volatile Organic Compounds (SVOC)\nSVOC includes Phenols.",285,313.5]
[null,"SS-SING-027","Silica - Total\nIncludes specialised NaOH high temperature fusion extraction of silicon.",135,148.5]
[null,"SS-SING-223","Silica Gel Clean-up TRH\nIncludes TRH C9-C40 Natural/ Petroleum differentiation – silica gel clean-up (removes all of the biogenic, more polar material leaving just the petrogenic based TRH).",120,132]
[null,"SS-SING-140","Synthetic Pyrethroids\n",135,148.5]
[null,"SS-SING-255","Fats, Oils and Grease of Solids - Hexane 1.5 hr soxlet extraction from wet weight solids\nIncludes separate moisture content for conversion of results to dry weight.",66,72.599999999999994]
[null,"SS-SING-126","Volatile Halogenated Compounds (VHC)\n",88,96.8]
[null,"SS-SING-026","Volatile Organic Compounds (VOC)\n",130,143]
[null,"SS-SING-288","PFAS Full Suite – 30 Trace Compounds (0.1 µg/kg)                                        \n",370,407]
[null,"SS-SING-289","TOPA – PFAS Full Suite – 30 Trace Compounds (0.1 µg/kg)                                  \n",435,478.5]
[null,"SS-SING-290","ASLP Leachate – PFAS Full Suite – 30 Trace Compounds (0.001-0.005 µg/L)                      \n",370,407]
[null,"SS-SING-291","TOF – Total OrganoFluorine                   \n",280,308]
[null,"SS-SING-285","Contamination Foreign Material Fraction Percentage – Modified RMS T276\nIncludes Fraction % (Rubber, plastic, bitumen, paper, cardboard, cloth, paint, glass, metal, Timber (engineered, painted, coated or treated)other vegetable matter). Includes photo per sample and each individual fraction.",150,165]
[]
[null,"WATER ASSESSMENT TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SPECIFIC WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-018","Effluent Monitoring\nIncludes pH, Total Suspended Solids (TSS); Biochemical Oxygen Demand (BOD); Total Oils and Grease (TOG); Total Nitrogen (TN), Total Phosphorus (TP); Nitrate, Nitrite, Phosphate, Ammonium; Faecal Coliforms.",210,231]
[null,"SW-PACK-058","Gas Contamination Monitoring for Dissolved Gases\nIncludes Acetylene, Butane, Ethane, Ethene, Methane and Propane.",155,170.5]
[null,"SW-PACK-056","Gas Contamination Water Quality Monitoring\nIncludes pH, EC, Total Dissolved Salts (TDS) (calculation), Total Alkalinity, Total Suspended Solids (TSS); Total Petroleum Hydrocarbons (TPH C10-C40), BTEX (Equivalent TPH C6-C10); Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",180,198]
[null,"SW-PACK-015","Wastewater Monitoring\nIncludes pH, Total Suspended Solids (TSS); Biochemical Oxygen Demand (BOD); Total Oils and Grease (TOG).",104,114.4]
[null,"SW-PACK-079","Water Contamination Assessment\nIncludes Metals (Total Available Al, As, Cd, Cr, Cu, Fe Pb, Mn, Hg, Ni, Se, Ag, Zn), PAH, TPH, BTEX, and speciated Phenolics.",240,264]
[null,"SW-PACK-071","Water quality for concrete mixes under AS1379 \nIncludes pH, EC, TDS (by calc), Total Suspended Solids, Total Oils and Grease, Sugars (Biological Oxygen Demand), Chloride, Sodium and Sulfate.",155,170.5]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","RESIDUE WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-072","Complete Waters Residue Screen \nIncludes RS1 + RS2 (OCOP Pesticides + Synthetic Pyrethroids – 80+ Residues + Herbicide and Fungicide – 40+ Residue).",240,264]
[null,"SW-PACK-009","Pesticide Screen 1a\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).",77,84.7]
[null,"SW-PACK-010","Pesticide Screen 1b\nIncludes Organo-chlorines (OC), Organo-phosphates (OP) and Polychlorinated biphenyls (PCB).",99,108.9]
[null,"SW-PACK-024","Pesticide Screen 2a - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC) and Organo-phosphates (OP).",140,154]
[null,"SW-PACK-027","Pesticide Screen 2b - Low Level \nIncludes Low Level Pesticide Analysis: Organo-chlorines (OC), Organo-phosphates (OP), Polychlorinated Biphenyls (PCB).",155,170.5]
[null,"SW-PACK-059","Pesticide Screen 3 - In Oil (Detection est. <10ppm)\nIncludes Organo-chlorines (OC), Organo-phosphates (OP).\r\nNote: 25 mL required.",165,181.5]
[null,"SW-PACK-075","Pesticides/ Residue Screen – In Oil (Detection 0.1ppm) \nIncludes Organo-chlorines (OC), Organo-phosphates (OP) and a Multi-residue scan.\r\nNote: 25 mL required.",200,220]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","METAL WATER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PACK-031","Basic Metals Scan - As Supplied (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",60,66]
[null,"SW-PACK-040","Basic Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-030","Basic Metals Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",71,78.099999999999994]
[null,"SW-PACK-029","Basic Metals Scan - Total Available / Acid Soluble (acidified) (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",66,72.599999999999994]
[null,"SW-PACK-043","Extra Metals Scan - As Supplied (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",60,66]
[null,"SW-PACK-044","Extra Metals Scan - Dissolved (filtered then acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-045","Extra Metals Scan - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",66,72.599999999999994]
[null,"SW-PACK-046","Extra Metals Scan - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",71,78.099999999999994]
[null,"SW-PACK-060","Saline Water Metals (Low Level) > 20 mS/cm (As Supplied) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",88,96.8]
[null,"SW-PACK-061","Saline Water Metals (Low Level) > 20 mS/cm (Dissolved) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",93,102.3]
[null,"SW-PACK-062","Saline Water Metals (Low Level) > 20 mS/cm (Total Available/Acid Soluble) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",93,102.3]
[null,"SW-PACK-063","Saline Water Metals (Low Level) > 20 mS/cm (Total Recoverable) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Barium, Beryllium, Bismuth, Cobalt,  Molybdenum, Thallium, Uranium and Vanadium).",99,108.9]
[null,"SW-PACK-051","Special - Metals and Salts Combo - As Supplied (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",120,132]
[null,"SW-PACK-052","Special - Metals and Salts Combo - Dissolved (filtered then acidified) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",130,143]
[null,"SW-PACK-053","Special - Metals and Salts Combo - Total Available/Acid Soluble (acidified) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",130,143]
[null,"SW-PACK-054","Special - Metals and Salts Combo - Total Recoverable (digested with nitric acid) (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Bromide, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Chloride, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",135,148.5]
[null,"SW-PACK-067","Speciated Arsenic\nIncludes toxic arsenic species AsV and AsIII determination using HPLC-ICPMS (Total Arsenic analysis also included) 1% of volume HCl preservation in PP.",385,423.5]
[null,"SW-PACK-068","Speciated Chromium\nIncludes toxic hexavalent chromium species CrVI and CrIII determination using HPLC-ICPMS (Total Chromium analysis also included) 1M NaOH preservation (approx.. 3 Drops/30ml to adjust pH to 8-9.5) in PP.",385,423.5]
[null,"SW-PACK-066","Speciated Mercury\nIncludes toxic mercury species Methyl Mercury and Hg2+ determination using HPLC-ICPMS. (Total Mercury analysis also included) 1% of volume HCl preservation in glass jar.",385,423.5]
[null,"SW-PACK-074","Metals Screen in Oil - Total Acid Digestible (ICPMS)\nIncludes Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.\r\nNote: 25 mL required to complete testing.",99,108.9]
[]
[]
[null,"ITEM CODE","WATER PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-PREP-003","Filtered/Dissolved Metals\nImmediate filtration through 0.45 µm filter followed by acidification with Nitric acid. It is particularly important where waters are high in suspended clay matter, where Iron and Aluminium may be present.",5,5.5]
[null,"SW-PREP-006","Saline Waters Instrument Setup (per batch)\n",110,121]
[null,"SW-PREP-002","Total Available/Acid Soluble Metals\nAcidification with Nitric acid.  Used on nearly all environmental waters, acid sulfate waters, groundwater and surface waters (According to ANZECC guidelines).  Also used for clean waters, drinking waters, when acidified in the field and when requested.",5,5.5]
[null,"SW-PREP-001","Total Recoverable Metals\nNitric Acid digest. Used on high sludge/solid waters and when requested.",16,17.600000000000001]
[]
[null,null,null,null,"Sample Preparation may be required unless a Discounted Testing Suite is selected."]
[null,"ITEM CODE","INDIVIDUAL WATER TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SW-SING-142","Absorbance (Wavelength 440nm – Filtered 0.22 micron)\n",22,24.2]
[null,"SW-SING-012","Biochemical Oxygen Demand (BOD) - Total\n",49,53.9]
[null,"SW-SING-013","Chemical Oxygen Demand (COD)\n",49,53.9]
[null,"SW-SING-030","Chromium VI - Hexavalent \nSpeciation by a screening colourimetric technique which may be subject to matrix interference. Refer to separate analysis codes for speciation using HPLC-ICPMS analysis.",39,42.9]
[null,"SW-SING-056","Conductivity - Electrical\n",11,12.1]
[null,"SW-SING-029","Cyanide - Total\n",55,60.5]
[null,"SW-SING-102","General Metals - As Supplied (external prep)\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-103","General Metals - Dissolved\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-104","General Metals - Total Available/Acid Soluble\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SW-SING-105","General Metals - Total Recoverable\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Bromide, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SS-SING-133","Non-Standard Metals -  ICPMS\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-116","Glyphosate (Round Up)\n",190,209]
[null,"SW-SING-098","Herbicides Phenoxy Acid\n",190,209]
[null,"SW-SING-062","Hydrocarbons - BTEX (Equivalent to TPH C6-C10)\n",55,60.5]
[null,"SW-SING-008","Hydrocarbons - Polycyclic Aromatic Hydrocarbons (PAH)\n",71,78.099999999999994]
[null,"SW-SING-063","Hydrocarbons - Total Petroleum (TPH C10-C40)\n",55,60.5]
[null,"SW-SING-112","Methane\n",120,132]
[null,"SW-SING-106","Non-Standard Metals - As Supplied\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-107","Non-Standard Metals - Dissolved\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-108","Non-Standard Metals - Total Available/Acid Soluble\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-109","Non-Standard Metals - Total Recoverable\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Gallium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SW-SING-064","Organo-chlorines (OC)\n",71,78.099999999999994]
[null,"SW-SING-113","Organo-chlorines (OC) - In Oil\nNote: 25 mL required.",135,148.5]
[null,"SW-SING-143","Chemical Oxygen Demand - Filtered (COD-F)\nFiltered GFC 1.2micron equivalent",55,60.5]
[null,"SW-SING-096","Organo-chlorines (OC) - Low Level\n",99,108.9]
[null,"SW-SING-065","Organo-phosphates (OP)\n",71,78.099999999999994]
[null,"SW-SING-114","Organo-phosphates (OP) - In Oil\nNote: 25 mL required.",135,148.5]
[null,"SW-SING-097","Organo-phosphates (OP) - Low Level \n",99,108.9]
[null,"SW-SING-117","Organotins (MBT, TBT, DBT)\n",285,313.5]
[null,"SW-SING-058","Oxygen - Dissolved (DO)\n",11,12.1]
[null,"SW-SING-121","PFAS in water – standard level 28 suite with detection 0.01 - 0.05 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in water.",165,181.5]
[null,"SW-SING-134","PFAS in water – LOW level 28 suite with detection 0.0002 µg/L\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in water.",190,209]
[null,"SW-SING-055","pH\n",11,12.1]
[null,"SW-SING-038","Phenol - Total \n",66,72.599999999999994]
[null,"SW-SING-026","Phenolics - Speciated Phenols\n",99,108.9]
[null,"SW-SING-066","Polychlorinated Biphenyls (PCB)\n",71,78.099999999999994]
[null,"SW-SING-099","Polychlorinated Biphenyls (PCB) - Low Level \n",99,108.9]
[null,"SW-SING-057","Salinity\n",11,12.1]
[null,"SW-SING-111","Semi-Volatile Organic Compounds (SVOC)\nSVOC includes Phenols.",240,264]
[null,"SW-SING-141","Silica Gel Clean-up TRH\nIncludes TRH C9-C40 Natural/ Petroleum differentiation – silica gel clean-up (removes all of the biogenic, more polar material leaving just the petrogenic based TRH).",120,132]
[null,"SW-SING-122","Silica - Total\nIncludes specialised NaOH high temperature fusion extraction of silicon as per dry weight. ",165,181.5]
[null,"SW-SING-011","Total Oils and Grease (TOG) - Hexane extractable\n",55,60.5]
[null,"SW-SING-003","Total Suspended Solids (TSS)\n",22,24.2]
[null,"SW-SING-037","Trihalomethanes (THM)\n",66,72.599999999999994]
[null,"SW-SING-095","Volatile Halogenated Compounds (VHC)\n",99,108.9]
[null,"SW-SING-094","Volatile Organic Compounds (VOC)\nVOC includes BTEX.",130,143]

{"sheet":"Physical","index":8,"n_rows":94,"n_cols":5,"rows_kept":94,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[null,"PHYSICAL PARAMETERS ANALYTICAL SERVICES"]
[null,"PHYSICAL PARAMETER TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","PHYSICAL PARAMETER SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-138","Atterberg Limits\nIncludes Liquid Limit, Plastic Limit, Plastic Index and Shrinkage Limit.\r\nNote: 1kg of sample required.",190,209]
[null,"SS-PACK-125","RUSLE Soil Erodibility Factor\nIncludes texture grading through ISSS Hydrometer and 0.1, 0.2 and 2.0 mm Sieve analysis, Organic Matter by calculation from LECO Total Organic Carbon, Emerson Dispersion Class using the Emerson Aggregate Test and determination of K Factor. \r\nClient must provide field assessment of Soil Structure and Permeability using RUSLE classes for K Factor calculation.\r\n",240,264]
[]
[null,null,null,null,"Individual tests may require sample preparation."]
[null,"ITEM CODE","PARTICLE SIZE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-194","Gravel Content\nIncludes sieving > 2 mm stones and organic material.",22,24.2]
[null,"SS-PACK-155","Biochar Particle Size Analysis - Dry Sieving\nDry sieving for fractions > 2 mm, 1-2 mm, 500 µm-1 mm, 250-500 µm, 125-250 µm, 63-125 µm, < 63 µm.",99,108.9]
[null,"SS-SING-123","Particle Size Grading under AS4454\nIncludes percentage mass retained on 5 mm and 16 mm sieve. Note: 2 kg of sample is required to complete testing.",33,36.299999999999997]
[null,"SS-SING-184","Particles Size Grading - Large particles under AS4419:2003\nIncludes percentage mass retained on 10 mm, 20 mm, 50 mm and 75 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-226","Particles Size Grading - Large particles under AS4419:2018\nIncludes percentage mass retained on 2 mm, 5 mm, 20 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-244","Particles Size Grading for Structural Support under AS4419:2018\nIncludes percentage mass passing on 63.0 mm, 53.0 mm, 37.5 mm, 26.5 mm, 19.0 mm, 13.2 mm, 4.75 mm fractions. Note: 2 kg of sample is required to complete testing.",66,72.599999999999994]
[null,"SS-SING-227","Top Dress - Particles under AS4419:2018\nIncludes percentage mass retained of organics particles on 2 mm, 5 mm, 8 mm sieve. Also mass retained of mineral particles on 2 mm sieve. Note: 2 kg of sample is required to complete testing.\r\n",44,48.4]
[null,"SS-SING-243","Particle Size Analysis for Wetlands under AS4419:2018\nParticle size of sediment and soil by hydrometer and sieve. Percentage mass retained on sieve. Includes > 2 mm, 1.0–2.0 mm, 0.5–1.0 mm, 0.25–0.5 mm, 0.1–0.25 mm, 50 µm–0.1 mm, 2–50 µm, < 2 µm fractions.  Note: 500 g of sample is required to complete testing.      ",120,132]
[null,"SS-SING-254","Particle Size Analysis - Dry Sieving (FMSBS 2015)\nDry sieving for fractions >2.0 mm, 1-2 mm, 0.5-1 mm, 0.25-0.5 mm, 0.15-0.25 mm, 0.05-0.15 mm, < 0.05 mm.",82,90.2]
[null,"SS-SING-011","Particle Size Analysis - Dry Sieving\nDry sieving for fractions > 2 mm, 1-2 mm, 500 µm-1 mm, 250-500 µm, 125-250 µm, 63-125 µm, < 63 µm.",82,90.2]
[null,"SS-SING-198","Particle Size Analysis - Wet Sieving\nWet sieving for fractions > 2 mm, 1-2 mm, 500 µm-1 mm, 250-500 µm, 125-250 µm, 63-125 µm, < 63 µm.",165,181.5]
[null,"SS-SING-012","Particle Size Analysis - ISSS Hydrometer\nParticle size of sediment and soil by hydrometer. Includes > 2 mm, > 20 µm, 20–2 mm, 2–20 µm and < 2 µm fractions.",99,108.9]
[null,"SS-PACK-126","Particle Size Analysis – ISSS Hydrometer plus 0.2 and 2.0 mm Sieving\nIncludes particle sizing of soils and sediments for ISSS classification: < 2 µm, 2–20 µm and 20 µm¬–2 mm by hydrometer; 0.2–2.0 mm and > 2 mm by sieving.\r\n",110,121]
[null,"SS-SING-236","Particle Size Analysis – ISSS and USDA Hydrometer\nParticle size of sediment and soil by hydrometer. Includes > 2 mm, > 50 µm, > 20 µm, 50 µm–2 mm, 2–50 µm, 2–20 µm and < 2 µm fractions.",130,143]
[null,"SS-SING-235","Particle Size Analysis – USDA Hydrometer\nParticle size of sediment and soil by hydrometer. Includes > 2 mm, > 50 µm, 50 µm–2 mm, 2–50 µm and < 2 µm fractions.",120,132]
[null,"SS-SING-146","Particle Size Analysis - Laser Diffraction\nParticle size analysis using a Malvern Mastersizer 3000. Span 0.01 to 3000 µm. Size classes dictated by client requirements. Includes organic and acid digestion of organic matter and shell, as required.\r\nPrice dependent upon application and sample amounts.",180,198]
[null,"SS-SING-237","Laser Diffraction – Methylated Spirits\nIncludes dry or wet sieving at 2 mm followed by digestion and dispersion as required. Particle size distribution from 2000 to 0.01 µm. Size classes dictated by clients requirements.\r\nPrice dependent upon application and sample amounts.\r\n",190,209]
[null,"FA-PACK-013","Particle Size Analysis – Laser Diffraction – Fine Fertiliser\nLaser Diffraction Particle Size Analysis including 2000 to 0.01 µm. Size fractions include < 0.01 mm, 0.01-0.02 mm, 0.02-0.03 mm, 0.03-0.04 mm, 0.04-0.05 mm, 0.05-0.06 mm, 0.06-0.07 mm, 0.07-0.08 mm, 0.08-0.09 mm, 0.09-0.1 mm, 0.1-0.125 mm, 0.125-0.25 mm, 0.25-0.5 mm, 0.5-1.0 mm, > 1.0 mm fractions.\r\nPrice dependent upon application and sample amounts.",190,209]
[null,"FA-PACK-012","Particle Size Analysis – Dry Sieving – Coarse Fertiliser\nDry sieving Particle Size Analysis including  > 1 mm, 0.85-1 mm, 0.3-0.85 mm, < 0.3 mm fractions.",55,60.5]
[null,"SS-SING-245","Vermicast Sieve Test under AS4454:2012\nIncludes percentage mass retained on 1.18 mm sieve. Note: 1 kg of sample is required to complete testing.",44,48.4]
[]
[null,null,null,null,"Individual tests may require sample preparation."]
[null,"ITEM CODE","DISPERSION AND AGGREGATION TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-167","Dispersibility under AS4419\n",44,48.4]
[null,"SS-SING-215","Dispersion Percent\nIncludes Dispersion Percent and ISSS Hydrometer particle size analysis.\r\n",120,132]
[null,"SS-SING-205","Emerson Aggregate Stability Test for Wastewater\nThis modified Emerson aggregate test (MEAT alternative) is the best option for assessment of aggregate stability for land application areas. Unlike MEAT results, the classes determined by this test can be directly related to those of the Emerson Aggregate Test.",33,36.299999999999997]
[null,"SS-SING-025","Emerson Aggregate Test (EAT)\nProvides an Emerson Dispersion Class",49,53.9]
[null,"SS-SING-085","Emerson Dispersion Index (Loveday and Pyle, 1973)\n",49,53.9]
[null,"SS-SING-015","Modified Emerson Aggregate Test (MEAT)\n",49,53.9]
[null,"SS-SING-206","R1 and R2 Dispersion Ratio\n",120,132]
[null,"SS-SING-196","Slaking and Clouding - Test Methods Q161 and Q162\n",33,36.299999999999997]
[null,"SS-SING-286","R1 Dispersion Index - additional extra option to PSA\nIncludes R1 Dispersion Index. ONLY available when selected with hydrometer particle size techniques.",52,57.2]
[]
[null,null,null,null,"Individual tests may require sample preparation."]
[null,"ITEM CODE","WATER HOLDING AND PERMEABILITY TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"CA-PACK-021","AFP and WHC under AS3743:2003\nIncludes Air-Filled Porosity (AFP) and Water Holding Capacity (WHC). Note: 2 kg of sample is required to complete testing.",55,60.5]
[null,"SS-PACK-195","Available Water Capacity (AWC by Pressure Plate)\nAnalysis of soils for PWP (Permanent Wilting Point) and FC (Field Capacity) using pressure plate at 0.3 and 15bar (suitable for disturbed soil @0.3 bar, clods or intact cores @ 0.1bar) \r\nApprox. 200g of disturbed soil or core size on request.",135,148.5]
[null,"SS-SING-120","Air-filled Porosity (AFP) under AS3743\nNote: 2 kg of sample is required to complete testing.",27,29.7]
[null,"SS-SING-229","Water repellence of soil under AS4419:2018\nIncludes water repellence of soil and if required, further testing to ethanol repellence of soil. Note: 200 g of sample is required to complete testing.",15,16.5]
[null,"SS-SING-156","Permeability under AS4419:2003\nNote: 2 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-230","Permeability under AS4419:2018\nThis includes 8, 16 and 32 drops. Note: 1 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-231","Saturated Hydraulic Conductivity under ASTM F1815 - 11\nNote: 1 kg of sample is required to complete testing.",82,90.2]
[null,"SS-SING-013","Soil Water Retention Curve - Estimation by surrogate methods \nPurely soil materials. Not suitable for mine tailings. Includes estimation of soil hydraulic properties comprising Field Capacity, Permanent Wilting Point, Saturated Hydraulic Conductivity and van Genuchten Soil Moisture Curve parameters. Required: field soil Bulk Density or target Bulk Density, or if unknown then a simple statement of intended land use (eg. horticulture, pasture,  MEDLI etc). The method uses USDA hydrometer particle size analysis and pedotransfer software.",165,181.5]
[null,"SS-SING-207","Soil Water Retention Curve - in-situ soil cores - Ceramic Plate & Dewpoint Potentiometer\nIncludes data for three points on the Soil Water Retention Curve: wet-end soil water content at 1 kPa and 10 kPa (Field Capacity) and dry-end soil water content at Air-Dryness (100 MPa). A ceramic plate and hanging water column is used for the wet end, while the dry end is measured using a dew point potentiometer (Decagon WP4-T). Soil water content at 33 kPa (Field Capacity) and 1500 kPa (Permanent Wilting Point) can be included with selection of SS-SING-247.\r\nNote: In-situ soil cores of 30–50 mm height and no more than 75 mm diameter are required.",275,302.5]
[null,"SS-SING-210","Soil Water Content at Field Capacity and Air-dryness\nApplicable to soils supporting native vegetation. Includes soil water content at 1 kPa, 10 kPa (Field Capacity) and 100 MPa (Air-dryness). Equipment used: ceramic plate and hanging water column for the 1 kPa and 10 kPa points, and a dew point potentiometer (WP4C) for the 100 MPa point. Required: 500 g loose soil (or 1 kg inclusive of both tests when chosen in combination with SS-SING-247), and a target Bulk Density value for each sample, preferably plus a simple statement of intended land use eg. pasture, horticulture, greens,  land remediation etc.",385,423.5]
[null,"SS-SING-247","Soil Water Content at Field Capacity and Permanent Wilting Point\nIncludes soil water content at 33 kPa (Field Capacity) and 1500 kPa (Permanent Wilting Point).  Equipment used: ceramic plate and hanging water column for the 33 kPa point and dew point potentiometer (WP4C) for the 1500 kPa point. \nRequired: 500 g loose soil (or 1 kg inclusive of both tests when chosen in combination with SS-SING-210), and a target Bulk Density value for each sample, preferably plus a simple statement of intended land use eg. pasture, horticulture, greens,  land remediation etc.",155,170.5]
[null,"SS-SING-256","Soil Water Retention Curve - 6 point curve \nIncludes soil water content at 1 kPa, 3 kPa, 10 kPa (Field Capacity upper limit), 33 kPa (Field Capacity lower limit), 1500 kPa (Permanent Wilting Point) and 100 MPa (Air-dryness). Equipment used:  ceramic plate and hanging water column for 1 kPa, 3 kPa, 10 kPa and 33 kPa points, and a dew point potentiometer (WP4C) for the 1500 kPa and 100 MPa points. \nRequired: 1 kg loose soil and a target Bulk Density value for each sample, preferably plus a simple statement of intended land use eg. pasture, horticulture, greens,  land remediation etc.",180,198]
[null,"SS-SING-121","Water Holding Capacity (WHC) under AS3743\nNote: 2 kg of sample is required to complete testing.",27,29.7]
[null,"SS-SING-275","Water Holding Capacity under AS4419:2018\nNote: 500g of sample is required to complete testing.",27,29.7]
[null,"SS-SING-197","Water repellence of soil - Test Method Q160\n",16,17.600000000000001]
[null,"SS-SING-182","Wettability under AS4419\n\r\n",22,24.2]
[null,"SS-SING-072","Wettability under AS4454/AS3743\n",22,24.2]
[]
[]
[null,"ITEM CODE","MOISTURE CONTENT TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-221","Air Dry Moisture Content - ADMC (%) at 105°C.\nMoisture content of an air-dry (40°C) sample, further dried to 105°C (oven-dry equivalent).",11,12.1]
[null,"SS-SING-225","Dry Matter Content (%) at 105°C\nProportion of moisture and oven-dry solid in ‘as received’ sample (105°C). ",11,12.1]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-SING-233","Moisture Content - As Received (%) at 40°C \nMoisture content as a per cent of air-dry equivalent soil (40°C).",11,12.1]
[null,"SS-SING-222","Moisture Content - As Received (%) Gravimetric at 105°C\nSoil moisture as a per cent of dry mass at 105°C (oven-dry equivalent).",11,12.1]
[null,"SS-PREP-007","Total Dry Weight - Air dry basis\nMass of the sample dried at 40°C.\r\n",6,6.6]
[null,"SS-PREP-017","Total Dry Weight - Oven dry basis\nMass of the sample dried at 105°C. Used to calculate bulk density when cores are supplied.",11,12.1]
[]
[]
[null,"ITEM CODE","BULK DENSITY TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-021","Bulk Density - Lab Based\nBulk Density – Lab based compacting of a supplied loose soil/sediment to a set volume, to simulate equivalent field conditions – note for the most accurate method use field bulk density rings of known volume with SS-PREP-017 for total oven dry weight.  ",11,12.1]
[null,"SS-SING-183","Bulk Density under AS4419\nLab based bulk density on landscape soils. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-139","Bulk Density under AS4454/AS3743\nLab based bulk density on compost and potting mix. Note: 1 kg of sample is required to complete testing.",22,24.2]
[null,"SS-SING-274","Bulk Density under AS4419:2018 \nThis includes 8, 16 and 32 drops. Note 1kg of sample is required to complete testing.",66,72.599999999999994]
[]
[]
[null,"ITEM CODE","COLOUR AND TEXTURE\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-218","Colour (Munsell Soil Colour Classification)  \n",8,8.8000000000000007]
[null,"SS-SING-086","Texture – Full under AS 1547:2012",27,29.7]
[null,"SS-SING-164","Texture - Full under AS4419\n",27,29.7]
[null,"SS-SING-208","Texture - Full (NCST, 2009)\nThis method is used for acid sulfate soil action criteria.",27,29.7]
[]
[null,null,null,null,"Individual tests may require sample preparation."]
[null,"ITEM CODE","PHYSICAL CONTAMINANTS TESTS\n","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-127","Contamination Foreign Material Fraction Percentage\nIncludes Fraction % (metal, plaster, rubber, plastic, paper, cloth, paint, wood, other vegetable matter).",44,48.4]
[null,"SS-SING-228","Physical Contaminants under AS4419:2018\nApplies to soil types as identified by AS4419:2018. Includes contamination with glass, metal, rigid plastics, light flexible film plastics. Note: 2 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-245","Vermicast Sieve Test under AS4454:2012\nIncludes percentage mass retained on 1.18 mm sieve. Note: 1 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-122","Visible Contaminants under AS4454\nApplies to composts from agricultural or source separated organics. Includes contamination with glass, metal, rigid plastics, stones, lumps of clay, light flexible film plastics. Note: 2 kg of sample is required to complete testing.",44,48.4]
[null,"SS-SING-285","Contamination Foreign Material Fraction Percentage – Modified RMS T276\nIncludes Fraction % (Rubber, plastic, bitumen, paper, cardboard, cloth, paint, glass, metal, Timber (engineered, painted, coated or treated)other vegetable matter). Includes photo per sample and each individual fraction.",150,165]

{"sheet":"Other Solids","index":9,"n_rows":272,"n_cols":5,"rows_kept":272,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[null,"OTHER SOLID ANALYTICAL SERVICES"]
[null,"GENERAL SOLIDS TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","SOLIDS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-015","Aggressivity Assessment\nIncludes Moisture, Basic Texture; pH, EC, Resistivity (calculation), Soluble Chloride, Sulfate.",77,84.7]
[null,"SS-PACK-163","Biochar Totals Analysis Plus \nIncludes Moisture Content, Bulk Density; Ash Content and Loss on Ignition (750°C); pH, EC (1:10 water); Total Nitrogen (TN), Total Carbon (TC), Total Organic Carbon (TOC); Hydrogen, Oxygen Calc., H/Corg and O/Corg Calc; Totals (Ca, Mg, K, Na, S, P, Zn, Mn, Fe, Cu, B, Si, Al, Mo, Co, Se, Cd, Pb, As, Cr, Ni, Hg, Ag); Acid Neutralising Capacity (ANC). Note: 500 g of sample is required to complete testing.",470,517]
[null,"SS-PACK-053","Concrete Quality Analysis\nIncludes concrete crushing, Chloride and Sulfate.",88,96.8]
[null,"SS-PACK-034","Micronutrients - 12A1 - DTPA Extractable \nIncludes Iron, Copper, Zinc, Manganese.",44,48.4]
[null,"SS-PACK-073","Incubation - Slab\nThis method is used to assess the effectiveness of a soil's Acid Neutralising Capacity (ANC). The incubation is maintained and pH-INC taken fortnightly until the soil pH changes by at least 0.5 pH unit to below 4, or for at least 8 weeks until pH-INC is stable.",200,220]
[null,"SS-PACK-088","LECO - Total Carbon and Total Sulfur\nIncludes Total Carbon (TC) and Total Sulfur (TS) (LECO SC832).",38,41.8]
[null,"SS-PACK-022","Excavated Natural Material (ENM) Classification 2012  (replaced by SS-PACK-051)\nIncludes pH, EC (water 1:5); Foreign Material; Copper, Lead, Cadmium, Zinc, Arsenic, Chromium, Nickel, Mercury; Polycyclic Aromatic Hydrocarbons (PAH); Total Petroleum Hydrocarbons (C10-C36), BTEX (C6-C9), Volatile Halogen Compounds (VHC).",330,363]
[null,"SS-PACK-019","Nutrients - KCl Extractable\nIncludes Nitrate, Ammonium, Phosphate.",55,60.5]
[null,"SS-PACK-033","Nutrients - Water Extractable\nIncludes Nitrate, Phosphate, Ammonium.",55,60.5]
[null,"SS-PACK-036","Mehlich III  Exchangeable Cations\nIncludes Mehlich III Extractable Sodium, Potassium, Calcium, Magnesium, Phosphorus.",44,48.4]
[null,"SS-PACK-037","Mehlich III Exchangeable Cations and Micronutrients\nIncludes Mehlich III Extractable Sodium, Potassium, Calcium, Magnesium, Phosphorus, Sulfur, Aluminium, Iron, Copper, Zinc, Manganese, Boron.",66,72.599999999999994]
[null,"SS-PACK-141","Microbial Biomass Assessment - Compost \nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-140","Microbial Biomass Assessment - Soil\nIncludes biomasses of 12 microbial groups relevant for soil quality, health and function. ",285,313.5]
[null,"SS-PACK-038","Micronutrients - 12C2 - Hot 0.01M CaCl2 Extractable\nIncludes Plant available Boron, Silica.",33,36.299999999999997]
[null,"SS-PACK-039","Morgan Soluble Salt Extract\nIncludes Calcium, Magnesium, Potassium, Phosphorus.",44,48.4]
[null,"SS-PACK-010","pH and EC\nIncludes soil pH and EC (1:5 water).",27,29.7]
[null,"SS-PACK-003","Septic Disposal Soil Assessment\nIncludes moisture, pH(CaCl2), EC, Total Dissolved Salts (TDS) (calculation); Exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium, Hydrogen, Exchangeable Sodium Percentage, Cation Exchange Capacity; Phosphorus Sorption Capacity; Emerson Aggregate Stability Test for Wastewater.",180,198]
[null,"SS-PACK-143","Soil Testing for Biochar Application\nIncludes Moisture, pH, EC (1:5 water); Total Organic Carbon (TOC), Total Nitrogen (TN), TC/TN Ratio; Available Nitrogen (Nitrate); Soluble Chloride; Total Metals (Sb, As, Be, B, Cd, Co, Cu, Cr, Pb, Mn, Mo, Ni, Se, Sn, V, Zn, S, P, Hg); Soluble Cations (Ca, Mg, K, Na). Note: 300 g of sample is required to complete testing.",225,247.5]
[null,"SS-PACK-035","SOUR Test\nIncludes Moisture, Volatile Solids Concentration,  Specific Oxygen Uptake Rate (SOUR) with an incubation of 20oC.",110,121]
[null,"SS-PACK-164","Sulfate to Chloride Ratio\nIncludes Sulfate and Chloride (1:5 water) and Sulfate/Chloride Ratio.\r\n",55,60.5]
[null,"SS-PACK-110","Total NPK Analysis\nIncludes Total Nitrogen, Total Phosphorus, Total Potassium.",66,72.599999999999994]
[null,"SS-PACK-203","Solids Leachable SAR Analysis\nIncludes Sodium Absorption Ratio (SAR) of Solids (1:10 water leach of solid material and analysis of dissolved salts (Na, Ca, Mg)).",50,55]
[]
[null,null,null,null,"SS-PREP-010"]
[null,"ITEM CODE","SOLIDS PREPARATIONS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PREP-024","Ash Analysis Preparation\nIncludes moisture (105°C) and ash content(550°C) whereby ash is analysed.",33,36.299999999999997]
[null,"SS-PREP-021","Bulk Density - Lab Based\nBulk Density – Lab based compacting of a supplied loose soil/sediment to a set volume, to simulate equivalent field conditions – note for the most accurate method use field bulk density rings of known volume with SS-PREP-017 for total oven dry weight.  ",11,12.1]
[null,"SS-PREP-015","Exchangeable Cation Pre-treatment for Soluble Salts\nIncludes pre-treatment with aqueous ethanol and aqueous glycerol to remove soluble salts. Recommended on soils with EC > 0.3 dS/m.",11,12.1]
[null,"SS-PREP-020","Exchangeable Cation Suppression of Carbonates \nIncludes pre-treatment with aqueous ethanol and aqueous glycerol to remove soluble salts then extraction with 1M Alcoholic NH4Cl to suppress solid phase carbonates. Testing according to Method 15C1 with other agricultural tests.",44,48.4]
[null,"SS-PREP-014","Fertiliser Handling Charge\n",55,60.5]
[null,"SS-PREP-016","Fizz Test for Carbonates \nThis method is used to indicate the presence of carbonates.",3,3.3]
[null,"SS-PREP-027","Freeze Drying of solid samples (ie. marine organisms, flesh)\nUsed for tissue or marine samples not suitable for oven drying.",26,28.6]
[null,"SS-PREP-002","Hotblock Digest\nIncludes total Aqua-Regia or Nitric Acid digestion of solid samples.",13,14.3]
[null,"SS-PREP-013","Biosecurity Handling Charge\n",110,121]
[null,"SS-PREP-003","Leaching\nIncludes 1:10 solid/water leaching with filtration.",8,8.8000000000000007]
[null,"SS-PREP-009","Leaf Washing\nPlease advise with samples.",11,12.1]
[null,"SS-PREP-025","Medicinal Cannabis and Hemp Handling Fee\n",84,92.4]
[null,"SS-PREP-008","Microwave Digest\n",22,24.2]
[null,"SS-PREP-028","Pore Water Extraction of sediment sample\n(ie. centrifuge of 50ml subsamples of sediment to extract available pore water or alternative backup option of water added and extracted)",22,24.2]
[null,"SS-PREP-019","Repacking to Target Bulk Density\n",115,126.5]
[null,"SS-PREP-004","Sample Compositing\nIncludes sample compositing and storage of individual samples for at least 2 months to allow for individual testing if required. Charge per individual sample used in the composite.",4,4.4000000000000004]
[null,"SS-PREP-023","Sample Compositing for Soil Carbon Subsoils (30-100cm)\nIncludes compositing charge for composite subsoil samples tested under 2018 CFI methodology.",38,41.8]
[null,"SS-PREP-022","Sample Compositing for Soil Carbon Topsoils (0-30cm)\nIncludes compositing charge for composite topsoil samples tested under 2018 CFI methodology.",16,17.600000000000001]
[null,"SS-PREP-001","Sample Preparation\nIncludes drying and ring mill grinding.",11,12.1]
[null,"SS-PREP-026","Sample Preparation - Crushing/grinding only \nIncludes crushing/grinding when samples are supplied already dried.",6,6.6]
[null,"SS-PREP-012","Sample Storage of Fresh Samples\nIncludes sample storage of supplied samples (1st month storage is free) for up to 12 months at $10.00 per month.",11,12.1]
[null,"SS-PREP-018","Saturated Paste Extract\nIncludes extraction of saturated paste (14A3). Please select required analytical parameters from the waters codes.",77,84.7]
[null,"SS-PREP-005","TCLP Extractions\nToxicity Characteristic Leaching Procedure.",49,53.9]
[null,"SS-PREP-007","Total Dry Weight - Air dry basis\nMass of the sample dried at 40°C.\r\n",6,6.6]
[null,"SS-PREP-017","Total Dry Weight - Oven dry basis\nMass of the sample dried at 105°C. Used to calculate bulk density when cores are supplied.",11,12.1]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL SOLIDS TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-090","Acid Neutralising Capacity (ANC-BT)\nThis method is used to measure Acid Neutralising Capacity (ANC-BT) where pH-KCl > 6.5.",33,36.299999999999997]
[null,"SS-SING-201","Acid Neutralising Capacity by Total Inorganic Carbon (C-IN)\nThis method is used to measure Acid Neutralising Capacity (ANC) where the pH-KCl > 6.5.\r\n\r\n",49,53.9]
[null,"SS-SING-251","Aluminium - 1 M KCl\nIncludes exchangeable aluminium by 1 M KCl.",22,24.2]
[null,"SS-SING-149","Arsenic - Total\nIncludes sample preparation / acid digest and analysis by ICPMS.",33,36.299999999999997]
[null,"SS-SING-063","Asbestos Identification (Not Quantifiable)\nIdentification in building material, soil, compost and dust.",77,84.7]
[null,"SS-SING-161","Asbestos Identification and Quantification in Soil\nIdentification and quantification in soil (using AS4964-2004 or WA/NEPM) (% ACM, % Friable).",88,96.8]
[null,"SS-SING-021","Ash Content by Combustion\nIncludes moisture content and ash content by combustion.",33,36.299999999999997]
[null,"SS-SING-155","Ash Content by Combustion - Routine and Acid Insoluble\nIncludes standard Ash content by combustion then treatment of filter with hydrochloric acid and re-ashing.",38,41.8]
[null,"SS-SING-134","Boron - 12C2 - Hot 0.01M CaCl2 Extractable",27,29.7]
[null,"SS-SING-160","Brix Reading\n",11,12.1]
[null,"SS-SING-038","Chloride - Water Extractable",33,36.299999999999997]
[null,"SS-SING-153","Cyanide - Free\n",49,53.9]
[null,"SS-SING-148","Cyanide - Total\n",66,72.599999999999994]
[null,"SS-SING-225","Dry Matter Content (%) at 105°C\nProportion of moisture and oven-dry solid in ‘as received’ sample (105°C). ",11,12.1]
[null,"SS-SING-064","Electrical Conductivity (1:5 water)\n",16,17.600000000000001]
[null,"SS-SING-273","Extractable Sulfate Sulfur (10% HCl extractable)\nIncludes extraction of soil using 10% HCl following method BS1377 and analysis by ICPOES.",26,28.6]
[null,"SS-SING-067","Fluoride - Water Extractable",66,72.599999999999994]
[null,"SS-SING-147","Fluoride - Total by fusion\n",77,84.7]
[null,"SS-SING-022","Iodine - NaOH Extraction\n",110,121]
[null,"SS-SING-150","Lead - Total\nIncludes sample preparation, acid digest and analysis by ICPMS.",33,36.299999999999997]
[null,"SS-SING-001","Moisture Content - As Received (%) at 105°C\nOven-dry moisture content as a per cent of the ‘as-received’ sample (105°C).",11,12.1]
[null,"SS-SING-233","Moisture Content - As Received (%) at 40°C \nMoisture content as a per cent of air-dry equivalent soil (40°C).",11,12.1]
[null,"SS-SING-068","Neutralising Value\nIncludes Acid Neutralising Capacity -  Carbonate.",33,36.299999999999997]
[null,"SS-SING-138","Organic Matter \nIncludes Total Organic Carbon and organic matter by calculation.",33,36.299999999999997]
[null,"SS-SING-070","Paint Analysis for Lead\n",33,36.299999999999997]
[null,"SS-SING-069","Paramagnetism\n",11,12.1]
[null,"SS-SING-216","PFAS in solid – standard level 28 suite with detection 0.01 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",190,209]
[null,"SS-SING-279","PFAS-28 Standard Level - TOF\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus any Total Organofluorine compounds.",230,253]
[null,"SS-SING-278","PFAS-28 Standard Level - TOPA\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil plus PFAS Precursor compounds.",360,396]
[null,"SS-SING-253","PFAS in solid – LOW level 28 suite with detection 0.0008-0.0016 mg/kg\nIncludes the analysis of per- and poly-fluoroalkyl substances (PFAS) in soil.\r\n",210,231]
[null,"SS-SING-084","Phosphorus Buffer Index (PBI) - Colwell corrected\nIncludes Phosphorus Buffer Index (PBI) and is corrected using Colwell Phosphorus.",44,48.4]
[null,"SS-SING-083","Potassium - 18C1 - BSES 1M HNO3",33,36.299999999999997]
[null,"SS-SING-076","Potassium - Colwell \n",27,29.7]
[null,"SS-SING-136","Protein (Crude)\nIncludes Total Nitrogen (TN) and Crude Protein (Calculation).",33,36.299999999999997]
[null,"SS-SING-131","Redox Potential\nTested on 'as supplied' sample.",33,36.299999999999997]
[null,"SS-SING-028","Scanning Electron Microscopy (SEM) - Sample Feasibility Assessment\nIncludes sample preparation and instrument setup. A quote for analysis is provided following Sample Feasibility Assessment.",400,440]
[null,"SS-PACK-047","Salts – Water Soluble\nIncludes water soluble Sodium, Calcium, Magnesium, Potassium. ",38,41.8]
[null,"SS-SING-199","Scanning Electron Microscopy (SEM) - Imaging and X-ray analysis\nImaging, X-ray analysis or both. Price is sample dependent; a quote can be provided following SEM Sample Feasibility Assessment (SS-SING-028).",310,341]
[null,"SS-SING-080","Silicon - 13D1 - BSES 0.005M H2SO4",22,24.2]
[null,"SS-SING-078","Silicon - 0.01M CaCl2 Extractable",22,24.2]
[null,"SS-SING-135","Silicon - 12C2 - Hot 0.01M CaCl2 Extractable",27,29.7]
[null,"SS-SING-081","Sulfur - KCl-40 \n",22,24.2]
[null,"SS-SING-082","Sulfur - MCP\n",22,24.2]
[null,"SS-SING-124","Sulfur - Morgan Soluble Extract",22,24.2]
[null,"SS-SING-144","Total Sulfur (TS) by LECO\n",22,24.2]
[null,"SS-SING-010","X-ray Diffraction (XRD) Identification - excluding clay minerals\nIncludes identification of minerals and mineral assemblages.  Price dependent upon application and sample amounts. Price does NOT include clay identification.",165,181.5]
[null,"SS-SING-200","X-ray Diffraction (XRD) Identification of Clay Minerals\nIncludes preparation and identification of clay minerals. All other minerals are removed during sample preparation. Price dependent upon application and sample amounts.",610,671]
[null,"SS-SING-031","X-ray Fluorescence (XRF) \nIncludes total elemental concentration of elements with atomic weight greater than Oxygen. Price dependent upon application and sample amounts. Price includes Total Carbon (TC) and Total Nitrogen (TN).",200,220]
[null,"SS-SING-079","Zinc - BSES HCl\n",22,24.2]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","BIOSOLID SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"BS-PACK-001","Contaminated Grade Assessment\nIncludes Total Dry Solids Concentration, Metals Analysis Arsenic, Cadmium, Chromium, Copper, Lead, Mercury, Nickel, Selenium, Zinc; Low Level (Organo-chlorines Pesticides (OC), Polychlorinated biphenyls (PCB)).",250,275]
[null,"BS-PACK-004","Enteric Viruses Determination\nIncludes Reovirus, Enterovirus, Adenovirus (viruses per 10 g).",460,506]
[null,"BS-PACK-006","Enteric Viruses Determination plus Helminth Ova\nIncludes Reovirus, Enterovirus, Adenovirus (viruses per 10 g) plus Helminth Ova.",550,605]
[null,"BS-PACK-002","Nutrient Determination\nIncludes Moisture Content; Total Nitrogen (TN), Total Phosphorus, Total Kjeldahl Nitrogen (TKN) (by calculation); and available Nutrients (1:10 KCL extractable Nitrate, Ammonium).",99,108.9]
[null,"BS-PACK-005","SOUR Test\nIncludes Moisture, Volatile Solids Concentration, Specific Oxygen Uptake Rate (SOUR) with an incubation of 20oC.",110,121]
[null,"BS-PACK-003","Stabilisation Confirmation\nIncludes Moisture, Microbial Assessment (E.Coli, Faecal Coliforms, and Salmonella sp.), Volatile Solids Concentration, Specific Oxygen Uptake Rate (SOUR).",220,242]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","CARBON SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-020","Carbon Stability\nIncludes Total Carbon (TC), Labile Carbon.",55,60.5]
[null,"SS-PACK-011","LECO - Total Carbon and Total Nitrogen\nIncludes Total Carbon (TC) and Total Nitrogen (TN), TC/TN Ratio.",33,36.299999999999997]
[null,"SS-PACK-088","LECO - Total Carbon and Total Sulfur\nIncludes Total Carbon (TC) and Total Sulfur (TS) (LECO SC832).",38,41.8]
[null,"SS-PACK-012","LECO - Total Carbon, Total Nitrogen and Total Sulfur\nIncludes Total Carbon (TC) and Total Nitrogen (TN), Total Sulfur (TS), TC/TN Ratio.",49,53.9]
[null,"SS-PACK-174","Inorganic (Carbonate) Carbon by LECO\nIncludes Total Carbon (TC), Total Organic Carbon (TOC).",60,66]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL CARBON TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-018","Carbon - Labile - Blair 0.333M KMnO4",22,24.2]
[null,"SS-SING-062","Carbon - Organic by Walkley Black\n",44,48.4]
[null,"SS-SING-061","Carbon - Total Organic by LECO\n",33,36.299999999999997]
[null,"SS-SING-059","Inorganic (Carbonate) Carbon by LECO\nIncludes Total Carbon (TC), Total Organic Carbon (TOC).",49,53.9]
[null,"SS-SING-060","Total Carbon by LECO\n",22,24.2]
[null,"SS-SING-138","Organic Matter \nIncludes Total Organic Carbon and organic matter by calculation.",33,36.299999999999997]
[]
[null,"EXCHANGEABLE CATIONS TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","EXCHANGEABLE CATIONS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-073","Incubation - Slab\nThis method is used to assess the effectiveness of a soil's Acid Neutralising Capacity (ANC). The incubation is maintained and pH-INC taken fortnightly until the soil pH changes by at least 0.5 pH unit to below 4, or for at least 8 weeks until pH-INC is stable.",200,220]
[null,"SS-PACK-028","Exchangeable Acidity - 15G1 - 1 M KCl\nIncludes exchangeable acidity (Hydrogen + Aluminium) by 1 M KCl.\r\n\r\n",33,36.299999999999997]
[null,"SS-PACK-074","Exchangeable Cations - 15A1 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. No pre-treatment for soluble salts.\r\n\r\n\r\n",44,48.4]
[null,"SS-PACK-075","Exchangeable Cations - 15A2 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-029","Exchangeable Cations - 15A3 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium. \r\n\r\n\r\n",60,66]
[null,"SS-PACK-076","Exchangeable Cations - 15B1 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. No pre-treatment for soluble salts.\r\n\r\n\r\n\r\n\r\n",44,48.4]
[null,"SS-PACK-077","Exchangeable Cations - 15B2 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-078","Exchangeable Cations - 15B3 - 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium.\r\n\r\n\r\n\r\n\r\n\r\n",60,66]
[null,"SS-PACK-027","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.\r\n\r\n\r\n ",77,84.7]
[null,"SS-PACK-026","Exchangeable Cations - 15D1 - 1 M NH4OAc\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-041","Exchangeable Cations - 15D3 - 1 M NH4OAc\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0. No pre-treatment for soluble salts.\r\n\r\n\r\n",44,48.4]
[null,"SS-PACK-001","Exchangeable Cations - 15D3 - 1 M NH4OAc plus Acidity (15G1)\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium by 1 M NH4OAc at pH 7.0 and exchangeable acidity (Hydrogen + Aluminium) by 1 M KCl.\r\n\r\n\r\n\r\n",55,60.5]
[null,"SS-PACK-205","Exchangeable Cations - 15D1 - 1 M NH4OAc plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by 1 M NH4OAc at pH 7.0. Pre-treatment for soluble salts when EC is > 0.3 dS/m.",74,81.400000000000006]
[null,"SS-PACK-206","Exchangeable Cations - 15C1 - Alcoholic 1 M NH4Cl  plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by Alcoholic 1 M NH4Cl at pH 8.5. Ideal for soils where pH > 7.3.",95,104.5]
[null,"SS-PACK-207","Exchangeable Cations - 15B3 - 1 M NH4Cl plus Aluminium\nIncludes exchangeable Sodium, Potassium, Calcium, Magnesium, Aluminium by 1 M NH4Cl at pH 7.0. When EC is > 0.3 dS/m soluble Chloride is analysed to adjust the exchangeable sodium.",74,81.400000000000006]
[]
[null,"METALS TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","METALS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-004","Basic Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Aluminium, Arsenic, Beryllium, Boron, Cadmium, Chromium, Cobalt, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc.",77,84.7]
[null,"SS-PACK-043","Extra Metals Scan - Total Acid Extractable (ICPMS)\nIncludes Antimony, Barium, Bismuth, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium.",77,84.7]
[null,"SS-PACK-050","Hair Tissue Mineral Analysis (HTMA) - Human and Animal\nIncludes Antimony, Aluminium, Arsenic, Barium, Beryllium, Bismuth, Boron, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium and Zinc.\r\nData only (no interpretation), Nitric Acid digest, minimum of 0.5 g of hair required which is equivalent to one heaped tablespoon. Collect from nape as close as possible to scalp as this reflects new growth.  Provide sample double bagged to avoid contamination when opened at the laboratory.",88,96.8]
[null,"SS-PACK-044","Salts Scan - Total Acid Extractable (ICPMS)\nIncludes Calcium, Magnesium, Phosphorus, Potassium, Sodium and Sulfur.",49,53.9]
[null,"SS-PACK-046","Special - Metals and Salts Combo - Total Acid Extractable (ICPMS)\nIncludes Basic (Aluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Selenium, Silver and Zinc); Extra (Antimony, Barium, Beryllium, Bismuth, Boron, Cobalt, Lithium, Molybdenum, Silicon, Strontium, Thallium, Thorium, Uranium and Vanadium) and Salts (Calcium, Magnesium, Phosphorus, Potassium, Sodium and Sulfur).",135,148.5]
[null,"SS-PACK-069","Speciated Arsenic\nIncludes toxic arsenic species AsV and AsIII determination using HPLC-ICPMS (Total Arsenic analysis also included). ",330,363]
[null,"SS-PACK-070","Speciated Chromium\nIncludes toxic hexavalent chromium species CrVI and CrIII determination using HPLC-ICPMS (Total Chromium analysis also included).",330,363]
[null,"SS-PACK-068","Speciated Mercury\nIncludes toxic mercury species Methyl Mercury and Hg2+ determination using HPLC-ICPMS. (Total Mercury analysis also included).",330,363]
[null,"SS-PACK-031","Specific - Rare Earth - Total Acid Extractable (ICPMS) \nIncludes Cerium, Dysprosium, Erbium, Europium, Gadolinium, Holmium, Lanthanum, Lutetium, Neodymium, Praseodymium, Samarium, Scandium, Terbium, Thorium, Thulium, Uranium, Ytterbium and Yttrium.",104,114.4]
[null,"SS-PACK-161","Specific - ASLP Extractable (ICPMS) \nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride, Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-032","Specific - TCLP Extractable (ICPMS) \nIncludes Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-162","Specific - SPLP Extractable (ICPMS) \nIncludes Sodium, Potassium, Calcium, Magnesium, Sulfur, Chloride, Copper, Lead, Cadmium, Zinc, Arsenic, Selenium, Iron, Manganese, Silver, Chromium, Nickel, Aluminium, Mercury.",99,108.9]
[null,"SS-PACK-053","Concrete Quality Analysis\nIncludes concrete crushing, Chloride and Sulfate.",88,96.8]
[null,"SS-PACK-045","Total Acid Extractable - Heavy Metals  (ICPMS)\nIncludes Lead, Cadmium, Arsenic, Nickel, Aluminium, Mercury, Chromium, Silver, Selenium.",55,60.5]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL METALS TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-132","General Metals -  ICPMS\nPrice per element\nAluminium, Antimony, Arsenic, Barium, Beryllium, Bismuth, Boron, Cadmium, Calcium, Chromium, Cobalt, Copper, Iron, Lead, Lithium, Magnesium, Manganese, Mercury, Molybdenum, Nickel, Phosphorus, Potassium, Selenium, Silicon, Silver, Sodium, Strontium, Sulfur, Thallium, Thorium, Uranium, Vanadium or Zinc.",11,12.1]
[null,"SS-SING-133","Non-Standard Metals -  ICPMS\nPrice per element\nCaesium, Cerium, Dysprosium, Erbium, Europium, Gadolinium, Germanium, Gold, Holmium, Lanthanum, Lutetium, Neodymium, Palladium, Platinum, Praseodymium, Rubidium, Samarium, Scandium, Tantalum, Terbium, Thulium, Tin, Titanium, Tungsten, Ytterbium, Yttrium or Zirconium.",16,17.600000000000001]
[null,"SS-SING-024","Specific Metals - TCLP Extractable ICPMS\nPrice per element\nAluminium, Arsenic, Cadmium, Chromium, Copper, Iron, Lead, Manganese, Mercury, Nickel, Silver or  Zinc.",15,16.5]
[]
[null,"MICROBIAL AND NITROGEN TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","MICROBIAL SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-185","Cryptosporidium and Giardia \nNote: 500 g of sample is required to complete testing.",940,1034]
[null,"SS-PACK-192","Food Microbiology (ie. Macadamia kernel)\nIncludes E.Coli, Total Coliforms, Salmonella and Total Plate Count.",115,126.5]
[null,"SS-PACK-176","General Plant Pathogen Scan\nNote: 500 g of sample is required to complete testing.",385,423.5]
[null,"SS-PACK-184","General Plant Pathogen Scan Plus\nGeneral plant pathogen scan including Phytophthora, Pythium, Rhizoctonia and Fusarium.\r\n\r\nNote: 500 g of sample is required to complete testing.",550,605]
[null,"SS-PACK-141","Microbial Biomass Assessment - Compost \nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-166","Microbial Biomass Assessment - Soil with high Organics\nIncludes biomasses of 12 microbial groups relevant for compost quality, health and function. ",330,363]
[null,"SS-PACK-140","Microbial Biomass Assessment - Soil\nIncludes biomasses of 12 microbial groups relevant for soil quality, health and function. ",285,313.5]
[null,"SS-PACK-167","MIC-01: Basic Analysis of Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Total fungi (moulds), Gram negative bacteria, Filamentous actinomycetes, Yeasts. ",99,108.9]
[null,"SS-PACK-168","MIC-02: Extended Microbial Activity in Soil (Plate Count)\nPreferably examined in relation to texture, moisture content, pH, C:N ratio, and organic matter content. \r\nIncludes Total aerobic bacteria, Filamentous actinomycetes, Actinobacteria, Gram negative bacteria, Filamentous fungi (Moulds), Yeasts, Lactic acid bacteria, Total Anaerobes (includes facultative anaerobes), Sulfite Reducing Anaerobes.",210,231]
[null,"SS-PACK-059","Pathogens\nIncludes Moisture, Ecoli, Faecal Coliforms, Salmonella.",155,170.5]
[null,"SS-PACK-175","Phytophthora and Pythium\nNote: 500 g of sample is required to complete testing.",165,181.50000000000003]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL MICROBIAL TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-047","Aerobic Plate Count\n",44,48.4]
[null,"SS-SING-265","Bacillus cereus\n",135,148.5]
[null,"SS-SING-044","E.Coli\n",44,48.4]
[null,"SS-SING-266","Clostridium perfringens\n",82,90.2]
[null,"SS-SING-267","Campylobacter\n",165,181.5]
[null,"SS-SING-043","Faecal Coliforms\n",44,48.4]
[null,"SS-SING-203","Helminth Ova\n",285,313.5]
[null,"SS-SING-046","Listeria\n",66,72.599999999999994]
[null,"SS-SING-269","Nematodes\n",110,121]
[null,"SS-SING-045","Salmonella\n",66,72.599999999999994]
[null,"SS-SING-195","SOLVITA - Compost Emissions Maturity Test\nIncludes measurement of carbon dioxide and ammonia gas released from compost due to biological activity.",66,72.599999999999994]
[null,"SS-SING-209","SOLVITA - Soil CO2 Burst\nIncludes measurement of carbon dioxide released from soil due to biological activity.",66,72.599999999999994]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","NITROGEN SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-019","Nutrients - KCl Extractable\nIncludes Nitrate, Ammonium, Phosphate.",55,60.5]
[null,"SS-PACK-033","Nutrients - Water Extractable\nIncludes Nitrate, Phosphate, Ammonium.",55,60.5]
[null,"SS-PACK-204","Nitrogen - Water Extractable\nIncludes Nitrate, Nitrite, Ammonium.",55,60.5]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL NITROGEN TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-048","Ammonium - Water Extractable",33,36.299999999999997]
[null,"SS-SING-049","Nitrate - Water Extractable\n",33,36.299999999999997]
[null,"SS-SING-050","Total Nitrogen by LECO\n",22,24.2]
[]
[null,"PHOSPHORUS TESTING"]
[]
[null,null,null,null,"All suites have preparation and digest/extract charges included."]
[null,"ITEM CODE","PHOSPHORUS SUITES","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-PACK-019","Nutrients - KCl Extractable\nIncludes Nitrate, Ammonium, Phosphate.",55,60.5]
[null,"SS-PACK-033","Nutrients - Water Extractable\nIncludes Nitrate, Phosphate, Ammonium.",55,60.5]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL PHOSPHORUS TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-191","MEDLI Adsorption Isotherm Parameters\nModelling (6 concentrations of Phosphorus), Colwell Phosphorus. ",110,121]
[null,"SS-SING-042","Phosphorus - Available by 1M KCl extract\n",22,24.2]
[null,"SS-SING-041","Phosphorus - Morgan Soluble Extract",22,24.2]
[null,"SS-SING-035","Phosphorus - Bray 1 \nIncludes plant available Phosphorous for acid soils.",22,24.2]
[null,"SS-SING-036","Phosphorus - Bray 2\nIncludes plant available and acid soluble forms of Phosphorous.",22,24.2]
[null,"SS-SING-040","Phosphorus - 9G2 - BSES 0.005M H2SO4",22,24.2]
[null,"SS-SING-248","Phosphorus - Citrate Soluble \nIncludes 2% Citrate Soluble Phosphorus.",44,48.4]
[null,"SS-SING-033","Phosphorus - Colwell\nIncludes Phosphorus for alkaline soils.",22,24.2]
[null,"SS-SING-264","Phosphorus – Formic Acid Soluble\nIncludes Formic Acid Soluble Phosphorus.",66,72.599999999999994]
[null,"SS-SING-034","Phosphorus - Olsen\nIncludes Olsen Phosphorous - a measure of the intensity of Phosphorus.",22,24.2]
[null,"SS-SING-032","Phosphorus - Total Acid Extractable (includes preparation)\n",44,48.4]
[null,"SS-SING-037","Phosphorus Buffer Index (PBI)\n",22,24.2]
[null,"SS-SING-084","Phosphorus Buffer Index (PBI) - Colwell corrected\nIncludes Phosphorus Buffer Index (PBI) and is corrected using Colwell Phosphorus.",44,48.4]
[null,"SS-SING-087","Phosphorus Sorption - 40ppm (as mg P/kg)",27,29.7]
[null,"SS-SING-039","Phosphorus Sorption Capacity\nIncludes 1 day preliminary trial, 7 day sorption capacity trial (Ryden and Pratt, 1980), In situ Phosphorous and calculations. ",88,96.8]
[null,"SS-SING-249","Phosphorus - Water Soluble \nIncludes Water Soluble Phosphorus.",22,24.2]
[]
[null,"STABLE ISOTOPES TESTING"]
[]
[null,null,null,null,"Single tests may require sample preparation."]
[null,"ITEM CODE","INDIVIDUAL STABLE ISOTOPE TESTS","PRICE excl. GST","PRICE incl. GST"]
[null,"SS-SING-118","Biomarker and Specific Compounds - 13C and / or 15N Isotopes\nPrice dependent upon application and sample amounts.",0,0]
[null,"SS-SING-116","Carbonate Analysis - 'as supplied' - 13C & 18O Isotopes\nWithout pre-concentration.",66,72.599999999999994]
[null,"SS-SING-257","Carbonate Analysis - 13C and 18O Isotopes\nNo pre-concentration, sample preparation included.",155,170.5]
[null,"SS-SING-114","Dissolved Gas Analysis\nIncludes N2/Ar non-isotope ratio measurement.",44,48.4]
[null,"SS-SING-109","Dissolved inorganic carbon in water - 13C isotopes\n",68,74.8]
[null,"SS-SING-112","Dissolved Nitrogen\nIncludes Dissolved N2 - ratio masses 29/28 and 30/28.",82,90.2]
[null,"SS-SING-113","Dissolved Nitrous Oxide\n",140,154]
[null,"SS-SING-110","Dissolved organic carbon in water - 13C isotopes \n",89,97.9]
[null,"SS-SING-260","Hydrogen and Oxygen in Bulk Solids - 2H and 18O Isotopes\nIncludes % H and % O - consult for sample suitability.",135,148.5]
[null,"SS-SING-261","Hydrogen and Oxygen Content in Bulk Solids - No Isotopes\n",66,72.599999999999994]
[null,"SS-SING-258","Hydrogen in Bulk Solids - 2H Isotopes\nIncludes % H - consult for sample suitability.",66,72.599999999999994]
[null,"SS-SING-242","Organic Carbon in Bulk Solids - 13C Isotopes\nIncludes acid treatment to remove inorganic carbon. % C also provided.",77,84.7]
[null,"SS-SING-117","Nitrogen Gas\nWithout pre-concentration.",49,53.9]
[null,"SS-SING-259","Oxygen in Bulk Solids - 18O Isotopes\nIncludes % O - consult for sample suitability.",66,72.599999999999994]
[null,"SS-SING-108","Total Carbon and Total Nitrogen in Filters - 13C and 15N Isotopes\nFilters (25 mm or smaller GFF quartz preferred) (charge per analyte, sample preparation included).",99,108.9]
[null,"SS-SING-106","Total Carbon in filters - 13C isotopes \n",99,108.9]
[null,"SS-SING-105","Total Carbon and Total Nitrogen in Bulk Solids - 13C and 15N Isotopes\nAlso includes % TC and % TN. ",77,84.7]
[null,"SS-SING-103","Total Carbon in Bulk Solids - 13C Isotopes\nAlso includes % TC.",66,72.599999999999994]
[null,"SS-SING-104","Total Nitrogen in Bulk Solids - 15N Isotopes\nAlso includes % TN. ",66,72.599999999999994]
[null,"SS-SING-107","Total Nitrogen in filters – 15N isotopes \n",99,108.9]

{"sheet":"Admin","index":10,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[null,"ADMIN CHARGES"]
[]
[null,null,null,null,"This discounted batch charge will be applied to each individual report to allow for administration costs."]
[null,"ITEM CODE","ADMIN PRICES","PRICE excl. GST","PRICE incl. GST"]
[null,"ADMIN","Admin Batch Charge\nCharge per batch to cover batch handling / reporting.",33,36.300000000000004]
[null,"ADMIN_50D","Admin Batch Charge - 50% Discount\nUsed for subsequent Admin charges within a single sample submission.",16.5,18.149999999999999]
[null,"ADMIN_P2D","Priority Testing 2 Day\n","Additional Charge","Additional Charge"]
[null,"ADMIN_P5D","Priority Testing 5 Day\n","Additional Charge","Additional Charge"]
[null,"ADMIN_PSD","Priority Testing Same Day\n","Additional Charge","Additional Charge"]
[null,"ADMIN_U1D","Urgency Surcharge 1 Day - 100%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable.","Additional Charge","Additional Charge"]
[null,"ADMIN_U2D","Urgency Surcharge 2 Day - 50%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable.","Additional Charge","Additional Charge"]
[null,"ADMIN_U3D","Urgency Surcharge 3 Day - 25%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable.","Additional Charge","Additional Charge"]
[null,"ADMIN_U4D","Urgency Surcharge 4 Day - 12.5%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable.","Additional Charge","Additional Charge"]
[null,"ADMIN_UA3D","Urgency Surcharge on Ag Samples 3 Day - 50%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable.","Additional Charge","Additional Charge"]
[null,"ADMIN_UC5D","Urgency Surcharge on Basic CA Samples 5 Day - 50%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable. Two day drying time required to complete this testing.","Additional Charge","Additional Charge"]
[null,"ADMIN_USD","Urgency Surcharge Same Day - 100%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable.","Additional Charge","Additional Charge"]
[null,"ADMIN_USL1","L1 Urgency Surcharge on Stds Testing 1-2 Wks - 50%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable. Includes modified testing on some parameters. Surcharges for urgent subcontracting are in addition to EAL surcharges and will be passed on.","Additional Charge","Additional Charge"]
[null,"ADMIN_USL2","L2 Urgency Surcharge on Stds Testing 2-3 Wks - 25%\nNote: days refer to Working Days and samples need to arrive in the morning; some analysis not applicable. Includes modified testing on some parameters. Surcharges for urgent subcontracting are in addition to EAL surcharges and will be passed on.","Additional Charge","Additional Charge"]